**3GPP TSG-CT WG1 Meeting #146C1-24xxxx**

**Online, 22– 26 January 2024**

**Source: Huawei, HiSilicon**

**Title:** **Consistent use of LCS-UPP message**

**Spec: 3GPP TS 24.572 v1.0.0**

**Agenda item: 18.2.19**

**Document for: Agreement**

**1. Introduction**

This p-CR is to corrent the use of term of <LCS-UPP message>.

**2. Reason for Change**

For LCS-UPP procedures, the term <LCS-UPP message> is used in TS 24.572 but still in one place, it uses < LCS-UP message>.

**3. Conclusions**

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.572 v1.0.0.

\* \* \* First Change \* \* \* \*

### 7.2.1 LCS-UPP message transport in IPv4, IPv6 or IPv4v6 PDU session

In order to send an LCS-UPP message over a PDU session of IPv4, IPv6 or IPv4v6 PDU session type, the UE shall establish the TLS connection. The UE and the LMF shall use the TLS connection to exchange LCS-UPP messages.

\* \* \* End of Changes \* \* \* \*