**3GPP TSG-CT WG1 Meeting #146C1-240302**

**Online , 22– 26 January 2024**

**Source: Lenovo**

**Title: Restructuring of resource URI for ADAES**

**Spec: 3GPP TS 24.559V0.3.1**

**Agenda item: 18.2.29**

**Document for: Agreement**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

Resource URI needs to be modified to cover all ADAE features

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.559V0.3.1.

\* \* \* First Change \* \* \* \*

#### 7.1.3.1 Overview

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 7.1.3.1-1 depicts the resource URI structure of the ADAE\_ServiceConfiguration API.



Figure 7.1.3.1-1: Resource URI structure of the ADAE\_ServiceConfiguration API

Table 7.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 7.1.3.1-1: Resources and methods overview



|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Application performance event subscription | /application-performance | POST | Subscription to the VAL performance analytics event |
| Individual application performance event subscription | /application-performance/{appPerfId} | DELETE | Deletes an individual VAL performance analytics event |
| Edge load event subscription | /edge-load | POST | Subscription to the edge load data collection event |
| Individual edge load event subscription | /edge-load/{edgeLdId} | DELETE | Deletes an individual edge load data collection subscription |
| Service experience | /service-experience | POST | Configure triggers for reports on the service experience information |
| Individual service experience | /service-experience/{srvTrigId} | DELETE | Delete an individual trigger-configuration for service experience report |

\* \* \* End of Changes \* \* \* \*