**3GPP TSG-CT WG1 Meeting #146C1-24xxxx**

**Online, 22– 26 January 2024**

**Source: ZTE, Nokia, Nokia Shanghai Bell**

**Title: General description on located UE discovery and selection**

**Spec: 3GPP TS 24.514 v0.5.0**

**Agenda item: 18.2.23**

**Document for: Agreement**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

General clause (6.4.1) for located UE discovery and selection gives description on the logical of located UE selection by target UE or LMF which is more appropriate to be specified in detailed procedure in following subclauses.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.514 v0.5.0.

\* \* \* First Change \* \* \* \*

### 6.4.1 General

Located UE selection can be performed by target UE or by LMF as specified in clause 5.2.2 of 3GPP TS 23.586 [2]. Whether the selection is done by the LMF or by the target UE, is based on the procedure in which the located UE selection is performed as specified in clause 6.20 of 3GPP TS 23.273 [11].

Procedure of target UE selecting located UE is specified in clause 6.4.2.1.

Procedure of LMF selecting located UE is specified in clause 6.4.2.2.

\* \* \* End of Changes \* \* \* \*