**3GPP TSG-CT WG3 Meeting #108-eC3-201433**

**E-Meeting, 19th – 28th February 2020 *(revision of C3-201192)***

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.512** | **CR** | **0427** | **rev** | **1** | **Current version:** | **16.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | TSCAI input container and TSN QoS container | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | C3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | Vertical\_LAN | | | | |  | ***Date:*** | | | 27 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | 6 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As defined in 23.501, clause 5.27.2, the TSC assistance information is provided from the SMF to 5G-AN upon QoS flow establishment, where the TSCAI parameters are set according to corresponding parameters obtained from the AF.  23.503, clause 6.3.1 specifies in table 6.3.1 the TSN AF container, which contains the Burst Arrival Time, Periodicity and Flow direction. This container defines the parameters provided by TSN AF and is included within a PCC rule.  23.503 clause 6.2.1.2 specifies that the TSN AF parameters received by the PCF are: Burst Arrival time, Periodicity, flow direction and delay requirement. Clause 6.1.3.23 specifes that “The PCF receives a request from the TSN AF that includes … TSN QoS parameters, i.e. priority and delay.  Burst Arrival Time, Periodicity and Flow direction are defined in TS 29.514 under the TSN QoS container concept. This is a bit confussing, because none of the attributes represent QoS profile data. It is proposed to rename it by TSCAI input container.  The specification is also missing information about how the QoS information included in the PCC rule is derived from the information received from the TSN AF. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clause 4.2.3.24 is renamed to Provisioning of TSCAI Input information and TSC QoS related data. In addition, it is clarified that the TSC traffic QoS information received from the TSN AF is used to derive the 5QI of the PCC rule, and the TSCAI input information is transparently added to the corresponding PCC rule. TSCAI input information is identified by the “tscaiInputUl” and “tscaiInputDl” attributes.  5.6.2.6 PccRule type is updated to include the “tscaiInputUl” and “tscaiInputDl” attributes.  OpenAPI file is updated accordingly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete and incorrect TSC traffic pattern and QoS information. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 3.2, 4.2.3.1, 4.2.3.24, 5.6.1, 5.6.26, A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR impacts the OpenAPI file with a backwards compatible feature. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):W**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5G-RG 5G Residential Gateway

AF Application Function

AMF Access and Mobility Management Function

API Application Programming Interface

ATSSS Access Traffic Steering, Switching, Splitting

ATSSS-LL ATSSS Low-Layer

BBF Broadband Forum

CHEM Coverage and Handoff Enhancements using Multimedia error robustness feature

CHF Charging Function

DN-AAA Data Network Authentication, Authorization and Accounting

DNN Data Network Name

DS-TT Device-side TSN translator

ePDG evolved Packet Data Gateway

FN-RG Fixed Network Residential Gateway

GFBR Guaranteed Flow Bit Rate

GUAMI Globally Unique AMF Identifier

HFC Hybrid Fiber Coax

HTTP Hypertext Transfer Protocol

MA Multi-Access

MPTCP Multi-Path TCP Protocol

NAS Non-Access-Stratum

NEF Network Exposure Function

NF Network Function

NID Network Identifier

NRF Network Repository Function

NW-TT Network-side TSN translator

PCC Policy and Charging Control

PCF Policy Control Function

PSAP Public Safety Answering Point

QoS Quality of Service

RTT Round-Trip Time

SDF Service Data Flow

SMF Session Management Function

SNPN Stand-alone Non-Public Network

S-NSSAI Single Network Slice Selection Assistance Information

TSC Time Sensitive Communication

TSCAI Time Sensitive Communication Assistance Information

TSN Time Sensitive Networking

TSN GM TSN Grand Master

UDM Unified Data Management

UDR Unified Data Repository

UE User Equipment

URLLC Ultra Reliable Low Latency Communication

W-5GAN Wireline 5G Access Network

W-5GBAN Wireline BBF Access Network

W-5GCAN Wireline 5G Cable Access Network

W-AGF Wireline Access Gateway Function

\*\*\* 2nd Change \*\*\*

#### 4.2.3.1 General

The UpdateNotify service operation provides updated Session Management related policies to the NF service consumer (SMF) or triggers the deletion of the context of SM related policies. The POST method is used for both, update and delete operations.

The following procedures using the Npcf\_SMPolicyControl\_UpdateNotify service operation are supported:

- PCF initiated update of the policies associated with the PDU session.

- PCF initiated deletion of SM Policy Association of a PDU session.

- Provisioning of PCC rules.

- Provisioning of policy control request triggers.

- Provisioning of revalidation time.

- Policy provisioning and enforcement of authorized AMBR per PDU session.

- Policy provisioning and enforcement of authorized default QoS.

- Provisioning of PCC rule for Application Detection and Control.

- 3GPP PS Data Off Support.

- IMS Emergency Session Support.

- Request Access Network Information.

- Request Usage Monitoring Control.

- Request for the result of PCC rule removal.

- Access Network Charging Identifier request.

- Request for the successful resource allocation notification.

- IMS Restoration Support.

- P-CSCF Restoration Enhancement Support.

- Access traffic steering, switching and splitting support.

- Policy provisioning and enforcement of the AF session with required QoS.

- Forwarding of TSN information received from AF.

- Provisioning of TSCAI input information and TSC QoS related data.

- Policy provisioning and enforcement of the AF session with required QoS.

\*\*\* 3rd Change \*\*\*

#### 4.2.3.24 Provisioning of TSCAI input information and TSC QoS related data

The PCF may receive the TSCAI input information and TSC traffic QoS related information from the AF.

If the feature "TimeSensitiveNetworking" is supported by both the SMF and PCF as described in subclause 5.8, the PCF shall provide for the derived PCC rule(s):

- a 5QI corresponding to a delay-critical GBR derived from the TSC traffic QoS information received from the TSN AF encoded within a QosData type referred in the "refQosData" of the PCC rule; and

- the TSCAI input information container as received from the TSN AF encoded in the "tscaiInputUl" attribute and/or "tscaiInputDl" attribute of the PCC rule.

The SMF shall convert the received TSCAI input information from the TSN GM into the 5G GM and, for the PCC rules bound to the same QoS flow, shall forward the derived TSCAI parameters to the AN-RAN.

The provisioning of TSCAI input information and TSC traffic QoS configuration per PCC Rule shall be performed using the PCC rule provisioning procedure as defined in subclause 4.2.6.2.1.

\*\*\* 4th Change \*\*\*

### 5.6.1 General

This subclause specifies the application data model supported by the API.

The Npcf\_SMPolicyControl API allows the SMF to retrieve the session management related policy from the PCF as defined in 3GPP TS 23.503 [6].

Table 5.6.1-1 specifies the data types defined for the Npcf\_SMPolicyControl service based interface protocol.

Table 5.6.1-1: Npcf\_SMPolicyControl specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| 5GSmCause | 5.6.3.2 | Indicates the 5GSM cause code value. | RAN-NAS-Cause |
| AccNetChargingAddress | 5.6.2.35 | Identifies the address of the network node performing charging and used for charging applications. |  |
| AccNetChId | 5.6.2.23 | Contains the access network charging identifier for the PCC rule(s) or whole PDU session. |  |
| AccuUsageReport | 5.6.2.18 | Contains the accumulated usage report information. | UMC |
| AfSigProtocol | 5.6.3.10 | Indicates the protocol used for signalling between the UE and the AF. | ProvAFsignalFlow |
| AuthorizedDefaultQos | 5.6.2.34 | Authorized Default QoS. |  |
| ChargingData | 5.6.2.11 | Contains charging related parameters. |  |
| ChargingInformation | 5.6.2.17 | Contains the addresses of the charging functions. |  |
| ConditionData | 5.6.2.9 | Contains conditions for applicability of a rule. |  |
| CreditManagementStatus | 5.6.3.16 | Indicates the reason of the credit management session failure. |  |
| ErrorReport | 5.6.2.36 | Contains the rule reports. |  |
| FailureCause | 5.6.3.14 | Indicates the cause of the failure in a Partial Success Report. |  |
| FailureCode | 5.6.3.9 | Indicates the reason of the PCC rule failure. |  |
| FlowDirection | 5.6.3.3 | Indicates the direction of the service data flow. |  |
| FlowDirectionRm | 5.6.3.15 | This data type is defined in the same way as the "FlowDirection" data type, but with the OpenAPI "nullable: true" property. |  |
| FlowInformation | 5.6.2.14 | Contains the flow information. |  |
| MeteringMethod | 5.6.3.5 | Indicates the metering method. |  |
| MulticastAccessControl | 5.6.3.20 | Indicates whether the service data flow, corresponding to the service data flow template, is allowed or not allowed. | WWC |
| RequestedQosMonitoringParameter | 5.6.3.21 | Indicates the requested QoS monitoring parameters to be measured. | QosMonitoring |
| PacketFilterInfo | 5.6.2.30 | Contains the information from a single packet filter sent from the SMF to the PCF. |  |
| PartialSuccessReport | 5.6.2.33 | Includes the information reported by the SMF when some of the PCC rules are not successfully installed/activated. |  |
| PccRule | 5.6.2.6 | Contains the PCC rule information. |  |
| PduSessionRelCause | 5.6.3.24 | Contains the SMF PDU Session release cause. | PDUSessionRelCause |
| PolicyControlRequestTrigger | 5.6.3.6 | Contains the policy control request trigger(s). |  |
| QosCharacteristics | 5.6.2.16 | Contains QoS characteristics for a non-standardized or non-configured 5QI. |  |
| QosData | 5.6.2.8 | Contains the QoS parameters. |  |
| QosMonitoringData | 5.6.2.40 | Contains QoS monitoring related control information. | QosMonitoring |
| QosMonitoringReport | 5.6.2.42 | Contains QoS monitoring reporting information. | QosMonitoring |
| QosNotificationControlInfo | 5.6.2.32 | Contains the QoS Notification Control Information. |  |
| RanNasRelCause | 5.6.2.28 | Contains the RAN/NAS release cause. | RAN-NAS-Cause |
| RedirectAddressType | 5.6.3.12 | Indicates the redirect address type. |  |
| RedirectInformation | 5.6.2.13 | Contains the redirect information. |  |
| ReportingFrequency | 5.6.3.22 | Indicates the frequency for the reporting | QosMonitoring |
| ReportingLevel | 5.6.3.4 | Indicates the reporting level. |  |
| RequestedQos | 5.6.2.31 | Contains the QoS information requested by the UE. |  |
| RequestedQosMonitoringParameter | 5.6.3.21 | Indicates the requested QoS monitoring parameters to be measured. | QosMonitoring |
| RequestedRuleData | 5.6.2.24 | Contains rule data requested by the PCF to receive information associated with PCC rules. |  |
| RequestedRuleDataType | 5.6.3.7 | Contains the type of rule data requested by the PCF. |  |
| RequestedUsageData | 5.6.2.25 | Contains usage data requested by the PCF requesting usage reports for the corresponding usage monitoring data instances. |  |
| RuleOperation | 5.6.3.11 | Indicates a UE initiated resource operation that causes a request for PCC rules. |  |
| RuleReport | 5.6.2.27 | Reports the status of PCC. |  |
| RuleStatus | 5.6.3.8 | Indicates the status of PCC or session rule. |  |
| ServingNfIdenty | 5.6.2.38 | Contains the serving Network Function identity. |  |
| SessionRule | 5.6.2.7 | Contains session level policy information. |  |
| SessionRuleFailureCode | 5.6.3.38 | Indicates the reason of the session rule failure. |  |
| SessionRuleReport | 5.6.2.37 | Reports the status of session rule. |  |
| SmPolicyAssociationReleaseCause | 5.6.3.23 | Represents the cause why the PCF requests the termination of the SM policy association. |  |
| SmPolicyControl | 5.6.2.2 | Contains the parameters to request the SM policies and the SM policies authorized by the PCF. |  |
| SmPolicyContextData | 5.6.2.3 | Contains the parameters to create individual SM policy resource. |  |
| SmPolicyDecision | 5.6.2.4 | Contains the SM policies authorized by the PCF. |  |
| SmPolicyNotification | 5.6.2.5 | Contains the update of the SM policies. |  |
| SmPolicyDeleteData | 5.6.2.15 | Contains the parameters to be sent to the PCF when the individual SM policy is deleted. |  |
| SmPolicyUpdateContextData | 5.6.2.19 | Contains the met policy control request trigger(s) and corresponding new value(s) or the error report of the policy enforcement. |  |
| SteeringFunctionality | 5.6.3.18 | Indicates functionality to support traffic steering, switching and splitting determined by the PCF. | ATSSS |
| SteeringMode | 5.6.2.39 | Contains the steering mode value and parameters determined by the PCF. | ATSSS |
| SteeringModeValue | 5.6.3.19 | Indicates the steering mode value determined by the PCF. | ATSSS |
| TerminationNotification | 5.6.2.21 | Termination Notification. |  |
| TrafficControlData | 5.6.2.10 | Contains parameters determining how flows associated with a PCCRule are treated (blocked, redirected, etc). |  |
| TsnBridgeInfo | 5.6.2.41 | Contains parameters that describe and identify the TSN bridge. | TimeSensitiveNetworking |
| UeCampingRep | 5.6.2.26 | Contains the current applicable values corresponding to the policy control request triggers. |  |
| UeInitiatedResourceRequest | 5.6.2.29 | Indicates a UE requests specific QoS handling for selected SDF. |  |
| UpPathChgEvent | 5.6.2.20 | Contains the UP path change event subscription from the AF. | TSC |
| UsageMonitoringData | 5.6.2.12 | Contains usage monitoring related control information. | UMC |
| Volume | 3GPP TS 29.122 [32] | Unsigned integer identifying a volume in units of bytes. |  |
| VolumeRm | 3GPP TS 29.122 [32] | This data type is defined in the same way as the "VolumeRm" data type, but with the OpenAPI "nullable: true" property. |  |

Table 5.6.1-2 specifies data types re-used by the Npcf\_SMPolicyControl service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Npcf\_SMPolicyControl service based interface.

Table 5.6.1-2: Npcf\_SMPolicyControl re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| 5GMmCause | 3GPP TS 29.571 [11] | Contains the cause value of 5GMM protocol. | RAN-NAS-Cause |
| 5Qi | 3GPP TS 29.571 [11] | Unsigned integer representing a 5G QoS Identifier (see subclause 5.7.2.1 of 3GPP TS 23.501 [2]), within the range 0 to 255. |  |
| 5QiPriorityLevel | 3GPP TS 29.571 [11] | Unsigned integer indicating the 5QI Priority Level (see subclauses 5.7.3.3 and 5.7.4 of 3GPP TS 23.501 [2]), within the range 1 to 127.  Values are ordered in decreasing order of priority, i.e. with 1 as the highest priority and 127 as the lowest priority. |  |
| 5QiPriorityLevelRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "5QiPriorityLevel" data type, but with the OpenAPI "nullable: true" property. |  |
| AccessType | 3GPP TS 29.571 [11] | The identification of the type of access network. |  |
| Ambr | 3GPP TS 29.571 [11] | Session AMBR. |  |
| AnGwAddress | 3GPP TS 29.514 [17] | Carries the control plane address of the access network gateway. (NOTE 1) |  |
| ApplicationChargingId | 3GPP TS 29.571 [11] | Application provided charging identifier allowing correlation of charging information. | AF\_Charging\_Identifier |
| Arp | 3GPP TS 29.571 [11] | ARP. |  |
| AverWindow | 3GPP TS 29.571 [11] | Averaging Window. |  |
| AverWindowRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "AverWindow" data type, but with the OpenAPI "nullable: true" property. |  |
| Bytes | 3GPP TS 29.571 [11] | String with format "byte". | TimeSensitiveNetworking |
| BitRate | 3GPP TS 29.571 [11] | String representing a bit rate that shall be formatted as follows:  pattern: "^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$"  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps". |  |
| BitRateRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "BitRate" data type, but with the OpenAPI "nullable: true" property. |  |
| ChargingId | 3GPP TS 29.571 [11] | Charging identifier allowing correlation of charging information. |  |
| ContentVersion | 3GPP TS 29.514 [17] | Indicates the content version of a PCC rule. It uniquely identifies a version of the PCC rule as defined in subclause 4.2.6.2.14. | RuleVersioning |
| DateTime | 3GPP TS 29.571 [11] | String with format "date-time" as defined in OpenAPI Specification [10]. |  |
| DateTimeRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "DateTime" data type, but with the OpenAPI "nullable: true" property. |  |
| DnaiChangeType | 3GPP TS 29.571 [11] | Describes the types of DNAI change. |  |
| Dnn | 3GPP TS 29.571 [11] | The DNN the user is connected to. |  |
| DurationSec | 3GPP TS 29.571 [11] | Identifies a period of time in units of seconds. |  |
| DurationSecRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "DurationSec" data type, but with the OpenAPI "nullable: true" property. |  |
| EthFlowDescription | 3GPP TS 29.514 [17] | Defines a packet filter for an Ethernet flow. (NOTE 2) |  |
| ExtMaxDataBurstVol | 3GPP TS 29.571 [11] | Maximum Data Burst Volume. | EMDBV |
| ExtMaxDataBurstVolRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "ExtMaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. | EMDBV |
| FinalUnitAction | 3GPP TS 32.291 [19] | Indicates the action to be taken when the user's account cannot cover the service cost. |  |
| FlowStatus | 3GPP TS 29.514 [17] | Describes whether the IP flow(s) are enabled or disabled. The value "REMOVED" is not applicable to Npcf\_SMPolicyControl service. |  |
| Gpsi | 3GPP TS 29.571 [11] | Identifies a GPSI. |  |
| GroupId | 3GPP TS 29.571 [11] | Identifies a group of internal globally unique ID. |  |
| Guami | 3GPP TS 29.571 [11] | Globally Unique AMF Identifier. |  |
| IpIndex | 3GPP TS 29.519 [15] | Information that identifies which IP pool or external server is used to allocate the IP address. |  |
| Ipv4Addr | 3GPP TS 29.571 [11] | Identifies an Ipv4 address. |  |
| Ipv6Addr | 3GPP TS 29.571 [11] | Identifies an IPv6 address. |  |
| Ipv6Prefix | 3GPP TS 29.571 [11] | The Ipv6 prefix allocated for the user. |  |
| MacAddr48 | 3GPP TS 29.571 [11] | MAC Address. |  |
| MaxDataBurstVol | 3GPP TS 29.571 [11] | Maximum Data Burst Volume. |  |
| MaxDataBurstVolRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "MaxDataBurstVol" data type, but with the OpenAPI "nullable: true" property. |  |
| NfInstanceId | 3GPP TS 29.571 [11] | The NF instance identifier. |  |
| NgApCause | 3GPP TS 29.571 [11] | Contains the cause value of NgAP protocol. | RAN-NAS-Cause |
| PacketDelBudget | 3GPP TS 29.571 [11] | Packet Delay Budget. |  |
| PacketErrRate | 3GPP TS 29.571 [11] | Packet Error Rate. |  |
| PacketLossRateRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "PacketLossRate" data type, but with the OpenAPI "nullable: true" property. |  |
| PduSessionId | 3GPP TS 29.571 [11] | The identification of the PDU session. |  |
| PduSessionType | 3GPP TS 29.571 [11] | Indicate the type of a PDU session. |  |
| Pei | 3GPP TS 29.571 [11] | The Identification of a Permanent Equipment. |  |
| PlmnIdNid | 3GPP TS 29.571 [11] | The identification of the Network. PLMN Identity, and for SNPN NID. |  |
| PolicyAssociationReleaseCause | 3GPP TS 29.507 [25] | The cause why the PCF requests the termination of the policy association. |  |
| PresenceInfo | 3GPP TS 29.571 [11] | Contains the information which describes a Presence Reporting Area. | PRA |
| PresenceInfoRm | 3GPP TS 29.571 [11] | This data type is defined in the same way as the "PresenceInfo" data type, but with the OpenAPI "nullable: true" property. |  |
| QosNotifType | 3GPP TS 29.514 [17] | Indicates whether the GBR targets for the indicated SDFs are "NOT\_GUARANTEED" or "GUARANTEED" again. |  |
| QosResourceType | 3GPP TS 29.571 [11] | Indicates whether the resource type is GBR, delay critical GBR, or non-GBR. |  |
| RatingGroup | 3GPP TS 29.571 [11] | Identifier of a rating group. |  |
| RatType | 3GPP TS 29.571 [11] | The identification of the RAT type. |  |
| RouteToLocation | 3GPP TS 29.571 [11] | A traffic routes to applications location. | TSC |
| ServiceId | 3GPP TS 29.571 [11] | Identifier of a service. |  |
| Snssai | 3GPP TS 29.571 [11] | Identifies the S-NSSAI. |  |
| SubscribedDefaultQos | 3GPP TS 29.571 [11] | Subscribed Default QoS. |  |
| Supi | 3GPP TS 29.571 [11] | The identification of the user (i.e. IMSI, NAI). |  |
| SupportedFeatures | 3GPP TS 29.571 [11] | Used to negotiate the applicability of the optional features defined in table 5.8-1. |  |
| TraceData | 3GPP TS 29.571 [11] |  |  |
| TimeZone | 3GPP TS 29.571 [11] | Contains the user time zone information. |  |
| TscaiInputContainer | 3GPP TS 29.514 [17] | TSCAI Input information. | TimeSensitiveNetworking |
| Uinteger | 3GPP TS 29.571 [11] | Unsigned Integer. | TimeSensitiveNetworking |
| Uri | 3GPP TS 29.571 [11] | URI. |  |
| UserLocation | 3GPP TS 29.571 [11] | Contains the user location. |  |
| NOTE 1: "AnGwAddr" data structure is only applicable to the 5GS and EPC/E-UTRAN interworking scenario as defined in Annex B.  NOTE 2: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange as specified in subclause 5.8 shall be supported. | | | |

\*\*\* 5th Change \*\*\*

#### 5.6.2.6 Type PccRule

Table 5.6.2.6-1: Definition of type PccRule

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| flowInfos | array(FlowInformation) | C | 1..N | An array of IP flow packet filter information. (NOTE 3) |  |
| appId | string | C | 0..1 | A reference to the application detection filter configured at the UPF. (NOTE 3) | ADC |
| contVer | ContentVersion | O | 0..1 | Indicates the content version of the PCC rule. | RuleVersioning |
| pccRuleId | string | M | 1 | Univocally identifies the PCC rule within a PDU session. |  |
| precedence | Uinteger | O | 0..1 | Determines the order in which this PCC rule is applied relative to other PCC rules within the same PDU session. It shall be included if the "flowInfos" attribute is included or may be included if the "appId" attribute is included when the PCF initially provisions the PCC rule. (NOTE 2) (NOTE 4) |  |
| afSigProtocol | AfSigProtocol | O | 0..1 | Indicates the protocol used for signalling between the UE and the AF. The default value "NO\_INFORMATION" shall apply, if the attribute is not present and has not been supplied previously. | ProvAFsignalFlow |
| appReloc | boolean | O | 0..1 | It indicates that the application can be relocated once a location of the application is selected by the 5GC when it is included and set to "true". Indication of application relocation possibility. The default value "false" shall apply, if the attribute is not present and has not been supplied previously. | TSC |
| addrPreserInd | boolean | O | 0..1 | Indicates whether UE IP address should be preserved.  This attribute shall set to "true" if preserved, otherwise, set to "false".  The default value "false" shall apply, if the attribute is not present and has not been supplied previously. | URLLC |
| refQosData | array(string) | O | 1..N | A reference to the QoSData policy type decision type. It is the qosId described in subclause 5.6.2.8.  (NOTE 1) |  |
| refAltQosParams | array(string) | O | 1..N | A Reference to the QoS Data policy decision type for the Alternative QoS parameter sets of the service data flow. Only the "qosId" attribute, "5qi" attribute, "maxbrUl" attribute, "maxbrDl" attribute, "gbrUl" attribute and "gbrDl" attribute are applicable within the QosData data type. This data type represents an ordered list, where the lower the index of the array for a given entry, the higher the priority. | AuthorizationWithRequiredQoS |
| refTcData | array(string) | O | 1..N | A reference to the TrafficControlData policy decision type. It is the tcId described in subclause 5.6.2.10.  (NOTE 1) |  |
| refChgData | array(string) | O | 1..N | A reference to the ChargingData policy decision type. It is the chgId described in subclause 5.6.2.11.  (NOTE 1) |  |
| refChgN3gData | array(string) | O | 1..N | A reference to the ChargingData policy decision type only applicable to Non-3GPP access. It is the chgId described in subclause 5.6.2.11.  (NOTE 1) (NOTE 5) | ATSSS |
| refUmData | array(string) | O | 1..N | A reference to UsageMonitoringData policy decision type. It is the umId described in subclause 5.6.2.12.  (NOTE 1) |  |
| refUmN3gData | array(string) | O | 1..N | A reference to UsageMonitoringData policy decision type only applicable to Non-3GPP access. It is the umId described in subclause 5.6.2.12.  (NOTE 1) (NOTE 6) | ATSSS |
| refCondData | string | O | 0..1 | A reference to the condition data. It is the condId described in subclause 5.6.2.9. |  |
| refQoSMon | array(string) | O | 1..N | A reference to QoSMonitoringData policy decision type. It is the qsId described in subclause 5.6.2.40.  (NOTE 1) | QosMonitoring |
| tscaiInputUl | TscaiInputContainer | O | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress interface of the DS-TT/UE (uplink flow direction). | TimeSensitiveNetworking |
| tscaiInputDl | TscaiInputContainer | O | 0..1 | Transports TSCAI input parameters for TSC traffic at the ingress of the NW-TT (downlink flow direction). | TimeSensitiveNetworking |
| NOTE 1: Arrays are only introduced for future compatibility. In this release of the specification the maximum number of elements in the array is 1.  NOTE 2: For a PCC rule with the "appId" attribute, the precedence can be preconfigured in SMF or provided in the PCC rule from PCF. The precedence provided by the PCF shall take precedence.  NOTE 3: Either the "flowInfos" attribute or "appId" attribute shall be supplied by the PCF when the PCC rule is initially provisioned. If the "appId" attribute is supplied, the PCF shall not modify the application identifier supplied within the "appId" attribute later.  NOTE 4: The "precedence" attribute is used to specify the precedence of the PCC rule among all PCC rules associated with the PDU session. It includes an integer value in the range from 0 to 255 (decimal). The higher the value of the "precedence" attribute, the lower the precedence of that PCC rule is. The precedence value range from 70 to 99 (decimal) shall be used for the PCC rules subject to Reflective QoS.  NOTE 5: For a MA PDU Session, Charging Data decision referred by the "refChgData" attribute applies to both accesses if there is no "refChgN3gData" attribute included. If there is a "refChgN3gData" attribute included, the Charging Data decision referred by the "refChgN3gData" attribute applies to non-3GPP access and the Charging Data decision referred by the "refChgData" attribute applies to 3GPP access. The value(s) of attribute(s) within the Charging Data decision except the “chgId" attribute referred by the "refChgN3gData" attribute shall be the same as the one(s) within the Charging Data decision referred by the "refChgData" attribute.  NOTE 6: For a MA PDU Session, Usage Monitoring Data decision referred by the "refUmData" attribute applies to both accesses if there is no "refUmN3gData" attribute included. If there is a "refUmN3gData" attribute included, the Usage Monitoring Data decision referred by the "refUmN3gData" attribute applies to non-3GPP access and the Usage Monitoring Data decision referred by the "refUmData" attribute applies to 3GPP access. | | | | | | | |

\*\*\* 6th Change \*\*\*

# A.2 Npcf\_SMPolicyControl API

openapi: 3.0.0

info:

title: Npcf\_SMPolicyControl API

version: 1.1.1.alpha-4

description: |

Session Management Policy Control Service

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.512 V16.3.0; 5G System; Session Management Policy Control Service.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.512/'

security:

- {}

- oAuth2Clientcredentials:

- npcf-smpolicycontrol

servers:

- url: '{apiRoot}/npcf-smpolicycontrol/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

paths:

/sm-policies:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyContextData'

responses:

'201':

description: Created

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyDecision'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'308':

description: Permanent Redirect

headers:

Location:

description: 'Contains the URI of the PCF within the existing PCF binding information stored in the BSF for the same UE ID, S-NSSAI and DNN combination '

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

description: Not Found

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

SmPolicyUpdateNotification:

'{$request.body#/notificationUri}/update':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyNotification'

responses:

'200':

description: OK. The current applicable values corresponding to the policy control request trigger is reported

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/UeCampingRep'

- type: array

items:

$ref: '#/components/schemas/PartialSuccessReport'

minItems: 1

'204':

description: No Content, Notification was succesfull

'400':

description: Bad Request.

content:

application/json:

schema:

$ref: '#/components/schemas/ErrorReport'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

SmPolicyControlTerminationRequestNotification:

'{$request.body#/notificationUri}/terminate':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TerminationNotification'

responses:

'204':

description: No Content, Notification was succesful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-policies/{smPolicyId}:

get:

parameters:

- name: smPolicyId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyControl'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-policies/{smPolicyId}/update:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyUpdateContextData'

parameters:

- name: smPolicyId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'200':

description: OK. Updated policies are returned

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyDecision'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/sm-policies/{smPolicyId}/delete:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SmPolicyDeleteData'

parameters:

- name: smPolicyId

in: path

description: Identifier of a policy association

required: true

schema:

type: string

responses:

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2Clientcredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-smpolicycontrol: Access to the Npcf\_SMPolicyControl API

schemas:

SmPolicyControl:

type: object

properties:

context:

$ref: '#/components/schemas/SmPolicyContextData'

policy:

$ref: '#/components/schemas/SmPolicyDecision'

required:

- context

- policy

SmPolicyContextData:

type: object

properties:

accNetChId:

$ref: '#/components/schemas/AccNetChId'

chargEntityAddr:

$ref: '#/components/schemas/AccNetChargingAddress'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

interGrpIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

pduSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

pduSessionType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

chargingcharacteristics:

type: string

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

pei:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

ipv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6AddressPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

ipDomain:

type: string

description: Indicates the IPv4 address domain

subsSessAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

authProfIndex:

type: string

description: Indicates the DN-AAA authorization profile index

subsDefQos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

numOfPackFilter:

type: integer

description: Contains the number of supported packet filter for signalled QoS rules.

online:

type: boolean

description: If it is included and set to true, the online charging is applied to the PDU session.

offline:

type: boolean

description: If it is included and set to true, the offline charging is applied to the PDU session.

3gppPsDataOffStatus:

type: boolean

description: If it is included and set to true, the 3GPP PS Data Off is activated by the UE.

refQosIndication:

type: boolean

description: If it is included and set to true, the reflective QoS is supported by the UE.

traceReq:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

sliceInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

qosFlowUsage:

$ref: '#/components/schemas/QosFlowUsage'

servNfId:

$ref: '#/components/schemas/ServingNfIdentity'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

smfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

recoveryTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

required:

- supi

- pduSessionId

- pduSessionType

- dnn

- notificationUri

- sliceInfo

SmPolicyDecision:

type: object

properties:

sessRules:

type: object

additionalProperties:

$ref: '#/components/schemas/SessionRule'

minProperties: 1

description: A map of Sessionrules with the content being the SessionRule as described in subclause 5.6.2.7.

pccRules:

type: object

additionalProperties:

$ref: '#/components/schemas/PccRule'

minProperties: 1

description: A map of PCC rules with the content being the PCCRule as described in subclause 5.6.2.6.

nullable: true

pcscfRestIndication:

type: boolean

description: If it is included and set to true, it indicates the P-CSCF Restoration is requested.

qosDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/QosData'

minProperties: 1

description: Map of QoS data policy decisions.

chgDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/ChargingData'

minProperties: 1

description: Map of Charging data policy decisions.

nullable: true

chargingInfo:

$ref: '#/components/schemas/ChargingInformation'

traffContDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/TrafficControlData'

minProperties: 1

description: Map of Traffic Control data policy decisions.

umDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/UsageMonitoringData'

minProperties: 1

description: Map of Usage Monitoring data policy decisions.

nullable: true

qosChars:

type: object

additionalProperties:

$ref: '#/components/schemas/QosCharacteristics'

minProperties: 1

description: Map of QoS characteristics for non standard 5QIs. This map uses the 5QI values as keys.

qosMonDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/QosMonitoringData'

minProperties: 1

description: Map of QoS Monitoring data policy decisions.

nullable: true

reflectiveQoSTimer:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

conds:

type: object

additionalProperties:

$ref: '#/components/schemas/ConditionData'

minProperties: 1

description: A map of condition data with the content being as described in subclause 5.6.2.9.

nullable: true

revalidationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

offline:

type: boolean

description: Indicates the offline charging is applicable to the PDU session or PCC rule.

online:

type: boolean

description: Indicates the online charging is applicable to the PDU session or PCC rule.

policyCtrlReqTriggers:

type: array

items:

$ref: '#/components/schemas/PolicyControlRequestTrigger'

minItems: 1

description: Defines the policy control request triggers subscribed by the PCF.

nullable: true

lastReqRuleData:

type: array

items:

$ref: '#/components/schemas/RequestedRuleData'

minItems: 1

description: Defines the last list of rule control data requested by the PCF.

lastReqUsageData:

$ref: '#/components/schemas/RequestedUsageData'

praInfos:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfoRm'

minProperties: 1

description: Map of PRA information.

nullable: true

ipv4Index:

$ref: 'TS29519\_Policy\_Data.yaml#/components/schemas/IpIndex'

ipv6Index:

$ref: 'TS29519\_Policy\_Data.yaml#/components/schemas/IpIndex'

qosFlowUsage:

$ref: '#/components/schemas/QosFlowUsage'

relCause:

$ref: '#/components/schemas/SmPolicyAssociationReleaseCause'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

SmPolicyNotification:

type: object

properties:

resourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

smPolicyDecision:

$ref: '#/components/schemas/SmPolicyDecision'

PccRule:

type: object

properties:

flowInfos:

type: array

items:

$ref: '#/components/schemas/FlowInformation'

minItems: 1

description: An array of IP flow packet filter information.

appId:

type: string

description: A reference to the application detection filter configured at the UPF.

contVer:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

pccRuleId:

type: string

description: Univocally identifies the PCC rule within a PDU session.

precedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

afSigProtocol:

$ref: '#/components/schemas/AfSigProtocol'

appReloc:

type: boolean

description: Indication of application relocation possibility.

refQosData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to the QoSData policy type decision type. It is the qosId described in subclause 5.6.2.8.

refAltQosParams:

type: array

items:

type: string

minItems: 1

description: A Reference to the QoS Data policy decision type for the Alternative QoS parameter sets of the service data flow.

refTcData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to the TrafficControlData policy decision type. It is the tcId described in subclause 5.6.2.10.

refChgData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to the ChargingData policy decision type. It is the chgId described in subclause 5.6.2.11.

nullable: true

refChgN3gData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to the ChargingData policy decision type only applicable to Non-3GPP access if "ATSSS" feature is supported. It is the chgId described in subclause 5.6.2.11.

nullable: true

refUmData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to UsageMonitoringData policy decision type. It is the umId described in subclause 5.6.2.12.

nullable: true

refUmN3gData:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to UsageMonitoringData policy decision type only applicable to Non-3GPP access if "ATSSS" feature is supported. It is the umId described in subclause 5.6.2.12.

nullable: true

refCondData:

type: string

description: A reference to the condition data. It is the condId described in subclause 5.6.2.9.

nullable: true

refQosMon:

type: array

items:

type: string

minItems: 1

maxItems: 1

description: A reference to the QosMonitoringData policy type decision type. It is the qmId described in subclause 5.6.2.40.

nullable: true

addrPreserInd:

type: boolean

nullable: true

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

required:

- pccRuleId

nullable: true

SessionRule:

type: object

properties:

authSessAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

authDefQos:

$ref: '#/components/schemas/AuthorizedDefaultQos'

sessRuleId:

type: string

description: Univocally identifies the session rule within a PDU session.

refUmData:

type: string

description: A reference to UsageMonitoringData policy decision type. It is the umId described in subclause 5.6.2.12.

nullable: true

refUmN3gData:

type: string

description: A reference to UsageMonitoringData policy decision type to apply for Non-3GPP access. It is the umId described in subclause 5.6.2.12.

nullable: true

refCondData:

type: string

description: A reference to the condition data. It is the condId described in subclause 5.6.2.9.

nullable: true

required:

- sessRuleId

nullable: true

QosData:

type: object

properties:

qosId:

type: string

description: Univocally identifies the QoS control policy data within a PDU session.

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

maxbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

arp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

qnc:

type: boolean

description: Indicates whether notifications are requested from 3GPP NG-RAN when the GFBR can no longer (or again) be guaranteed for a QoS Flow during the lifetime of the QoS Flow.

priorityLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevelRm'

averWindow:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindowRm'

maxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVolRm'

reflectiveQos:

type: boolean

description: Indicates whether the QoS information is reflective for the corresponding service data flow.

sharingKeyDl:

type: string

description: Indicates, by containing the same value, what PCC rules may share resource in downlink direction.

sharingKeyUl:

type: string

description: Indicates, by containing the same value, what PCC rules may share resource in uplink direction.

maxPacketLossRateDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

maxPacketLossRateUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

defQosFlowIndication:

type: boolean

description: Indicates that the dynamic PCC rule shall always have its binding with the QoS Flow associated with the default QoS rule

extMaxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

required:

- qosId

nullable: true

ConditionData:

type: object

properties:

condId:

type: string

description: Uniquely identifies the condition data within a PDU session.

activationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

deactivationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

required:

- condId

nullable: true

TrafficControlData:

type: object

properties:

tcId:

type: string

description: Univocally identifies the traffic control policy data within a PDU session.

flowStatus:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowStatus'

redirectInfo:

$ref: '#/components/schemas/RedirectInformation'

addRedirectInfo:

type: array

items:

$ref: '#/components/schemas/RedirectInformation'

minItems: 1

muteNotif:

type: boolean

description: Indicates whether applicat'on's start or stop notification is to be muted.

trafficSteeringPolIdDl:

type: string

description: Reference to a pre-configured traffic steering policy for downlink traffic at the SMF.

nullable: true

trafficSteeringPolIdUl:

type: string

description: Reference to a pre-configured traffic steering policy for uplink traffic at the SMF.

nullable: true

routeToLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: A list of location which the traffic shall be routed to for the AF request

upPathChgEvent:

$ref: '#/components/schemas/UpPathChgEvent'

steerFun:

$ref: '#/components/schemas/SteeringFunctionality'

steerModeDl:

$ref: '#/components/schemas/SteeringMode'

steerModeUl:

$ref: '#/components/schemas/SteeringMode'

mulAccCtrl:

$ref: '#/components/schemas/MulticastAccessControl'

required:

- tcId

nullable: true

ChargingData:

type: object

properties:

chgId:

type: string

description: Univocally identifies the charging control policy data within a PDU session.

meteringMethod:

$ref: '#/components/schemas/MeteringMethod'

offline:

type: boolean

description: Indicates the offline charging is applicable to the PCC rule.

online:

type: boolean

description: Indicates the online charging is applicable to the PCC rule.

sdfHandl:

type: boolean

description: Indicates whether the service data flow is allowed to start while the SMF is waiting for the response to the credit request.

ratingGroup:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

reportingLevel:

$ref: '#/components/schemas/ReportingLevel'

serviceId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

sponsorId:

type: string

description: Indicates the sponsor identity.

appSvcProvId:

type: string

description: Indicates the application service provider identity.

afChargingIdentifier:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

afChargId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

required:

- chgId

nullable: true

UsageMonitoringData:

type: object

properties:

umId:

type: string

description: Univocally identifies the usage monitoring policy data within a PDU session.

volumeThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

volumeThresholdUplink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

volumeThresholdDownlink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

timeThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

monitoringTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTimeRm'

nextVolThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

nextVolThresholdUplink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

nextVolThresholdDownlink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/VolumeRm'

nextTimeThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

inactivityTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

exUsagePccRuleIds:

type: array

items:

type: string

minItems: 1

description: Contains the PCC rule identifier(s) which corresponding service data flow(s) shall be excluded from PDU Session usage monitoring. It is only included in the UsageMonitoringData instance for session level usage monitoring.

nullable: true

required:

- umId

nullable: true

RedirectInformation:

type: object

properties:

redirectEnabled:

type: boolean

description: Indicates the redirect is enable.

redirectAddressType:

$ref: '#/components/schemas/RedirectAddressType'

redirectServerAddress:

type: string

description: Indicates the address of the redirect server.

FlowInformation:

type: object

properties:

flowDescription:

$ref: '#/components/schemas/FlowDescription'

ethFlowDescription:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

packFiltId:

type: string

description: An identifier of packet filter.

packetFilterUsage:

type: boolean

description: The packet shall be sent to the UE.

tosTrafficClass:

type: string

description: Contains the Ipv4 Type-of-Service and mask field or the Ipv6 Traffic-Class field and mask field.

nullable: true

spi:

type: string

description: the security parameter index of the IPSec packet.

nullable: true

flowLabel:

type: string

description: the Ipv6 flow label header field.

nullable: true

flowDirection:

$ref: '#/components/schemas/FlowDirectionRm'

SmPolicyDeleteData:

type: object

properties:

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

userLocationInfoTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

ranNasRelCauses:

type: array

items:

$ref: '#/components/schemas/RanNasRelCause'

minItems: 1

description: Contains the RAN and/or NAS release cause.

accuUsageReports:

type: array

items:

$ref: '#/components/schemas/AccuUsageReport'

minItems: 1

description: Contains the usage report

pduSessRelCause:

$ref: '#/components/schemas/PduSessionRelCause'

QosCharacteristics:

type: object

properties:

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

resourceType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

priorityLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevel'

packetDelayBudget:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

packetErrorRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

averagingWindow:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindow'

maxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVol'

extMaxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

required:

- 5qi

- resourceType

- priorityLevel

- packetDelayBudget

- packetErrorRate

ChargingInformation:

type: object

properties:

primaryChfAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

secondaryChfAddress:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

required:

- primaryChfAddress

- secondaryChfAddress

AccuUsageReport:

type: object

properties:

refUmIds:

type: string

description: An id referencing UsageMonitoringData objects associated with this usage report.

volUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

volUsageUplink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

volUsageDownlink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

timeUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

nextVolUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

nextVolUsageUplink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

nextVolUsageDownlink:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

nextTimeUsage:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- refUmIds

SmPolicyUpdateContextData:

type: object

properties:

repPolicyCtrlReqTriggers:

type: array

items:

$ref: '#/components/schemas/PolicyControlRequestTrigger'

minItems: 1

description: The policy control reqeust trigges which are met.

accNetChIds:

type: array

items:

$ref: '#/components/schemas/AccNetChId'

minItems: 1

description: Indicates the access network charging identifier for the PCC rule(s) or whole PDU session.

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

relIpv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv4Address:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

description: Indicates the IPv4 address domain

ipv6AddressPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

relIpv6AddressPrefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

addIpv6AddrPrefixes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

addRelIpv6AddrPrefixes:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

relUeMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

subsSessAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

authProfIndex:

type: string

description: Indicates the DN-AAA authorization profile index

subsDefQos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

numOfPackFilter:

type: integer

description: Contains the number of supported packet filter for signalled QoS rules.

accuUsageReports:

type: array

items:

$ref: '#/components/schemas/AccuUsageReport'

minItems: 1

description: Contains the usage report

3gppPsDataOffStatus:

type: boolean

description: If it is included and set to true, the 3GPP PS Data Off is activated by the UE.

appDetectionInfos:

type: array

items:

$ref: '#/components/schemas/AppDetectionInfo'

minItems: 1

description: Report the start/stop of the application traffic and detected SDF descriptions if applicable.

ruleReports:

type: array

items:

$ref: '#/components/schemas/RuleReport'

minItems: 1

description: Used to report the PCC rule failure.

sessRuleReports:

type: array

items:

$ref: '#/components/schemas/SessionRuleReport'

minItems: 1

description: Used to report the session rule failure.

qncReports:

type: array

items:

$ref: '#/components/schemas/QosNotificationControlInfo'

minItems: 1

description: QoS Notification Control information.

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

userLocationInfoTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPraInfos:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

description: Reports the changes of presence reporting area.

ueInitResReq:

$ref: '#/components/schemas/UeInitiatedResourceRequest'

refQosIndication:

type: boolean

description: If it is included and set to true, the reflective QoS is supported by the UE. If it is included and set to false, the reflective QoS is revoked by the UE.

qosFlowUsage:

$ref: '#/components/schemas/QosFlowUsage'

creditManageStatus:

$ref: '#/components/schemas/CreditManagementStatus'

servNfId:

$ref: '#/components/schemas/ServingNfIdentity'

traceReq:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TraceData'

UpPathChgEvent:

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifCorreId:

type: string

description: It is used to set the value of Notification Correlation ID in the notification sent by the SMF.

dnaiChgType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

afAckInd:

type: boolean

required:

- notificationUri

- notifCorreId

- dnaiChgType

nullable: true

TerminationNotification:

type: object

properties:

resourceUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

cause:

$ref: '#/components/schemas/SmPolicyAssociationReleaseCause'

required:

- resourceUri

- cause

AppDetectionInfo:

type: object

properties:

appId:

type: string

description: A reference to the application detection filter configured at the UPF

instanceId:

type: string

description: Identifier sent by the SMF in order to allow correlation of application Start and Stop events to the specific service data flow description, if service data flow descriptions are deducible.

sdfDescriptions:

type: array

items:

$ref: '#/components/schemas/FlowInformation'

minItems: 1

description: Contains the detected service data flow descriptions if they are deducible.

required:

- appId

AccNetChId:

type: object

properties:

accNetChaIdValue:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

refPccRuleIds:

type: array

items:

type: string

minItems: 1

description: Contains the identifier of the PCC rule(s) associated to the provided Access Network Charging Identifier.

sessionChScope:

type: boolean

description: When it is included and set to true, indicates the Access Network Charging Identifier applies to the whole PDU Session

required:

- accNetChaIdValue

AccNetChargingAddress:

description: Describes the network entity within the access network performing charging

type: object

anyOf:

- required: [anChargIpv4Addr]

- required: [anChargIpv6Addr]

properties:

anChargIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

anChargIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

RequestedRuleData:

type: object

properties:

refPccRuleIds:

type: array

items:

type: string

minItems: 1

description: An array of PCC rule id references to the PCC rules associated with the control data.

reqData:

type: array

items:

$ref: '#/components/schemas/RequestedRuleDataType'

minItems: 1

description: Array of requested rule data type elements indicating what type of rule data is requested for the corresponding referenced PCC rules.

required:

- refPccRuleIds

- reqData

RequestedUsageData:

type: object

properties:

refUmIds:

type: array

items:

type: string

minItems: 1

description: An array of usage monitoring data id references to the usage monitoring data instances for which the PCF is requesting a usage report. This attribute shall only be provided when allUmIds is not set to true.

allUmIds:

type: boolean

description: Thooleanean indicates whether requested usage data applies to all usage monitoring data instances. When it's not included, it means requested usage data shall only apply to the usage monitoring data instances referenced by the refUmIds attribute.

UeCampingRep:

type: object

properties:

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

servNfId:

$ref: '#/components/schemas/ServingNfIdentity'

servingNetwork:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

userLocationInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

ueTimeZone:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

RuleReport:

type: object

properties:

pccRuleIds:

type: array

items:

type: string

minItems: 1

description: Contains the identifier of the affected PCC rule(s).

ruleStatus:

$ref: '#/components/schemas/RuleStatus'

contVers:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

minItems: 1

description: Indicates the version of a PCC rule.

failureCode:

$ref: '#/components/schemas/FailureCode'

finUnitAct:

$ref: 'TS32291\_Nchf\_ConvergedCharging.yaml#/components/schemas/FinalUnitAction'

ranNasRelCauses:

type: array

items:

$ref: '#/components/schemas/RanNasRelCause'

minItems: 1

description: indicates the RAN or NAS release cause code information.

required:

- pccRuleIds

- ruleStatus

RanNasRelCause:

type: object

properties:

ngApCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NgApCause'

5gMmCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5GMmCause'

5gSmCause:

$ref: '#/components/schemas/5GSmCause'

UeInitiatedResourceRequest:

type: object

properties:

pccRuleId:

type: string

ruleOp:

$ref: '#/components/schemas/RuleOperation'

precedence:

type: integer

packFiltInfo:

type: array

items:

$ref: '#/components/schemas/PacketFilterInfo'

minItems: 1

reqQos:

$ref: '#/components/schemas/RequestedQos'

required:

- ruleOp

- packFiltInfo

PacketFilterInfo:

type: object

properties:

packFiltId:

type: string

description: An identifier of packet filter.

packFiltCont:

$ref: '#/components/schemas/PacketFilterContent'

tosTrafficClass:

type: string

description: Contains the Ipv4 Type-of-Service and mask field or the Ipv6 Traffic-Class field and mask field.

spi:

type: string

description: The security parameter index of the IPSec packet.

flowLabel:

type: string

description: The Ipv6 flow label header field.

flowDirection:

$ref: '#/components/schemas/FlowDirection'

RequestedQos:

type: object

properties:

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

gbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

required:

- 5qi

QosNotificationControlInfo:

type: object

properties:

refPccRuleIds:

type: array

items:

type: string

minItems: 1

description: An array of PCC rule id references to the PCC rules associated with the QoS notification control info.

notifType:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/QosNotifType'

contVer:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ContentVersion'

gfbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

gfbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

altQosParamId:

type: string

required:

- refPccRuleIds

- notifType

PartialSuccessReport:

type: object

properties:

failureCause:

$ref: '#/components/schemas/FailureCause'

ruleReports:

type: array

items:

$ref: '#/components/schemas/RuleReport'

minItems: 1

description: Information about the PCC rules provisioned by the PCF not successfully installed/activated.

sessRuleReports:

type: array

items:

$ref: '#/components/schemas/SessionRuleReport'

minItems: 1

description: Information about the session rules provisioned by the PCF not successfully installed.

ueCampingRep:

$ref: '#/components/schemas/UeCampingRep'

required:

- failureCause

AuthorizedDefaultQos:

type: object

properties:

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

arp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

priorityLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevelRm'

averWindow:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindowRm'

maxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MaxDataBurstVolRm'

maxbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

qnc:

type: boolean

description: Indicates whether notifications are requested from 3GPP NG-RAN when the GFBR can no longer (or again) be guaranteed for a QoS Flow during the lifetime of the QoS Flow.

extMaxDataBurstVol:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

ErrorReport:

type: object

properties:

error:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

ruleReports:

type: array

items:

$ref: '#/components/schemas/RuleReport'

minItems: 1

description: Used to report the PCC rule failure.

sessRuleReports:

type: array

items:

$ref: '#/components/schemas/SessionRuleReport'

minItems: 1

description: Used to report the session rule failure.

SessionRuleReport:

type: object

properties:

ruleIds:

type: array

items:

type: string

minItems: 1

description: Contains the identifier of the affected session rule(s).

ruleStatus:

$ref: '#/components/schemas/RuleStatus'

sessRuleFailureCode:

$ref: '#/components/schemas/SessionRuleFailureCode'

required:

- ruleIds

- ruleStatus

ServingNfIdentity:

type: object

properties:

servNfInstId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

guami:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

anGwAddr:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/AnGwAddress'

SteeringMode:

type: object

properties:

steerModeValue:

$ref: '#/components/schemas/SteerModeValue'

active:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

standby:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

3gLoad:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

prioAcc:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

required:

- steerModeValue

QosMonitoringData:

type: object

properties:

qmId:

type: string

description: Univocally identifies the QoS monitoring policy data within a PDU session.

reqQosMonParams:

type: array

items:

$ref: '#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

maxItems: 3

description: indicates the UL packet delay, DL packet delay and/or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for URLLC is enabled for the service data flow..

repFreq:

$ref: '#/components/schemas/ReportingFrequency'

repThreshDl:

type: integer

description: Unsigned integer identifying a period of time in units of miliiseconds for DL packet delay.

repThreshUl:

type: integer

description: Unsigned integer identifying a period of time in units of miliiseconds for UL packet delay.

repThreshRp:

type: integer

description: Unsigned integer identifying a period of time in units of miliiseconds for round trip packet delay.

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

notifyUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifyCorreId:

type: string

required:

- qmId

nullable: true

QosMonitoringReport:

type: object

properties:

refPccRuleIds:

type: array

items:

type: string

minItems: 1

description: An array of PCC rule id references to the PCC rules associated with the QoS monitoring report.

ulDelays:

type: array

items:

type: integer

dlDelays:

type: array

items:

type: integer

rttDelays:

type: array

items:

type: integer

required:

- refPccRuleIds

5GSmCause:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

PacketFilterContent:

type: string

description: Defines a packet filter for an IP flow.Refer to subclause 5.3.54 of 3GPP TS 29.212 for encoding.

FlowDescription:

type: string

description: Defines a packet filter for an IP flow.Refer to subclause 5.4.2 of 3GPP TS 29.212 for encoding.

FlowDirection:

anyOf:

- type: string

enum:

- DOWNLINK

- UPLINK

- BIDIRECTIONAL

- UNSPECIFIED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- DOWNLINK: The corresponding filter applies for traffic to the UE.

- UPLINK: The corresponding filter applies for traffic from the UE.

- BIDIRECTIONAL: The corresponding filter applies for traffic both to and from the UE.

- UNSPECIFIED: The corresponding filter applies for traffic to the UE (downlink), but has no specific direction declared. The service data flow detection shall apply the filter for uplink traffic as if the filter was bidirectional. The PCF shall not use the value UNSPECIFIED in filters created by the network in NW-initiated procedures. The PCF shall only include the value UNSPECIFIED in filters in UE-initiated procedures if the same value is received from the SMF.

FlowDirectionRm:

anyOf:

- type: string

enum:

- DOWNLINK

- UPLINK

- BIDIRECTIONAL

- UNSPECIFIED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- DOWNLINK: The corresponding filter applies for traffic to the UE.

- UPLINK: The corresponding filter applies for traffic from the UE.

- BIDIRECTIONAL: The corresponding filter applies for traffic both to and from the UE.

- UNSPECIFIED: The corresponding filter applies for traffic to the UE (downlink), but has no specific direction declared. The service data flow detection shall apply the filter for uplink traffic as if the filter was bidirectional. The PCF shall not use the value UNSPECIFIED in filters created by the network in NW-initiated procedures. The PCF shall only include the value UNSPECIFIED in filters in UE-initiated procedures if the same value is received from the SMF.

nullable: true

ReportingLevel:

anyOf:

- type: string

enum:

- SER\_ID\_LEVEL

- RAT\_GR\_LEVEL

- SPON\_CON\_LEVEL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SER\_ID\_LEVEL: Indicates that the usage shall be reported on service id and rating group combination level.

- RAT\_GR\_LEVEL: Indicates that the usage shall be reported on rating group level.

- SPON\_CON\_LEVEL: Indicates that the usage shall be reported on sponsor identity and rating group combination level.

nullable: true

MeteringMethod:

anyOf:

- type: string

enum:

- DURATION

- VOLUME

- DURATION\_VOLUME

- EVENT

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- DURATION: Indicates that the duration of the service data flow traffic shall be metered.

- VOLUME: Indicates that volume of the service data flow traffic shall be metered.

- DURATION\_VOLUME: Indicates that the duration and the volume of the service data flow traffic shall be metered.

- EVENT: Indicates that events of the service data flow traffic shall be metered.

nullable: true

PolicyControlRequestTrigger:

anyOf:

- type: string

enum:

- PLMN\_CH

- RES\_MO\_RE

- AC\_TY\_CH

- UE\_IP\_CH

- UE\_MAC\_CH

- AN\_CH\_COR

- US\_RE

- APP\_STA

- APP\_STO

- AN\_INFO

- CM\_SES\_FAIL

- PS\_DA\_OFF

- DEF\_QOS\_CH

- SE\_AMBR\_CH

- QOS\_NOTIF

- NO\_CREDIT

- PRA\_CH

- SAREA\_CH

- SCNN\_CH

- RE\_TIMEOUT

- RES\_RELEASE

- SUCC\_RES\_ALLO

- RAT\_TY\_CH

- REF\_QOS\_IND\_CH

- NUM\_OF\_PACKET\_FILTER

- UE\_STATUS\_RESUME

- UE\_TZ\_CH

- AUTH\_PROF\_CH

- QOS\_MONITORING

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- PLMN\_CH: PLMN Change

- RES\_MO\_RE: A request for resource modification has been received by the SMF. The SMF always reports to the PCF.

- AC\_TY\_CH: Access Type Change

- UE\_IP\_CH: UE IP address change. The SMF always reports to the PCF.

- UE\_MAC\_CH: A new UE MAC address is detected or a used UE MAC address is inactive for a specific period

- AN\_CH\_COR: Access Network Charging Correlation Information

- US\_RE: The PDU Session or the Monitoring key specific resources consumed by a UE either reached the threshold or needs to be reported for other reasons.

- APP\_STA: The start of application traffic has been detected.

- APP\_STO: The stop of application traffic has been detected.

- AN\_INFO: Access Network Information report

- CM\_SES\_FAIL: Credit management session failure

- PS\_DA\_OFF: The SMF reports when the 3GPP PS Data Off status changes. The SMF always reports to the PCF.

- DEF\_QOS\_CH: Default QoS Change. The SMF always reports to the PCF.

- SE\_AMBR\_CH: Session AMBR Change. The SMF always reports to the PCF.

- QOS\_NOTIF: The SMF notify the PCF when receiving notification from RAN that QoS targets of the QoS Flow cannot be guranteed or gurateed again.

- NO\_CREDIT: Out of credit

- PRA\_CH: Change of UE presence in Presence Reporting Area

- SAREA\_CH: Location Change with respect to the Serving Area

- SCNN\_CH: Location Change with respect to the Serving CN node

- RE\_TIMEOUT: Indicates the SMF generated the request because there has been a PCC revalidation timeout

- RES\_RELEASE: Indicate that the SMF can inform the PCF of the outcome of the release of resources for those rules that require so.

- SUCC\_RES\_ALLO: Indicates that the requested rule data is the successful resource allocation.

- RAT\_TY\_CH: RAT Type Change.

- REF\_QOS\_IND\_CH: Reflective QoS indication Change

- NUM\_OF\_PACKET\_FILTER: Indicates that the SMF shall report the number of supported packet filter for signalled QoS rules

- UE\_STATUS\_RESUME: Indicates that the UE’s status is resumed.

- UE\_TZ\_CH: UE Time Zone Change

- AUTH\_PROF\_CH: The DN-AAA authorization profile index has changed

- QOS\_MONITORING: Indicate that the SMF notifies the PCF of the QoS Monitoring information.

RequestedRuleDataType:

anyOf:

- type: string

enum:

- CH\_ID

- MS\_TIME\_ZONE

- USER\_LOC\_INFO

- RES\_RELEASE

- SUCC\_RES\_ALLO

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CH\_ID: Indicates that the requested rule data is the charging identifier.

- MS\_TIME\_ZONE: Indicates that the requested access network info type is the UE's timezone.

- USER\_LOC\_INFO: Indicates that the requested access network info type is the UE's location.

- RES\_RELEASE: Indicates that the requested rule data is the result of the release of resource.

- SUCC\_RES\_ALLO: Indicates that the requested rule data is the successful resource allocation.

RuleStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- ACTIVE: Indicates that the PCC rule(s) are successfully installed (for those provisioned from PCF) or activated (for those pre-defined in SMF), or the session rule(s) are successfully installed

- INACTIVE: Indicates that the PCC rule(s) are removed (for those provisioned from PCF) or inactive (for those pre-defined in SMF) or the session rule(s) are removed.

FailureCode:

anyOf:

- type: string

enum:

- UNK\_RULE\_ID

- RA\_GR\_ERR

- SER\_ID\_ERR

- NF\_MAL

- RES\_LIM

- MAX\_NR\_QoS\_FLOW

- MISS\_FLOW\_INFO

- RES\_ALLO\_FAIL

- UNSUCC\_QOS\_VAL

- INCOR\_FLOW\_INFO

- PS\_TO\_CS\_HAN

- APP\_ID\_ERR

- NO\_QOS\_FLOW\_BOUND

- FILTER\_RES

- MISS\_REDI\_SER\_ADDR

- CM\_END\_USER\_SER\_DENIED

- CM\_CREDIT\_CON\_NOT\_APP

- CM\_AUTH\_REJ

- CM\_USER\_UNK

- CM\_RAT\_FAILED

- UE\_STA\_SUSP

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UNK\_RULE\_ID: Indicates that the pre-provisioned PCC rule could not be successfully activated because the PCC rule identifier is unknown to the SMF.

- RA\_GR\_ERR: Indicate that the PCC rule could not be successfully installed or enforced because the Rating Group specified within the Charging Data policy decision which the PCC rule refers to is unknown or, invalid.

- SER\_ID\_ERR: Indicate that the PCC rule could not be successfully installed or enforced because the Service Identifier specified within the Charging Data policy decision which the PCC rule refers to is invalid, unknown, or not applicable to the service being charged.

- NF\_MAL: Indicate that the PCC rule could not be successfully installed (for those provisioned from the PCF) or activated (for those pre-defined in SMF) or enforced (for those already successfully installed) due to SMF/UPF malfunction.

- RES\_LIM: Indicate that the PCC rule could not be successfully installed (for those provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those already successfully installed) due to a limitation of resources at the SMF/UPF.

- MAX\_NR\_QoS\_FLOW: Indicate that the PCC rule could not be successfully installed (for those provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those already successfully installed) due to the fact that the maximum number of QoS flows has been reached for the PDU session.

- MISS\_FLOW\_INFO: Indicate that the PCC rule could not be successfully installed or enforced because neither the "flowInfos" attribute nor the "appId" attribute is specified within the PccRule data structure by the PCF during the first install request of the PCC rule.

- RES\_ALLO\_FAIL: Indicate that the PCC rule could not be successfully installed or maintained since the QoS flow establishment/modification failed, or the QoS flow was released.

- UNSUCC\_QOS\_VAL: indicate that the QoS validation has failed or when Guaranteed Bandwidth > Max-Requested-Bandwidth.

- INCOR\_FLOW\_INFO: Indicate that the PCC rule could not be successfully installed or modified at the SMF because the provided flow information is not supported by the network (e.g. the provided IP address(es) or Ipv6 prefix(es) do not correspond to an IP version applicable for the PDU session).

- PS\_TO\_CS\_HAN: Indicate that the PCC rule could not be maintained because of PS to CS handover.

- APP\_ID\_ERR: Indicate that the rule could not be successfully installed or enforced because the Application Identifier is invalid, unknown, or not applicable to the application required for detection.

- NO\_QOS\_FLOW\_BOUND: Indicate that there is no QoS flow which the SMF can bind the PCC rule(s) to.

- FILTER\_RES: Indicate that the Flow Information within the "flowInfos" attribute cannot be handled by the SMF because any of the restrictions defined in subclause 5.4.2 of 3GPP TS 29.212 was not met.

- MISS\_REDI\_SER\_ADDR: Indicate that the PCC rule could not be successfully installed or enforced at the SMF because there is no valid Redirect Server Address within the Traffic Control Data policy decision which the PCC rule refers to provided by the PCF and no preconfigured redirection address for this PCC rule at the SMF.

- CM\_END\_USER\_SER\_DENIED: Indicate that the charging system denied the service request due to service restrictions (e.g. terminate rating group) or limitations related to the end-user, for example the end-user's account could not cover the requested service.

- CM\_CREDIT\_CON\_NOT\_APP: Indicate that the charging system determined that the service can be granted to the end user but no further credit control is needed for the service (e.g. service is free of charge or is treated for offline charging).

- CM\_AUTH\_REJ: Indicate that the charging system denied the service request in order to terminate the service for which credit is requested.

- CM\_USER\_UNK: Indicate that the specified end user could not be found in the charging system.

- CM\_RAT\_FAILED: Indicate that the charging system cannot rate the service request due to insufficient rating input, incorrect AVP combination or due to an attribute or an attribute value that is not recognized or supported in the rating.

- UE\_STA\_SUSP: Indicates that the UE is in suspend state.

AfSigProtocol:

anyOf:

- type: string

enum:

- NO\_INFORMATION

- SIP

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NO\_INFORMATION: Indicate that no information about the AF signalling protocol is being provided.

- SIP: Indicate that the signalling protocol is Session Initiation Protocol.

nullable: true

RuleOperation:

anyOf:

- type: string

enum:

- CREATE\_PCC\_RULE

- DELETE\_PCC\_RULE

- MODIFY\_PCC\_RULE\_AND\_ADD\_PACKET\_FILTERS

- MODIFY\_ PCC\_RULE\_AND\_REPLACE\_PACKET\_FILTERS

- MODIFY\_ PCC\_RULE\_AND\_DELETE\_PACKET\_FILTERS

- MODIFY\_PCC\_RULE\_WITHOUT\_MODIFY\_PACKET\_FILTERS

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CREATE\_PCC\_RULE: Indicates to create a new PCC rule to reserve the resource requested by the UE.

- DELETE\_PCC\_RULE: Indicates to delete a PCC rule corresponding to reserve the resource requested by the UE..

- MODIFY\_PCC\_RULE\_AND\_ADD\_PACKET\_FILTERS: Indicates to modify the PCC rule by adding new packet filter(s).

- MODIFY\_ PCC\_RULE\_AND\_REPLACE\_PACKET\_FILTERS: Indicates to modify the PCC rule by replacing the existing packet filter(s).

- MODIFY\_ PCC\_RULE\_AND\_DELETE\_PACKET\_FILTERS: Indicates to modify the PCC rule by deleting the existing packet filter(s).

- MODIFY\_PCC\_RULE\_WITHOUT\_MODIFY\_PACKET\_FILTERS: Indicates to modify the PCC rule by modifying the QoS of the PCC rule.

RedirectAddressType:

anyOf:

- type: string

enum:

- IPV4\_ADDR

- IPV6\_ADDR

- URL

- SIP\_URI

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- IPV4\_ADDR: Indicates that the address type is in the form of "dotted-decimal" IPv4 address.

- IPV6\_ADDR: Indicates that the address type is in the form of IPv6 address.

- URL: Indicates that the address type is in the form of Uniform Resource Locator.

- SIP\_URI: Indicates that the address type is in the form of SIP Uniform Resource Identifier.

QosFlowUsage:

anyOf:

- type: string

enum:

- GENERAL

- IMS\_SIG

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- GENERAL: Indicate no specific QoS flow usage information is available.

- IMS\_SIG: Indicate that the QoS flow is used for IMS signalling only.

FailureCause:

anyOf:

- type: string

enum:

- PCC\_RULE\_EVENT

- PCC\_QOS\_FLOW\_EVENT

- RULE\_PERMANENT\_ERROR

- RULE\_TEMPORARY\_ERROR

- type: string

CreditManagementStatus:

anyOf:

- type: string

enum:

- END\_USER\_SER\_DENIED

- CREDIT\_CTRL\_NOT\_APP

- AUTH\_REJECTED

- USER\_UNKNOWN

- RATING\_FAILED

- type: string

SessionRuleFailureCode:

anyOf:

- type: string

enum:

- NF\_MAL

- RES\_LIM

- UNSUCC\_QOS\_VAL

- UE\_STA\_SUSP

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NF\_MAL: Indicate that the PCC rule could not be successfully installed (for those provisioned from the PCF) or activated (for those pre-defined in SMF) or enforced (for those already successfully installed) due to SMF/UPF malfunction.

- RES\_LIM: Indicate that the PCC rule could not be successfully installed (for those provisioned from PCF) or activated (for those pre-defined in SMF) or enforced (for those already successfully installed) due to a limitation of resources at the SMF/UPF.

- UNSUCC\_QOS\_VAL: indicate that the QoS validation has failed.

- UE\_STA\_SUSP: Indicates that the UE is in suspend state.

SteeringFunctionality:

anyOf:

- type: string

enum:

- MPTCP

- ATSSS\_LL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- MPTCP: Indicates that PCF authorizes the MPTCP functionality to support traffic steering, switching and splitting.

- ATSSS\_LL: Indicates that PCF authorizes the ATSSS-LL functionality to support traffic steering, switching and splitting.

SteerModeValue:

anyOf:

- type: string

enum:

- ACTIVE\_STANDBY

- LOAD\_BALANCING

- SMALLEST\_DELAY

- PRIORITY\_BASED

- type: string

MulticastAccessControl:

anyOf:

- type: string

enum:

- ALLOWED

- NOT\_ALLOWED

- type: string

RequestedQosMonitoringParameter:

anyOf:

- type: string

enum:

- DOWNLINK

- UPLINK

- ROUND\_TRIP

- type: string

ReportingFrequency:

anyOf:

- type: string

enum:

- EVENT\_TRIGGERED

- PERIODIC

- SESSION\_RELEASE

- EVENT\_TRIGGERED\_AND\_SESSION\_RELEASE

- PERIODIC\_AND\_SESSION\_RELEASE

- type: string

SmPolicyAssociationReleaseCause:

anyOf:

- type: string

enum:

- UNSPECIFIED

- UE\_SUBSCRIPTION

- INSUFFICIENT\_RES

- VALIDATION\_CONDITION\_NOT\_MET

- type: string

PduSessionRelCause:

anyOf:

- type: string

enum:

- PS\_TO\_CS\_HO

- type: string

#

\*\*\* End of Changes \*\*\*