**TSG-CT WG3 Meeting #108-e *C3-201336***

**E-Meeting, 19th – 28th February 2020 (Revision of C3-201136)**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **0127** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification of IPTV configuration |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | 5WWC |  | ***Date:*** | 2020-02-17 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | According to TS 23.316, subclause 7.7.1.1.4 and subclause 8.5.2, application Id is mandatory to be provided during Nnef\_IPTV\_Configuratiuon create service procedure. In addition, DNN and/or S-NSSAI are optional. |
|  |  |
| ***Summary of change:*** | Make application Id mandatory and DNN and/or S-NSSAI optional in IptvConfigData. |
|  |  |
| ***Consequences if not approved:*** | Incorrect data type definition for IPTV configuration. |
|  |  |
| ***Clauses affected:*** | 4.4.18; 5.9.2.3.2; A.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible feature into OpenAPI file for IPTVConfiguration API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

### 4.4.18 Procedures for IPTV Configuration

The procedures are used by the AF to authorize the request and forward the request for IPTV configuration information via NEF.

In order to configure IPTV information, the AF shall send an HTTP POST message to the NEF to the resource "IPTV Configurations", the HTTP POST message shall include IptvConfigData data structure as request body. The IptvConfigData data structure shall include:

- indication of the UEs to which the subscription applies via:

a) identification of an individual UE via a "gpsi" attribute; or

b) identification of a group of UE(s) via a "exterGroupId" attribute;

- an application identifier as "appId" attribute; and

- a list of Multicast Access Control as "multiAccCtrls" attribute;

and may include:

- an DNN as "dnn" attribute;

- an S-NSSAI as "snssai" attribute.

In order to update an existing analytics exposure subscription, the AF shall send an HTTP PUT or HTTP PATCH message to the NEF to the resource "Individual IPTV Configuration" requesting to change the subscription.

In order to delete an existing analytics exposure subscription, the AF shall send an HTTP DELETE message to the NEF to the resource "Individual IPTV Configuration".

Upon receipt of the HTTP request from the AF, if the AF is authorized, the NEF shall interact with the UDM by invoking the Nudm\_SubscriberDataManagement service as described in 3GPP TS 29.503 [17] to retrieve the SUPI or Internal Group Identifier. Then the NEF shall interact with the UDR to create, update or delete the IPTV configuration by using the Nudr\_DataRepository service as defined in 3GPP TS 29.519 [23]. If the NEF receives an error code from the UDR, the NEF shall not create, update or delete the resource and shall respond to the AF with a status code set to 500 Internal Server Error.

After receiving a successful response from the UDR, the NEF shall,

- for the HTTP POST request, create a resource "Individual IPTV Configuration" which represents the IPTV configuration request, addressed by a URI that contains the AF Identifier and an NEF-created configuration identifier, and shall respond to the AF with a 201 Created status code, including a Location header field containing the URI for the created resource. The AF shall use the URI received in the Location header in subsequent requests to the NEF to refer to this IPTV configuration.

- for the HTTP PUT or HTTP PATCH request, update a resource "Individual IPTV Configuration" which represents the IPTV configuration, and shall responds to the AF with a 200 OK or 204 No Content status code.

- for the HTTP DELETE request, remove all properties of the resource and delete the corresponding active resource "Individual IPTV Configuration", then shall responds to the AF with a 204 No Content status code.

\*\*\* Next Change \*\*\*

##### 5.9.2.3.2 Type: IptvConfigData

Table 5.9.2.3.2-1: Definition of type IptvConfigData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| self | Link | C | 0..1 | Identifies the individual IPTV configuration resource URI.Shall be present in the HTTP GET response when reading all the configurations for an AF. |  |
|  |  |  |  |  |  |
| gpsi | Gpsi | C | 0..1 | Identifies GPSI.(NOTE) |  |
| exterGroupId | ExternalGroupId | C | 0..1 | Represents a group of users. (NOTE) |  |
| afAppId | string | M | 1 | Identifies an application. |  |
| dnn | Dnn | O | 0..1 | Identifies a DNN. |  |
| snssai | Snssai | O | 0..1 | Identifies an S-NSSAI. |  |
| multiAccCtrls | map(MulticastAccessControl) | M | 1..N | Identifies a list of multicast address access control information. |  |
| suppFeat | SupportedFeatures | M | 1 | Indicates the negotiated supported features. |  |
| NOTE: Only one of the "gpsi" or "exterGroupId" attribute shall be provided. |

\*\*\* Next Change \*\*\*

# A.7 IPTVConfiguration API

openapi: 3.0.0

info:

 title: 3gpp-iptvconfiguration

 version: 1.0.0.alpha-1

 description: |

 API for IPTV configuration.

 © 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.522 V16.2.0; 5G System; Network Exposure Function Northbound APIs.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/3gpp-iptvconfiguration/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

 /{afId}/configurations:

 get:

 summary: read all of the active configurations for the AF

 tags:

 - AF level GET Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get all of the active configurations for the AF)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/IptvConfigData'

 minItems: 0

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 post:

 summary: Creates a new configuration resource

 tags:

 - Configuration level POST Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 requestBody:

 description: new configuration creation

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 responses:

 '201':

 description: Created (Successful creation of configuration)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '204':

 description: Successful case. The resource has been successfully created and no additional content is to be sent in the response message.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{afId}/configurations/{configurationId}:

 get:

 summary: read an active configuration for the AF and the configuration Id

 tags:

 - Configuration level GET Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get the active configuration)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 summary: Updates/replaces an existing configuration resource

 tags:

 - Configuration level PUT Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 requestBody:

 description: Parameters to update/replace the existing configuration

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 responses:

 '200':

 description: OK (Successful deletion of the existing configuration)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 '204':

 description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Partial updates an existing configuration resource

 tags:

 - Configuration level PATCH Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/IptvConfigDataPatch'

 responses:

 '200':

 description: OK. The configuration was modified successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 '204':

 description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Deletes an already existing configuration

 tags:

 - Configuration level DELETE Operation

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content (Successful deletion of the existing configuration)

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 IptvConfigData:

 type: object

 properties:

 self:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 exterGroupId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

 afAppId:

 type: string

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 multiAccCtrls:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MulticastAccessControl'

 minProperties: 1

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - afTransId

 - afAppId

 - multiAccCtrls

 - supportedFeatures

 IptvConfigDataPatch:

 type: object

 properties:

 multiAccCtrls:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MulticastAccessControl'

 minProperties: 1

 MulticastAccessControl:

 type: object

 properties:

 srcIpv4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 srcIpv6Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 multicastV4Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 multicastV6Addr:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 accStatus:

 $ref: '#/components/schemas/AccessRightStatus'

 required:

 - accStatus

 AccessRightStatus:

 anyOf:

 - type: string

 enum:

 - FULLY\_ALLOWED

 - PREVIEW\_ALLOWED

 - NO\_ALLOWED

 - type: string

 description: >

 Possible values are

 - FULLY\_ALLOWED: The User is fully allowed to access to the channel.

 - PREVIEW\_ALLOWED: The User is preview allowed to access to the channel.

 - NO\_ALLOWED: The User is not allowed to access to the channel.

\*\*\* End of Changes \*\*\*