**3GPP TSG-CT3 Meeting #113e C3-210216r2**

**E-Meeting, 25th – 29th January 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **0263** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | OpenAPI reference |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2021-01-07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The OpenAPI Initiative (OAI) keeps the official specifications of the different OpenAPI versions in the web site:https://www.openapis.organd therefore CT4 agreed to use as reference in the 3GPP Technical Specifications an URL of the organization that defines and maintains the specification, see [C4-205258](https://www.3gpp.org/ftp/tsg_ct/WG4_protocollars_ex-CN4/TSGCT4_101e_meeting/Docs/C4-205258.zip) which updated TS 29.501 and SBI TS template.This specification refers to the OpenAPI specification and needs to be accordingly updated. |
|  |  |
| ***Summary of change:*** | Reference to the OpenAPI specification aligned with TS 29.501 and SBI TS template. |
|  |  |
| ***Consequences if not approved:*** | 3GPP specification would refer to incorrect reference and will not be aligned with SBI TS template. |
|  |  |
| ***Clauses affected:*** | 2, A.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not require a version update of the OpenAPI files. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.502: "Procedures for the 5G system".

[3] 3GPP TS 23.501: "System Architecture for the 5G".

[4] 3GPP TS 29.122: "T8 reference point for northbound Application Programming Interfaces (APIs)".

[5] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[6] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[7] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[8] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[9] 3GPP TS 29.521: "5G System; Binding Support Management Service; Stage 3".

[10] Void.

[11] 3GPP TS 23.222: "Common API Framework for 3GPP Northbound APIs; Stage 2".

[12] 3GPP TS 29.222: "Common API Framework for 3GPP Northbound APIs; Stage 3".

[13] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[14] 3GPP TS 33.122: "Security Aspects of Common API Framework for 3GPP Northbound APIs".

[15] Void.

[16] IETF RFC 5246: "The Transport Layer Security (TLS) Protocol Version 1.2".

[17] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[18] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[19] 3GPP TS 29.554: "5G System; Background Data Transfer Policy Control Service; Stage 3".

[20] 3GPP TS 29.504: "5G System; Unified Data Repository Services; Stage 3".

[21] 3GPP TR 21.900: "Technical Specification Group working methods".

[22] 3GPP TS 29.523: "5G System; Policy Control Event Exposure Service; Stage 3".

[23] 3GPP TS 29.519: "5G System; Usage of the Unified Data Repository service for Policy Control Data, Application Data and Structured Data for Exposure; Stage 3".

[24] 3GPP TS 29.541: "5G System; Network Exposure (NE) function services for Non-IP Data Delivery (NIDD); Stage 3".

[25] 3GPP TS 29.542: "5G System, Session management services for Non-IP Data Delivery (NIDD); Stage 3".

[26] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[27] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[28] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G system (5GS)".

[29] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[30] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[31] 3GPP TS 23.287: "Architecture enhancements for 5G System (5GS) to Vehicle-to-Everything (V2X) services".

[32] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[33] 3GPP TS 24.588: "Vehicle-to-Everything (V2X) services in 5G System (5GS); User Equipment (UE) policies; Stage 3".

[34] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[35] 3GPP TS 29.515: "5G System; Gateway Mobile Location Services; Stage 3".

[36] 3GPP TS 23.273: "5G System Location Services (LCS)".

[37] 3GPP TS 33.535: "Authentication and Key Management for Applications (AKMA) based on 3GPP credentials in the 5G System (5GS)".

[38] 3GPP TS 29.535: "5G System; AKMA Anchor Services".

\*\*\* 2nd Change \*\*\*

# A.1 General

This Annex is based on the OpenAPI Specification [5] and provides corresponding representations of all APIs defined in the present specification.

NOTE 1: An OpenAPIs representation embeds JSON Schema representations of HTTP message bodies.

This Annex shall take precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE 2: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see clause 5B of the 3GPP TR 21.900 [21] and subclause 5.3.1 of the 3GPP TS 29.501 [32] for further information).

\*\*\* End of Changes \*\*\*