**3GPP TSG-CT WG3 Meeting #113e C3-210251**

**E-Meeting, 25th – 29th January 2021 (Revision of C3-20xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.520** | **CR** | **0253** | **rev** | **-** | **Current version:** | **17.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction to S-NSSAI applicability | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNA | | | | |  | ***Date:*** | | | 2021-01-12 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | S-NSSAI subscription is not applicable to all the features, "UeMobility" and "NetworkPerformance" features are not applicable to S-NSSAI aligned both in Stage 2 and this specification. Type EventSubscription and type EventFilter define "ServiceExperience" and "NsiLoad" are applicable for "nsiIdInfos" attribute instead of "snssais" attribute.  Hence the related S-NSSAI subscription applicability need to be corrected in the related tables. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Correct the feature applicability to type "Snssai" and attribute "snssais" in the corresponding clauses. Update descriptions in table for "SLICE\_LOAD\_LEVEL" and "LOAD\_LEVEL\_INFORMATION" event for type "Snssai", attribute "snssais", and type "SliceLoadLevelInformation". Adding descriptions for Snssai and SliceLoadLevelInformation in Table 5.2.6.1-2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not correct scope of S-NSSAI features applicability, misaliagnment with stage 2 and in this specification | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.1.6.1, 5.1.6.2.3, 5.2.6.1, 5.2.6.2.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact the OpenAPI files. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.1.6.1 General

This subclause specifies the application data model supported by the API.

Table 5.1.6.1-1 specifies the data types defined for the Nnwdaf\_EventsSubscription service based interface protocol.

Table 5.1.6.1-1: Nnwdaf\_EventsSubscription specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AdditionalMeasurement | 5.1.6.2.26 |  | AbnormalBehaviour |
| AddressList | 5.4.6.2.28 |  | AbnormalBehaviour |
| Accuracy | 5.1.6.3.5 | Represents the preferred level of accuracy of the analytics. |  |
| AnySlice | 5.1.6.3.2 | Represents the any slices. |  |
| BwRequirement | 5.1.6.2.25 | Represents bandwidth requirement. | ServiceExperience |
| CircumstanceDescription | 5.1.6.2.29 |  | AbnormalBehaviour |
| CongestionInfo | 5.1.6.2.18 |  | UserDataCongestion |
| CongestionType | 5.1.6.3.7 |  | UserDataCongestion |
| EventNotification | 5.1.6.2.5 | Describes Notifications about events that occurred. |  |
| EventReportingRequirement | 5.1.6.2.7 | Represents the type of reporting the subscription requires. |  |
| EventSubscription | 5.1.6.2.3 | Represents the subscription to a single event. |  |
| ExpectedAnalyticsType | 5.1.6.3.11 |  | AbnormalBehaviour |
| IpEthFlowDescription | 5.1.6.2.27 |  | AbnormalBehaviour |
| LoadLevelInformation | 5.1.6.3.2 | Represents load level information of the network slice instance |  |
| LocationInfo | 5.1.6.2.11 |  | UeMobility |
| MatchingDirection | 5.1.6.3.12 | Defines the matching direction when crossing a threshold | NfLoad, QoSSustainability, UserDataCongestion, NetworkPerformance |
| NetworkPerfInfo | 5.1.6.2.23 |  | NetworkPerformance |
| NetworkPerfRequirement | 5.1.6.2.22 |  | NetworkPerformance |
| NetworkPerfType | 5.1.6.3.10 |  | NetworkPerformance |
| NfLoadLevelInformation | 5.1.6.2.31 | Represents load level information of a given NF instance. | NfLoad |
| NfStatus | 5.1.6.2.32 | Provides the percentage of time spent on various NF states | NfLoad |
| NwdafEvent | 5.1.6.3.4 | Describes the NWDAF Events. |  |
| NnwdafEventsSubscription | 5.1.6.2.2 | Represents an Individual NWDAF Event Subscription resource. |  |
| NnwdafEventsSubscriptionNotification | 5.1.6.2.4 | Represents an Individual NWDAF Event Subscription Notification resource. |  |
| NotificationMethod | 5.1.6.3.3 | Represents the notification methods that can be subscribed. |  |
| NsiIdInfo | 5.1.6.2.33 | Represents the S-NSSAI and the optionally associated Network Slice Instance Identifier(s). | ServiceExperience  NsiLoad |
| NsiLoadLevelInfo | 5.1.6.2.34 | Represents the load level information for an S-NSSAI and the optionally associated network slice instance. | NsiLoad |
| QosRequirement | 5.1.6.2.20 |  | QoSSustainability |
| QosSustainabilityInfo | 5.1.6.2.19 | Represents the QoS Sustainability information. | QoSSustainability |
| RetainabilityThreshold | 5.1.6.2.21 |  | QoSSustainability |
| ServiceExperienceInfo | 5.1.6.2.24 | Represents the service experience information. | ServiceExperience |
| SliceLoadLevelInformation | 5.1.6.2.6 | Represents the slices and the load level information. When subscribed event is "SLICE\_LOAD\_LEVEL", the Snssai shall be included. |  |
| TargetUeInformation | 5.1.6.2.8 | Identifies the target UE information. | ServiceExperience  NfLoad  NetworkPerformance  UserDataCongestion  UeMobility  UeCommunication  AbnormalBehaviour  QoSSustainability |
| ThresholdLevel | 5.1.6.2.30 | Describe a threshold level | UserDataCongestion  NfLoad |
| TimeUnit | 5.1.6.3.9 |  | QoSSustainability |
| TrafficCharacterization | 5.1.6.2.14 |  | UeCommunication |
| UeCommunication | 5.1.6.2.13 |  | UeCommunication |
| UeMobility | 5.1.6.2.10 |  | UeMobility |
| UserDataCongestionInfo | 5.1.6.2.17 | Represents the user data congestion information | UserDataCongestion |
| AbnormalBehaviour | 5.1.6.2.15 | Represents the abnormal behaviour information. | AbnormalBehaviour |
| Exception | 5.1.6.2.16 | Describes the Exception information. | AbnormalBehaviour |
| ExceptionId | 5.1.6.3.6 | Describes the Exception Id. | AbnormalBehaviour |
| ExceptionTrend | 5.1.6.3.7 | Describes the Exception Trend. | AbnormalBehaviour |

Table 5.1.6.1-2 specifies data types re-used by the Nnwdaf\_EventsSubscription service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nnwdaf service based interface.

Table 5.1.6.1-2: Nnwdaf\_EventsSubscription re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| 5Qi | 3GPP TS 29.571 [8] | Identifies the 5G QoS identifier | QoSSustainability |
| ApplicationId | 3GPP TS 29.571 [8] | Identifies the application identifier. | ServiceExperience  UeCommunication  AbnormalBehaviour |
| BitRate | 3GPP TS 29.571 [8] | String representing a bit rate that shall be formatted as follows:  pattern: "^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$"  Examples:  "125 Mbps", "0.125 Gbps", "125000 Kbps". | ServiceExperience  QoSSustainability |
| DateTime | 3GPP TS 29.571 [8] | Identifies the time. |  |
| Dnai | 3GPP TS 29.571 [8] | Identifies a user plane access to one or more DN(s). | ServiceExperience |
| Dnn | 3GPP TS 29.571 [8] | Identifies the DNN. | ServiceExperience  AbnormalBehaviour  UeCommunication |
| DurationSec | 3GPP TS 29.571 [8] |  |  |
| EthFlowDescription | 3GPP TS 29.514 [21] |  | UeCommunication  AbnormalBehaviour |
| ExpectedUeBehaviourData | 3GPP TS 29.503 [23] |  | AbnormalBehaviour |
| Float | 3GPP TS 29.571 [8] |  |  |
| FlowDescription | 3GPP TS 29.514 [21] |  | UeCommunication  AbnormalBehaviour |
| GroupId | 3GPP TS 29.571 [8] | Identifies a group of UEs. | UeMobility  UeCommunication  NetworkPerformance  AbnormalBehaviour  ServiceExperience |
| Ipv4Addr | 3GPP TS 29.571 [8] |  |  |
| Ipv6Addr | 3GPP TS 29.571 [8] |  |  |
| NetworkAreaInfo | 3GPP TS 29.554 [18] | Identifies the network area. | ServiceExperience  QoSSustainability  AbnormalBehaviour  UeMobility  UserDataCongestion  NetworkPerformance |
| NfInstanceId | 3GPP TS 29.571 [8] | Identifies an NF instance | NfLoad |
| NfSetId | 3GPP TS 29.571 [8] | Identifies an NF Set instance | NfLoad |
| NFType | 3GPP TS 29.510 [12] | Indentifies a type of NF | NfLoad |
| NsiId | 3GPP TS 29.531 [24] | Identifies a Network Slice Instance | ServiceExperience  NsiLoad |
| PacketDelBudget | 3GPP TS 29.571 [8] |  | QoSSustainability |
| PacketErrRate | 3GPP TS 29.571 [8] |  | QoSSustainability |
| ProblemDetails | 3GPP TS 29.571 [8] | Used in error responses to provide more detailed information about an error. |  |
| QosResourceType | 3GPP TS 29.571 [8] | Identifies the resource type in QoS characteristics. | QoSSustainability |
| ReportingInformation | 3GPP TS 29.523 [20] | Represents the type of reporting the subscription requires. |  |
| SamplingRatio | 3GPP TS 29.571 [8] |  |  |
| ScheduledCommunicationTime | 3GPP TS 29.122 [19] |  | UeMobility UeCommunication |
| Snssai | 3GPP TS 29.571 [8] | Identifies the S-NSSAI (Single Network Slice Selection Assistance Information). When subscribed event is "SLICE\_LOAD\_LEVEL", the Snssai shall be included. | NsiLoad  NfLoad  ServiceExperience  UeCommunication  QoSSustainability  AbnormalBehaviour  UserDataCongestion |
| Supi | 3GPP TS 29.571 [8] | The SUPI for an UE. | ServiceExperience,  NfLoad  NetworkPerformance,  UserDataCongestion  UeMobility  UeCommunication  AbnormalBehaviour |
| SupportedFeatures | 3GPP TS 29.571 [8] | Used to negotiate the applicability of the optional features defined in table 5.1.8-1. |  |
| SvcExperience | 3GPP TS 29.517 [22] |  | ServiceExperience |
| TimeWindow | 3GPP TS 29.122 [19] |  |  |
| Uinteger | 3GPP TS 29.571 [8] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible. |  |
| Uri | 3GPP TS 29.571 [8] |  |  |
| UserLocation | 3GPP TS 29.571 [8] |  | UeMobility |
| Volume | 3GPP TS 29.122 [19] |  | UeCommunication  AbnormalBehaviour |

\*\*\* 2nd Change \*\*\*

##### 5.1.6.2.3 Type EventSubscription

Table 5.1.6.2.3-1: Definition of type EventSubscription

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| anySlice | AnySlice | C | 0..1 | Default is "FALSE". (NOTE 1) |  |
| appIds | array(ApplicationId) | C | 1..N | Identification(s) of application to which the subscription applies.  The absence of appIds means subscription to all applications. (NOTE 8) | ServiceExperience  UeCommunication  AbnormalBehaviour |
| dnns | array(Dnn) | C | 1..N | Identification(s) of DNN to which the subscription applies. Each DNN is a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only.  The absence of dnns means subscription to all DNNs (NOTE 8) | ServiceExperience, AbnormalBehaviour  UeCommunication |
| dnais | array(Dnai) | C | 1..N | Identification(s) of user plane access to DN(s) which the subscription applies. | ServiceExperience |
| event | NwdafEvent | M | 1 | Event that is subscribed. |  |
| extraReportReq | EventReportingRequirement | O | 0..1 | The extra event reporting requirement information. |  |
| loadLevelThreshold | integer | C | 0..1 | Indicates that the NWDAF shall report the corresponding network slice load level to the NF service consumer where the load level of the network slice instance identified by snssais is reached. (NOTE 4)  May be included when subscribed event is "SLICE\_LOAD\_LEVEL". |  |
| matchingDir | MatchingDirection | O | 0..1 | A matching direction may be provided alongside a threshold. If omitted, the default value is CROSSED. | NfLoad, QoSSustainability, UserDataCongestion, NetworkPerformance |
| nfLoadLvlThds | array(ThresholdLevel) | C | 1..N | Shall be supplied in order to start reporting when an average load level is reached.(NOTE 4) | NfLoad |
| networkArea | NetworkAreaInfo | C | 0..1 | Identification of network area to which the subscription applies.  The absence of networkArea means subscription to all network areas. (NOTE 7), (NOTE 8) | ServiceExperience UeMobility  UeCommunication  QoSSustainability  AbnormalBehaviour  UserDataCongestion  NetworkPerformance |
| nfInstanceIds | array(NfInstanceId) | O | 1..N | Identification(s) of NF instances. | NfLoad |
| nfSetIds | array(NfSetId) | O | 1..N | Identification(s) of NF instance sets. | NfLoad |
| nfTypes | array(NFType) | O | 1..N | Identification(s) of NF types. | NfLoad |
| notificationMethod | NotificationMethod | O | 0..1 | Indicate the notification method. (NOTE 2) |  |
| nsiIdInfos | array(NsiIdInfo) | O | 1..N | Each element identifies the S-NSSAI and the optionally associated network slice instance(s).  May be included when subscribed event is "NSI\_LOAD\_LEVEL" or  "SERVICE\_EXPERIENCE".  (NOTE 1) | ServiceExperience  NsiLoad |
| nsiLevelThrds | array(Uinteger) | O | 1..N | Identifies the load threshold for each S-NSSAI or S-NSSAI and the optionally associated network slice instance identified by the "nsiIds" attribute within the "nsiIdInfos" attribute.  (NOTE 4) | NsiLoad |
| qosRequ | QosRequirement | C | 0..1 | Indicates the QoS requirements. It shall be included when subscribed event is "QOS\_SUSTAINABILITY". | QoSSustainability |
| qosFlowRetThds | array(RetainabilityThreshold) | C | 1..N | Represents the QoS flow retainability thresholds.Shall be supplied for the 5QI ("5qi" in "qosRequ") or resource type ("resType" in "qosRequ") of GBR resource type. (NOTE 4) | QoSSustainability |
| ranUeThrouThds | array(BitRate) | C | 1..N | Represents the RAN UE throughput thresholds.  Shall be supplied for the 5QI ("5qi" in "qosRequ") or resource type ("resType" in "qosRequ") of non-GBR resource type.(NOTE 4) | QoSSustainability |
| repetitionPeriod | DurationSec | C | 0..1 | Shall be supplied for notification Method "PERIODIC" by the "notificationMethod" attribute. |  |
| snssais | array(Snssai) | C | 1..N | Identification(s) of network slice to which the subscription applies. When subscribed event is "SLICE\_LOAD\_LEVEL", the snssai shall be included. (NOTE 1), (NOTE 8) | NfLoad  UeCommunication  QoSSustainability  AbnormalBehaviour  UserDataCongestion |
| tgtUe | TargetUeInformation | O | 0..1 | Identifies target UE information | (NOTE 3) |
| congThresholds | array(ThresholdLevel) | C | 1..N | Represents the congestion threshold levels. (NOTE 4) | UserDataCongestion |
| nwPerfRequs | array(NetworkPerfRequirement) | C | 1..N | Represents the network performance requirements. This attribute shall be included when subscribed eventis "NETWORK\_PERFORMANCE". | NetworkPerformance |
| bwRequs | array(BwRequirement) | O | 1..N | Represents the bandwidth requirement for each application. | ServiceExperience |
| excepRequs | array(Exception) | C | 1..N | Represents a list of Exception Ids with associated thresholds. May only be present when subscribed event is "ABNORMAL\_BEHAVIOUR".  (NOTE 5, NOTE 6) | AbnormalBehaviour |
| exptAnaType | ExpectedAnalyticsType | C | 0..1 | Represents expected UE analytics type.  It shall not be present if the "excepRequs" attribute is provided. (NOTE 6) | AbnormalBehaviour |
| exptUeBehav | ExpectedUeBehaviourData | O | 0..1 | Represents expected UE behaviour. | AbnormalBehaviour |
| NOTE 1: When subscribed event is "SLICE\_LOAD\_LEVEL", the identifications of network slices, either information about slice(s) identified by "snssais", or "anySlice" set to "TRUE" shall be included. When subscribed event is "QOS\_SUSTAINABILITY", "NF\_LOAD", "UE\_COMM", "ABNORMAL\_BEHAVIOUR" or "USER\_DATA\_CONGESTION", the identifications of network slices identified by "snssais" is optional. When subscribed event is "NSI\_LOAD\_LEVEL" or "SERVICE\_EXPERIENCE", the "snssais" attribute is not applicable, either the "nsiIdInfos" attribute or "anySlice" set to "TRUE" shall be included.  NOTE 2: When notificationMethod is not supplied, the default value is "THRESHOLD".  NOTE 3: Applicability is further described in the corresponding data type.  NOTE 4: This property shall be provided if the "notifMethod" in "evtReq" is set to "ON\_EVENT\_DETECTION" or "notificationMethod" in "eventSubscriptions" is set to "THRESHOLD" or omitted.  NOTE 5: Only "excepId" and "excepLevel" within the Exception data type apply to the "excepRequs" attribute within EventSubscription data type.  NOTE 6: Either "excepRequs" or "exptAnaType" shall be provided if subscribed event is "ABNORMAL\_BEHAVIOUR".  NOTE 7: For "NETWORK\_PERFORMANCE", "SERVICE\_EXPERIENCE" or "USER\_DATA\_CONGESTION" event, this attribute shall be provided if the event applied for all UEs (i.e. "anyUe" attribute set to true within the "tgtUe" attribute). For "QOS\_SUSTAINABILITY", this attribute shall be provided.  NOTE 8: For "ABNORMAL\_BEHAVIOUR" event with "anyUe" attribute in "tgtUe" attribute sets to true,  - at least one of the "networkArea" and the "snssais" attribute should be included, if the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via the "excepRequs" attribute is mobility related;  - at least one of the "networkArea", "appIds", "dnns" and "snssais" attribute should be included, if the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via the "excepRequs" attribute is communication related;  - the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via "excepRequs" attribute shall not be requested for both mobility and communication related analytics at the same time. | | | | | |

\*\*\* 3rd Change \*\*\*

#### 5.2.6.1 General

This subclause specifies the application data model supported by the API.

Table 5.2.6.1-1 specifies the data types defined for the Nnwdaf\_AnalyticsInfo service based interface protocol.

Table 5.2.6.1-1: Nnwdaf\_AnalyticsInfo specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AnalyticsData | 5.2.6.2.2 | Describes analytics with parameters indicated in the request |  |
| EventFilter | 5.2.6.2.3 | Also missing in release 15. |  |
| EventId | 5.2.6.3.3 | Describes the type of analytics. |  |

Table 5.2.6.1-2 specifies data types re-used by the Nnwdaf\_AnalyticsInfo service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nnwdaf service based interface.

Table 5.2.6.1-2: Nnwdaf\_AnalyticsInfo re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AnySlice | 5.1.6.3.2 |  |  |
| ApplicationId | 3GPP TS 29.571 [8] | Identifies the application. | ServiceExperience  UeCommunication  AbnormalBehaviour |
| BwRequirement | 5.1.6.2.25 |  | ServiceExperience |
| DateTime | 3GPP TS 29.571 [8] | Identifies the time. |  |
| Dnn | 3GPP TS 29.571 [8] | Identifies the DNN. | ServiceExperience  AbnormalBehaviour  UeCommunication |
| Dnai | 3GPP TS 29.571 [8] | Identifies a user plane access to one or more DN(s) | ServiceExperience |
| EventReportingRequirement | 5.1.6.2.7 |  |  |
| ExceptionId | 5.1.6.3.6 |  | AbnormalBehaviour |
| ExpectedUeBehaviourData | 3GPP TS 29.503 [23] |  | AbnormalBehaviour |
| ExpectedAnalyticsType | 5.1.6.3.11 |  | AbnormalBehaviour |
| GroupId | 3GPP TS 29.571 [8] | Internal Group Identifier of a group of UEs | UeMobility  UeCommunication  NetworkPerformance  AbnormalBehaviour  ServiceExperience |
| NetworkAreaInfo | 3GPP TS 29.554 [18] | The network area information. | UeMobility  NetworkPerformance  QoSSustainability  ServiceExperience  UserDataCongestion  AbnormalBehaviour |
| NetworkPerfInfo | 5.1.6.2.23 |  | NetworkPerformance |
| NetworkPerfType | 5.1.6.3.10 | Represents the network performance types. | NetworkPerformance |
| NfLoadLevelInformation | 5.1.6.2.31 | Represents load level information of a given NF instance. | NfLoad |
| NfInstanceId | 3GPP TS 29.571 [8] | Identifies an NF instance | NfLoad |
| NfSetId | 3GPP TS 29.571 [8] | Identifies an NF Set instance | NfLoad |
| NFType | 3GPP TS 29.510 [12] | Indentifies a type of NF | NfLoad |
| NsiId | 3GPP TS 29.531 [24] | Identifies a Network Slice Instance | ServiceExperience  NsiLoad |
| NsiIdInfo | 5.1.6.2.33 | Identify the S-NSSAI and the associated Network Slice Instance(s). | ServiceExperience  NsiLoad |
| NsiLoadLevelInfo | 5.1.6.2.34 | Represents the load level information for an S-NSSAI and the associated network slice instance. | NsiLoad |
| ProblemDetails | 3GPP TS 29.571 [8] | Used in error responses to provide more detailed information about an error. |  |
| QosRequirement | 5.1.6.2.20 |  | QoSSustainability |
| QosSustainabilityInfo | 5.1.6.2.19 |  | QoSSustainability |
| SamplingRatio | 3GPP TS 29.571 [8] |  |  |
| ServiceExperienceInfo | 5.1.6.2.24 |  | ServiceExperience |
| Supi | 3GPP TS 29.571 [8] | Identifies the UE. | ServiceExperience,  NfLoad  NetworkPerformance  UserDataCongestion  UeMobility  UeCommunication  AbnormalBehaviour |
| SupportedFeatures | 3GPP TS 29.571 [8] | Used to negotiate the applicability of the optional features defined in table 5.2.8-1. |  |
| Snssai | 3GPP TS 29.571 [8] | Identifies the S-NSSAI (Single Network Slice Selection Assistance Information). Shall be present when the requested event is "LOAD\_LEVEL\_INFORMATION". | NsiLoad  NfLoad  ServiceExperience  UeCommunication  QoSSustainability  AbnormalBehaviour  UserDataCongestion |
| SliceLoadLevelInformation | 5.1.6.2.6 | The slices and the load level information.  Shall be present when the requested event is "LOAD\_LEVEL\_INFORMATION". |  |
| TargetUeInformation | 5.1.6.2.8 | Identifies the target UE information. | ServiceExperience  NfLoad  NetworkPerformance  UserDataCongestion  UeMobility  UeCommunication  AbnormalBehaviour  QoSSustainability |
| UeCommunication | 5.1.6.2.13 |  | UeCommunication |
| UeMobility | 5.1.6.2.10 |  | UeMobility |
| Uinteger | 3GPP TS 29.571 [8] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible. |  |
| UserDataCongestionInfo | 5.1.6.2.17 |  | UserDataCongestion |
| AbnormalBehaviour | 5.1.6.2.15 | Represents the abnormal behaviour information. | AbnormalBehaviour |

\*\*\* 4th Change \*\*\*

##### 5.2.6.2.3 Type EventFilter

Table 5.2.6.2.3-1: Definition of type EventFilter

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| anySlice | AnySlice | C | 0..1 | Default is "FALSE". (NOTE 1) |  |
| appIds | array(ApplicationId) | C | 1..N | Identification(s) of application. The absence of appIds means applicable to all applications. (NOTE 4) | ServiceExperience  UeCommunication AbnormalBehaviour |
| dnns | array(Dnn) | C | 1..N | Identification(s) of DNN. Each DNN is a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. The absence of dnns means applicable to all DNNs. (NOTE 4) | ServiceExperience  UeCommunication  AbnormalBehaviour |
| dnais | array(Dnai) | C | 1..N | Identification(s) of user plane accesses to DN(s) which the subscription applies. It may be included when event-id is "SERVICE\_EXPERIENCE". | ServiceExperience |
| snssais | array(Snssai) | C | 1..N | Identification(s) of network slice to which the subscription belongs. Shall be present when the requested event is "LOAD\_LEVEL\_INFORMATION". (NOTE 1), (NOTE 4) | NfLoad  UeCommunication  QoSSustainability  AbnormalBehaviour  UserDataCongestion |
| nfInstanceIds | array(NfInstanceId) | O | 1..N | Identification(s) of NF instances. | NfLoad |
| nfSetIds | array(NfSetId) | O | 1..N | Identification(s) of NF instance sets. | NfLoad |
| nfTypes | array(NFType) | O | 1..N | Identification(s) of NF types. | NfLoad |
| networkArea | NetworkAreaInfo | C | 0..1 | This IE represents the network area where the NF service consumer wants to know the analytics result. (NOTE 2), (NOTE 4) | UeMobility  UeCommunication  NetworkPerformance  QoSSustainability  ServiceExperience  UserDataCongestion  AbnormalBehaviour |
| nsiIdInfos | array(NsiIdInfo) | O | 1..N | Each element identifies the S-NSSAI and the optionally associated network slice instance(s).  May be included when subscribed event is "NSI\_LOAD\_LEVEL" or  "SERVICE\_EXPERIENCE".  (NOTE 1) | ServiceExperience  NsiLoad |
| nwPerfTypes | array(NetworkPerfType) | C | 1..N | Represents the network performance types. This attribute shall be included when event-id is "NETWORK\_PERFORMANCE". | NetworkPerformance |
| qosRequ | QoSRequirement | C | 0..1 | Represents the QoS requirements. This attribute shall be included when event-id is "QOS\_SUSTAINABILITY". | QoSSustainability |
| bwRequs | array(BwRequirement) | O | 1..N | Represents the media/application bandwidth requirement for each application.  It may only be present if "appIds" attribute is provided. | ServiceExperience |
| excepIds | array(ExceptionId) | C | 1..N | Represents a list of Exception Ids.  (NOTE 3) | AbnormalBehaviour |
| exptAnaType | ExpectedAnalyticsType | C | 0..1 | Represents expected UE analytics type.  (NOTE 3) | AbnormalBehaviour |
| exptUeBehav | ExpectedUeBehaviourData | O | 0..1 | Represents expected UE behaviour. | AbnormalBehaviour |
| NOTE 1: When event-id in the request is "LOAD\_LEVEL\_INFORMATION", the identifications of network slices, either information about slice(s) identified by the "snssais" attribute, or "anySlice" set to "TRUE", shall be included. When subscribed event is "NSI\_LOAD\_LEVEL" or "SERVICE\_EXPERIENCE", the "snssais" attribute is not applicable, either the "nsiIdInfos" attribute or anySlice set to "TRUE" shall be included. When subscribed event is "QOS\_SUSTAINABILITY", "NF\_LOAD", "UE\_COMM", "ABNORMAL\_BEHAVIOUR" or "USER\_DATA\_CONGESTION", the identifications of network slices identified by the "snssais" attribute is optional.  NOTE 2: For "NETWORK\_PERFORMANCE", "SERVICE\_EXPERIENCE" or "USER\_DATA\_CONGESTION" event, this attribute shall be provided if the event applied for all UEs (i.e. "anyUe" attribute set to true). For "QOS\_SUSTAINABILITY", this attribute shall be provided.  NOTE 3: Either "excepIds" or "exptAnaType" shall be provided if event-id in the request is "ABNORMAL\_BEHAVIOUR".  NOTE 4: For "ABNORMAL\_BEHAVIOUR" event with "anyUe" attribute in "tgt-ue" attribute sets to true,  - at least one of the "networkArea" and the "snssais" attribute should be included, if the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via the "excepIds" attribute is mobility related;  - at least one of the "networkArea", "appIds", "dnns" and "snssais" attribute should be included, if the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via the "excepIds" attribute is communication related;  - the expected analytics type via the"exptAnaType" attribute or the list of Exception Ids via "excepIds" attribute shall not be requested for both mobility and communication related analytics at the same time. | | | | | |

\*\*\* End of Changes \*\*\*