**3GPP TSG-CT WG3 Meeting #116e C3-213226**

**E-Meeting, 19th – 28th May 2021 (Revision of C3-212485)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0348** | **rev** | **4** | **Current version:** | **17.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update DNN and S-NSSAI in AsSessionWithQoS API | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17, 5GS\_Ph1-CT, Vertical\_LAN | | | | |  | ***Date:*** | | | 2021-05-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | For Ethernet type PDU Session extending to support TSN and 5G LAN, current AsSessionWithQoS API provide only UE MAC address and ethernet flow info, these two attributes are not enough for NEF to discover the serving BSF to find the serving PCF in a dynamic way similar as the one for IP PDU session, since NEF is not able to find the right BSF via NRF by using UE MAC address which is not defined and not effective to be managed like IP Address in NF Registration and Discovery.  Meanwhile TrafficInfluence API already include DNN and S-NSSAI information, in which we can consider for NEF to also add DNN and S-NSSAI of the Ethernet type PDU Session in N33 interface to solve the issue.  TS 23.502 CR 2491 was agreed to introduce DNN and S-NSSAI for AsSessionWithQoS API, with the applicablility not limited to Ethernet PDU Session type.. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add DNN and S-NSSAI in data type AsSessionWithQoSSubscription in AsSessionWithQoS API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | For Ethernet type PDU Session, NEF can not dynamically discovery the corresponding servering BSF for the serving PCF with the AF request information, can not completely support the related application session QoS handling for the Ethernet PDU Session. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.14.2.1.1, 5.14.2.1.2, A.14 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 23.502 CR 2491 | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible feature into the OpenAPI file applicable to AsSessionWithQoS API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Updates in CT3#116e for Rev.4: remove the EthAsSessionQoS\_5G feature upon stage 2 DNN and S-NSSAI applicability not limited to Ethernet PDU Session. | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.14.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Table 5.14.2.1.1-1 specifies data types re-used by the AsSessionWithQoS API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the AsSessionWithQoS API.

Table 5.14.2.1.1-1: AsSessionWithQoS API re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |
| EthFlowDescription | 3GPP TS 29.514 [52] | Defines a packet filter for an Ethernet flow.(NOTE 1) |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. |
| ReportingFrequency | 3GPP TS 29.512 [8] | Indicates the frequency for the reporting, such as event triggered, periodic, when the PDU Session is released, and/or any combination. (NOTE 2) |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicate the UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for URLLC is enabled for the service data flow. (NOTE 2) |
| Snssai | 3GPP TS 29.571 [45] | Identifies the S-NSSAI. |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.14.4-1. |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange\_5G as specified in clause 5.14.4 shall be supported.  NOTE 2: In order to support QoS Monitoring, feature QoSMonitoring\_5G as specified in clause 5.14.4 shall be supported. | | |

\*\*\* 2nd Change \*\*\*

##### 5.14.2.1.2 Type: AsSessionWithQoSSubscription

This type represents an AS session request with specific QoS for the service provided by the SCS/AS to the SCEF via T8 interface. The structure is used for subscription request and response.

Table 5.14.2.1.2-1: Definition of type AsSessionWithQoSSubscription

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE 1) |
| self | Link | 0..1 | Link to the resource "Individual AS Session with Required QoS Subscription".  This parameter shall be supplied by the SCEF in HTTP responses. |  |
| supportedFeatures | SupportedFeatures | 0..1 | Used to negotiate the supported optional features of the API as described in subclause 5.2.7.  This attribute shall be provided in the POST request and in the response of successful resource creation. |  |
| dnn | Dnn | 0..1 | Identifies a DNN, a full DNN with both the Network Identifier and Operator Identifier, or a DNN with the Network Identifier only. (NOTE n) |  |
| snssai | Snssai | 0..1 | Identifies an S-NSSAI. (NOTE n) |  |
| notificationDestination | Link | 1 | Contains the URL to receive the notification bearer level event(s) from the SCEF. |  |
| flowInfo | array(FlowInfo) | 0..N | Describe the IP data flow which requires QoS.  (NOTE 2) |  |
| ethFlowInfo | array(EthFlowDescription) | 0..N | Identifies Ethernet packet flows.  (NOTE 2) | EthAsSessionQoS\_5G |
| qosReference | string | 0..1 | Identifies a pre-defined QoS information |  |
| altQoSReferences | array(string) | 0..N | Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority. | AlternativeQoS\_5G |
| ueIpv4Addr | Ipv4Addr | 0..1 | The Ipv4 address of the UE.  (NOTE 2) |  |
| ipDomain | string | 0..1 | The Ipv4 address domain identifier.  The attribute may only be provided if the ueIpv4Addr attribute is present. |  |
| ueIpv6Addr | Ipv6Addr | 0..1 | The Ipv6 address of the UE.  (NOTE 2) |  |
| macAddr | MacAddr48 | 0..1 | Identifies the MAC address.  (NOTE 2) | EthAsSessionQoS\_5G |
| usageThreshold | UsageThreshold | 0..1 | Time period and/or traffic volume in which the QoS is to be applied. |  |
| sponsorInfo | SponsorInformation | 0..1 | Indicates a sponsor information |  |
| qosMonInfo | QosMonitoringInformation | 0..1 | Qos Monitoring information. It can be present when the event "QOS\_MONITORING" is subscribed. | QoSMonitoring\_5G |
| requestTestNotification | boolean | 0..1 | Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise. | Notification\_test\_event |
| websockNotifConfig | WebsockNotifConfig | 0..1 | Configuration parameters to set up notification delivery over Websocket protocol as defined in subclause 5.2.5.4. | Notification\_websocket |
| NOTE 1: Properties marked with a feature as defined in subclause 5.14.4 are applicable as described in subclause 5.2.7. If no features are indicated, the related property applies for all the features.  NOTE 2: One of "ueIpv4Addr", "ueIpv6Addr" or "macAddr" shall be included. If ipv4 or ipv6 address is provided, IP flow information shall be provided. If MAC address is provided, Ethernet flow information shall be provided.  NOTE n: The property is only applicable for the NEF. | | | | |

\*\*\* 3rd Change \*\*\*

## A.14 AsSessionWithQoS API

openapi: 3.0.0

info:

title: 3gpp-as-session-with-qos

version: 1.1.3

description: |

API for setting us an AS session with required QoS.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V16.9.0 T8 reference point for Northbound APIs

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-as-session-with-qos/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: read all of the active subscriptions for the SCS/AS

tags:

- AsSessionWithQoS API SCS/AS level GET Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

tags:

- AsSessionWithQoS API Subscription level POST Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscriptions for the SCS/AS and the subscription Id

tags:

- AsSessionWithQoS API Subscription level GET Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource

tags:

- AsSessionWithQoS API subscription level PUT Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates/replaces an existing subscription resource

tags:

- AsSessionWithQoS API subscription level PATCH Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscriptionPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

tags:

- AsSessionWithQoS API Subscription level DELETE Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AsSessionWithQoSSubscription:

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

qosReference:

type: string

description: Identifies a pre-defined QoS information

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority.

disUeNotif:

type: boolean

ueIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ueIpv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

macAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

sponsorInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/SponsorInformation'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformation'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

required:

- notificationDestination

AsSessionWithQoSSubscriptionPatch:

type: object

properties:

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

qosReference:

type: string

description: Pre-defined QoS reference

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority.

disUeNotif:

type: boolean

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformationRm'

QosMonitoringInformation:

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- reqQosMonParams

- repFreqs

QosMonitoringInformationRm:

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

QosMonitoringReport:

type: object

properties:

ulDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

dlDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

rtDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

UserPlaneNotificationData:

type: object

properties:

transaction:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

eventReports:

type: array

items:

$ref: '#/components/schemas/UserPlaneEventReport'

minItems: 1

description: Contains the reported event and applicable information

required:

- transaction

- eventReports

UserPlaneEventReport:

type: object

properties:

event:

$ref: '#/components/schemas/UserPlaneEvent'

accumulatedUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

flowIds:

type: array

items:

type: integer

minItems: 1

description: Identifies the IP flows that were sent during event subscription

appliedQosRef:

type: string

description: The currently applied QoS reference. Applicable for event QOS\_NOT\_GUARANTEED or SUCCESSFUL\_RESOURCES\_ALLOCATION.

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: Contains the QoS Monitoring Reporting information

required:

- event

UserPlaneEvent:

anyOf:

- type: string

enum:

- SESSION\_TERMINATION

- LOSS\_OF\_BEARER

- RECOVERY\_OF\_BEARER

- RELEASE\_OF\_BEARER

- USAGE\_REPORT

- FAILED\_RESOURCES\_ALLOCATION

- QOS\_GUARANTEED

- QOS\_NOT\_GUARANTEED

- QOS\_MONITORING

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SESSION\_TERMINATION: Indicates that Rx session is terminated.

- LOSS\_OF\_BEARER : Indicates a loss of a bearer.

- RECOVERY\_OF\_BEARER: Indicates a recovery of a bearer.

- RELEASE\_OF\_BEARER: Indicates a release of a bearer.

- USAGE\_REPORT: Indicates the usage report event.

- FAILED\_RESOURCES\_ALLOCATION: Indicates the resource allocation is failed.

- QOS\_GUARANTEED: The QoS targets of one or more SDFs are guaranteed again.

- QOS\_NOT\_GUARANTEED: The QoS targets of one or more SDFs are not being guaranteed.

- QOS\_MONITORING: Indicates a QoS monitoring event.

- SUCCESSFUL\_RESOURCES\_ALLOCATION: Indicates the resource allocation is successful.

\*\*\* End of Changes \*\*\*