**3GPP TSG-CT WG3 Meeting #116e C3-213209**

**E-Meeting, 19th – 28th May 2021 (Revision of C3-21xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0439** | **rev** |  | **Current version:** | **17.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updates to support notification of GEM partial cancellation | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17\_GEM | | | | |  | ***Date:*** | | | 2021-05-10 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | TS 23.682 CR 0477 has been approved in SA2#144e meeting, adding Dynamic management of grouped based event monitoring supporting, including HSS initiated grouped based event monitoring partial cancellation to certain UEs within an active grouped based event monitoring subscription. Hence need to implement in this specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Update in type MonitoringNotification, adding cancellation externalId(s) or MSISDN(s) with new feature to support the partial cancellation initiated from HSS, to be notified to the SCS/AS, and only when the last UE in the group is deleted then to notify the cancellation indicator to SCS/AS to delete the "Individual Monitoring Event Subscription". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Monitoring event for some group members are cancelled unexpectedly. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3.2.2.2, 5.3.4, A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **X** |  | Other core specifications | | | | TS 23.682 CR 0477 | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible feature into the OpenAPI file applicable to MonitoringEvent API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.3.2.2.2 Type: MonitoringNotification

This data type represents a monitoring notification which is sent from the SCEF to the SCS/AS.

Table 5.3.2.2.2-1: Definition of type MonitoringNotification

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | Cardinality | Description | Applicability (NOTE) |
| subscription | Link | 1 | Link to the subscription resource to which this notification is related. |  |
| configResults | array(ConfigResult) | 0..N | Each element identifies a notification of grouping configuration result. |  |
| monitoringEventReports | array(MonitoringEventReport) | 0..N | Each element identifies a monitoring event report. |  |
| cancelInd | Boolean | 0..1 | Indicates whether to request to cancel the corresponding monitoring subscription. Set to false or omitted otherwise. |  |
| cancelExternalIds | array(ExternalId) | 0..N | Identifies the cancelled external Identifier(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data. | Partial\_group\_cancellation |
| cancelMsisdns | array(Msisdn) | 0..N | Identifies the cancelled MSISDN(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data. | Partial\_group\_cancellation |
| appliedParam | AppliedParameterConfiguration | 0..1 | Indicates the applied parameter configuration in the network. For the attributes included in AppliedParameterConfiguration data type, the "maximumLatency" and "maximumResponseTime" attributes require the "Ue-reachability\_notification" feature support, and the "maximumDetectionTime" attribute requires the "Loss\_of\_connectivity\_notification" feature support. | Enhanced\_param\_config |
| NOTE: Properties marked with a feature as defined in subclause 5.3.4 are applicable as described in subclause 5.2.7. If no features are indicated, the related property applies for all the features. | | | | |

\*\*\* 2nd Change \*\*\*

### 5.3.4 Used Features

The table below defines the features applicable to the MonitoringEvent API. Those features are negotiated as described in subclause 5.2.7.

Table 5.3.4-1: Features used by MonitoringEvent API

|  |  |  |
| --- | --- | --- |
| Feature Number | Feature | Description |
| 1 | Loss\_of\_connectivity\_notification | The SCS/AS is notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication |
| 2 | Ue-reachability\_notification | The SCS/AS is notified when the UE becomes reachable for sending either SMS or downlink data to the UE |
| 3 | Location\_notification | The SCS/AS is notified of the current location or the last known location of the UE |
| 4 | Change\_of\_IMSI\_IMEI\_association\_notification | The SCS/AS is notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed |
| 5 | Roaming\_status\_notification | The SCS/AS is notified when the UE's roaming status changes |
| 6 | Communication\_failure\_notification | The SCS/AS is notified of communication failure events |
| 7 | Availability\_after\_DDN\_failure\_notification | The SCS/AS is notified when the UE has become available after a DDN failure |
| 8 | Number\_of\_UEs\_in\_an\_area\_notification | The SCS/AS is notified the number of UEs present in a given geographic area  The feature supports pre-5G (e.g. 4G) requirement. |
| 9 | Notification\_websocket | The delivery of notifications over Websocket is supported according to subclause 5.2.5.4. This feature requires that the Notification\_test\_event featute is also supported. |
| 10 | Notification\_test\_event | The testing of notification connection is supported according to subclause 5.2.5.3. |
| 11 | Subscription\_modification | Modifications of an individual subscription resource. |
| 12 | Number\_of\_UEs\_in\_an\_area\_notification\_5G | The AF is notified the number of UEs present in a given geographic area.  The feature supports the 5G requirement. This feature may only be supported in 5G. |
| 13 | Pdn\_connectivity\_status | The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down. |
| 14 | Downlink\_data\_delivery\_status\_5G | The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed. The feature is not applicable to pre-5G. |
| 15 | Availability\_after\_DDN\_failure\_notification\_enhancement | The AF is notified when the UE has become available after a DDN failure and the traffic matches the packet filter provided by the AF. The feature is not applicable to pre-5G. |
| 16 | Enhanced\_param\_config | This feature supports the co-existence of multiple event configurations for target UE(s) if there are parameters affecting periodic RAU/TAU timer and/or Active Time. Supporting this feature also requires the support of feature number 1 or 2. |
| 17 | API\_support\_capability\_notification | The SCS/AS is notified of the availability of support of service APIs. This feature is only applicable in interworking SCEF+NEF scenario. |
| 18 | eLCS | This feature supports the enhanced location exposure service (e.g. location information preciser than cell level).  The feature is not applicable to pre-5G (e.g. 4G). |
| n | Partial\_group\_cancellation | This feature supports the partial cancellation to a certain UE(s) within the grouped event monitoring subscription. |
| Feature: A short name that can be used to refer to the bit and to the feature, e.g. "Notification".  Description: A clear textual description of the feature. | | |

\*\*\* 3rd Change \*\*\*

## A.3 MonitoringEvent API

openapi: 3.0.0

info:

title: 3gpp-monitoring-event

version: 1.2.0-alpha.1

description: |

API for Monitoring Event.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.1.0 T8 reference point for Northbound APIs

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-monitoring-event/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: read all of the active subscriptions for the SCS/AS

tags:

- MonitoringEvent API SCS/AS level GET Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the SCS/AS)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventSubscription'

minItems: 0

description: Monitoring event subscriptions

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource for monitoring event notification

tags:

- MonitoringEvent API Subscription level POST Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Subscription for notification about monitoring event

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: The operation is successful and immediate report is included.

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventReport'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscriptions for the SCS/AS and the subscription Id

tags:

- MonitoringEvent API Subscription level GET Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource

tags:

- MonitoringEvent API subscription level PUT Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing monitoring event subscription

tags:

- MonitoringEvent API Subscription level DELETE Operation

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: The subscription was terminated successfully, the monitoring event report(s) shall be included if received.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

MonitoringEventSubscription:

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

addExtGroupId:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

minItems: 2

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr :

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

maximumNumberOfReports:

type: integer

minimum: 1

description: Identifies the maximum number of event reports to be generated by the HSS, MME/SGSN as specified in subclause 5.6.0 of 3GPP TS 23.682 [2].

monitorExpireTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

groupReportGuardTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the number of packets that the serving gateway shall buffer in case that the UE is not reachable.

idleStatusIndication:

type: boolean

description: If "monitoringType" is set to "UE\_REACHABILITY" or "AVAILABILITY\_AFTER\_DDN\_FAILURE", this parameter may be included to indicate the notification of when a UE, for which PSM is enabled, transitions into idle mode. "true" indicates enabling of notification; "false" indicate no need to notify. Default value is "false".

locationType:

$ref: '#/components/schemas/LocationType'

accuracy:

$ref: '#/components/schemas/Accuracy'

minimumReportInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maxRptExpireIntvl:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

samplingInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reportingLocEstInd:

type: boolean

description: Indicates whether to request the location estimate for event reporting.

linearDistance:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LinearDistance'

locQoS:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LocationQoS'

svcId:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/ServiceIdentity'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

velocityRequested:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityRequested'

maxAgeOfLocEst:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AgeOfLocationEstimate'

locTimeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

supportedGADShapes:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/SupportedGADShapes'

codeWord:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/CodeWord'

associationType:

$ref: '#/components/schemas/AssociationType'

plmnIndication:

type: boolean

description: If "monitoringType" is "ROAMING\_STATUS", this parameter may be included to indicate the notification of UE's Serving PLMN ID. "true" indicates enabling of notification; "false" indicates disabling of notification. Default value is "false".

locationArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

locationArea5G:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

dddTraDescriptors:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

minItems: 1

dddStati:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

minItems: 1

apiNames:

type: array

items:

type: string

minItems: 1

monitoringEventReport:

$ref: '#/components/schemas/MonitoringEventReport'

required:

- notificationDestination

- monitoringType

anyOf:

- required: [maximumNumberOfReports]

- required: [monitorExpireTime]

MonitoringNotification:

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

configResults:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

minItems: 1

description: Each element identifies a notification of grouping configuration result.

monitoringEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: Monitoring event reports.

cancelInd:

type: boolean

description: Indicates whether to request to cancel the corresponding monitoring subscription. Set to false or omitted otherwise.

cancelExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Identifies the cancelled external Identifier(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data.

cancelMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Identifies the cancelled MSISDN(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data.

appliedParam:

$ref: '#/components/schemas/AppliedParameterConfiguration'

required:

- subscription

MonitoringEventReport:

type: object

properties:

imeiChange:

$ref: '#/components/schemas/AssociationType'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

idleStatusInfo:

$ref: '#/components/schemas/IdleStatusInfo'

locationInfo:

$ref: '#/components/schemas/LocationInfo'

locFailureCause:

$ref: '#/components/schemas/LocationFailureCause'

lossOfConnectReason:

type: integer

description: If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included if available to identify the reason why loss of connectivity is reported. Refer to 3GPP TS 29.336 [11] Subclause 8.4.58.

maxUEAvailabilityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

uePerLocationReport:

$ref: '#/components/schemas/UePerLocationReport'

plmnId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/PlmnId'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

roamingStatus:

type: boolean

description: If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true" if the UE is on roaming status. Set to false or omitted otherwise.

failureCause:

$ref: '#/components/schemas/FailureCause'

eventTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

pdnConnInfoList:

type: array

items:

$ref: '#/components/schemas/PdnConnectionInformation'

minItems: 1

dddStatus:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

dddTrafDescriptor:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

maxWaitTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

apiCaps:

type: array

items:

$ref: '#/components/schemas/ApiCapabilityInfo'

minItems: 0

required:

- monitoringType

IdleStatusInfo:

type: object

properties:

activeTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

edrxCycleLength:

format: float

type: number

minimum: 0

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: Identifies the number of packets shall be buffered in the serving gateway. It shall be present if the idle status indication is requested by the SCS/AS with "idleStatusIndication" in the "monitoringEventSubscription" sets to "true".

idleStatusTimestamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

periodicAUTimer:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

UePerLocationReport:

type: object

properties:

ueCount:

type: integer

minimum: 0

description: Identifies the number of UEs.

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

required:

- ueCount

LocationInfo:

type: object

properties:

ageOfLocationInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationMin'

cellId:

type: string

description: Indicates the Cell Global Identification of the user which identifies the cell the UE is registered.

enodeBId:

type: string

description: Indicates the eNodeB in which the UE is currently located.

routingAreaId:

type: string

description: Identifies the Routing Area Identity of the user where the UE is located.

trackingAreaId:

type: string

description: Identifies the Tracking Area Identity of the user where the UE is located.

plmnId:

type: string

description: Identifies the PLMN Identity of the user where the UE is located.

twanId:

type: string

description: Identifies the TWAN Identity of the user where the UE is located.

geographicArea:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

civicAddress:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

positionMethod:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

qosFulfilInd:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AccuracyFulfilmentIndicator'

ueVelocity:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

FailureCause:

type: object

properties:

bssgpCause:

type: integer

description: Identifies a non-transparent copy of the BSSGP cause code. Refer to 3GPP TS 29.128 [12].

causeType:

type: integer

description: Identify the type of the S1AP-Cause. Refer to 3GPP TS 29.128 [12].

gmmCause:

type: integer

description: Identifies a non-transparent copy of the GMM cause code. Refer to 3GPP TS 29.128 [12].

ranapCause:

type: integer

description: Identifies a non-transparent copy of the RANAP cause code. Refer to 3GPP TS 29.128 [12].

ranNasCause:

type: string

description: Indicates RAN and/or NAS release cause code information, TWAN release cause code information or untrusted WLAN release cause code information. Refer to 3GPP TS 29.214 [10].

s1ApCause:

type: integer

description: Identifies a non-transparent copy of the S1AP cause code. Refer to 3GPP TS 29.128 [12].

smCause:

type: integer

description: Identifies a non-transparent copy of the SM cause code. Refer to 3GPP TS 29.128 [12].

PdnConnectionInformation:

type: object

properties:

status:

$ref: '#/components/schemas/PdnConnectionStatus'

apn:

type: string

description: Identify the APN, it is depending on the SCEF local configuration whether or not this attribute is sent to the SCS/AS.

pdnType:

$ref: '#/components/schemas/PdnType'

interfaceInd:

$ref: '#/components/schemas/InterfaceIndication'

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addrs:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

required:

- status

- pdnType

AppliedParameterConfiguration:

type: object

properties:

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

ApiCapabilityInfo:

type: object

properties:

apiName:

type: string

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- apiName

- suppFeat

#

# ENUMS

#

MonitoringType:

anyOf:

- type: string

enum:

- LOSS\_OF\_CONNECTIVITY

- UE\_REACHABILITY

- LOCATION\_REPORTING

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION

- ROAMING\_STATUS

- COMMUNICATION\_FAILURE

- AVAILABILITY\_AFTER\_DDN\_FAILURE

- NUMBER\_OF\_UES\_IN\_AN\_AREA

- PDN\_CONNECTIVITY\_STATUS

- DOWNLINK\_DATA\_DELIVERY\_STATUS

- API\_SUPPORT\_CAPABILITY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- LOSS\_OF\_CONNECTIVITY: The SCS/AS requests to be notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication

- UE\_REACHABILITY: The SCS/AS requests to be notified when the UE becomes reachable for sending either SMS or downlink data to the UE

- LOCATION\_REPORTING: The SCS/AS requests to be notified of the current location or the last known location of the UE

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION: The SCS/AS requests to be notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed

- ROAMING\_STATUS: The SCS/AS queries the UE's current roaming status and requests to get notified when the status changes

- COMMUNICATION\_FAILURE: The SCS/AS requests to be notified of communication failure events

- AVAILABILITY\_AFTER\_DDN\_FAILURE: The SCS/AS requests to be notified when the UE has become available after a DDN failure

- NUMBER\_OF\_UES\_IN\_AN\_AREA: The SCS/AS requests to be notified the number of UEs in a given geographic area

- PDN\_CONNECTIVITY\_STATUS: The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down

- DOWNLINK\_DATA\_DELIVERY\_STATUS: The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed.

- API\_SUPPORT\_CAPABILITY: The SCS/AS requests to be notified of the availability of support of service APIs.

ReachabilityType:

anyOf:

- type: string

enum:

- SMS

- DATA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SMS : The SCS/AS requests to be notified when the UE becomes reachable for sending SMS to the UE

- DATA: The SCS/AS requests to be notified when the UE becomes reachable for sending downlink data to the UE

LocationType:

anyOf:

- type: string

enum:

- CURRENT\_LOCATION

- LAST\_KNOWN\_LOCATION

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION

- INITIAL\_LOCATION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CURRENT\_LOCATION: The SCS/AS requests to be notified for current location

- LAST\_KNOWN\_LOCATION: The SCS/AS requests to be notified for last known location

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION: The AF requests the current or last known location

- INITIAL\_LOCATION: The AF requests the initial location

AssociationType:

anyOf:

- type: string

enum:

- IMEI

- IMEISV

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- IMEI: The value shall be used when the change of IMSI-IMEI association shall be detected

- IMEISV: The value shall be used when the change of IMSI-IMEISV association shall be detected

Accuracy:

anyOf:

- type: string

enum:

- CGI\_ECGI

- ENODEB

- TA\_RA

- PLMN

- TWAN\_ID

- GEO\_AREA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CGI\_ECGI: The SCS/AS requests to be notified at cell level location accuracy.

- ENODEB: The SCS/AS requests to be notified at eNodeB level location accuracy.

- TA\_RA: The SCS/AS requests to be notified at TA/RA level location accuracy.

- PLMN: The SCS/AS requests to be notified at PLMN level location accuracy.

- TWAN\_ID: The SCS/AS requests to be notified at TWAN identifier level location accuracy.

- GEO\_AREA: The SCS/AS requests to be notified of the geographical area accuracy.

PdnConnectionStatus:

anyOf:

- type: string

enum:

- CREATED

- RELEASED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CREATED: The PDN connection is created.

- RELEASED: The PDN connection is released.

PdnType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- IPV4V6

- NON\_IP

- ETHERNET

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- IPV4: PDN connection of IPv4 type.

- IPV6: PDN connection of IPv6 type.

- IPV4V6: PDN connection of IPv4v6 type.

- NON\_IP: PDN connection of non-IP type.

- ETHERNET: PDN connection of Ethernet type.

InterfaceIndication:

anyOf:

- type: string

enum:

- EXPOSURE\_FUNCTION

- PDN\_GATEWAY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- EXPOSURE\_FUNCTION: SCEF is used for the PDN connection towards the SCS/AS.

- PDN\_GATEWAY: PDN gateway is used for the PDN connection towards the SCS/AS.

LocationFailureCause:

anyOf:

- type: string

enum:

- POSITIONING\_DENIED

- UNSUPPORTED\_BY\_UE

- NOT\_REGISTED\_UE

- UNSPECIFIED

- type: string

description: >

This string Indicates the location positioning failure cause.

Possible values are

- POSITIONING\_DENIED: Positioning is denied.

- UNSUPPORTED\_BY\_UE: Positioning is not supported by UE.

- NOT\_REGISTED\_UE: UE is not registered.

- UNSPECIFIED: Unspecified.

\*\*\* End of Changes \*\*\*