**3GPP TSG-CT3 Meeting #116e C3-213055\_r1**

**E-Meeting, 19th – 28th May 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **0343** | **rev** | **1** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Wrong attribute name in the OpenAPI file |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eV2XARC |  | ***Date:*** | 2021-05-xx |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The "paramOverUu" attribute of the ServiceParameterDataPatch data type is incorrectly written starting with a capital letter, i.e. "**P**aramOverUu" in the OpenAPI file of the ServiceParameter API. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Correct the above mentionned issue.
 |
|  |  |
| ***Consequences if not approved:*** | * Misalignment within the specification and potential interoperability issues.
 |
|  |  |
| ***Clauses affected:*** | A.9 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces does not impact OpenAPI specification files. |
|  |  |
| ***This CR's revision history:*** | Rev 1: As the initially proposed correction is non backwards compatible, it is proposed to rather add a NOTE in Table 5.11.2.3.3 to clarify the "**p**aramOverUu" attribute corresponds to the "**P**aramOverUu" attribute defined in OpenAPI file. |

\* \* \* Start of changes \* \* \* \*

##### 5.11.2.3.3 Type: ServiceParameterDataPatch

Table 5.11.2.3.3-1: Definition of type ServiceParameterDataPatch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| paramOverPc5 | ParameterOverPc5Rm | O | 0..1 | Contains the service parameter used over PC5 |  |
| paramOverUu | ParameterOverUuRm | O | 0..1 | Contains the service parameter used over Uu(NOTE) |  |
| NOTE: This attribute corresponds to the "ParamOverUu" attribute in the OpenAPI definition of the ServiceParameterDataPatch data type in subclause A.9. |

\* \* \* End of changes \* \* \* \*