**3GPP TSG-CT3 Meeting #116e C3-213056\_r1**

**E-Meeting, 19th – 28th May 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **0344** | **rev** | **1** | **Current version:** | **17.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Wrong attribute name in the OpenAPI file | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eV2XARC | | | | |  | ***Date:*** | | | 2021-05-xx |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The "paramOverUu" attribute of the ServiceParameterDataPatch data type is incorrectly written starting with a capital letter, i.e. "**P**aramOverUu" in the OpenAPI file of the ServiceParameter API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This CR proposes to:   * Correct the above mentionned issue. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | * Misalignment within the specification and potential interoperability issues. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.9 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR does not impact the OpenAPI specification files. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Rev 1: As the initially proposed correction is non backwards compatible, it is proposed to rather add a NOTE in Table 5.11.2.3.3 to clarify the "**p**aramOverUu" attribute corresponds to the "**P**aramOverUu" attribute defined in OpenAPI file. | | | | | | | | |

\* \* \* Start of changes \* \* \* \*

##### 5.11.2.3.3 Type: ServiceParameterDataPatch

Table 5.11.2.3.3-1: Definition of type ServiceParameterDataPatch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| paramOverPc5 | ParameterOverPc5Rm | O | 0..1 | Contains the service parameter used over PC5 |  |
| paramOverUu | ParameterOverUuRm | O | 0..1 | Contains the service parameter used over Uu  (NOTE) |  |
| NOTE: This attribute corresponds to the "ParamOverUu" attribute in the OpenAPI definition of the ServiceParameterDataPatch data type in subclause A.9. | | | | | |

\* \* \* End of changes \* \* \* \*