**3GPP TSG-CT WG3 Meeting #118eC3-215137**

**E-Meeting, 11th – 15th October 2021** (revision of C3-21xxxx)

**Source: Ericsson**

**Title: Pseudo-CR on OpenAPI definition of Eees\_SelectedTargetEAS service**

**Spec: 3GPP TS 29.558 v1.0.0**

**Agenda item: 17.9**

**Document for: Decision**

**1. Introduction**

This pCR proposes the OpenAPI definition of Eees\_SelectedTargetEAS PI.

**2. Reason for Change**

The OpenAPI file of Eees\_SelectedTargetEAS API is not defined yet.

**3. Conclusions**

Define OpenAPI for Eees\_SelectedTargetEAS service.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.558 v1.0.0.

\*\*\* 1st Change \*\*\*

## A.m(new) Eees\_SelectedTargetEAS API

openapi: 3.0.0

info:

title: EES SELECTED TARGET EAS\_API

description: |

API for EES SELECTED TARGET EAS.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: 1.0.0-alpha.1

externalDocs:

description: 3GPP TS 29.558 V1.1.0 Enabling Edge Applications; Application Programming Interface (API) specification; Stage 3

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

servers:

- url: '{apiRoot}/eees-selected-target-eas/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

paths:

/declare:

post:

summary: Declare the selected target EAS.

operationId: DeclareTargetEAS

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SelectedEAS'

responses:

'204':

description: No Content.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

schemas:

SelectedEAS:

description: Represents the selected target EAS information.

type: object

properties:

easId:

type: string

description: Identifier of the selected target EAS.

ueId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

endPt:

$ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

required:

- easId

- ueId

- endPt

\*\*\* End of Changes \*\*\*