**3GPP TSG-CT WG3 Meeting #118eC3-215137**

**E-Meeting, 11th – 15th October 2021** (revision of C3-21xxxx)

**Source: Ericsson**

**Title: Pseudo-CR on OpenAPI definition of Eees\_SelectedTargetEAS service**

**Spec: 3GPP TS 29.558 v1.0.0**

**Agenda item: 17.9**

**Document for: Decision**

**1. Introduction**

This pCR proposes the OpenAPI definition of Eees\_SelectedTargetEAS PI.

**2. Reason for Change**

The OpenAPI file of Eees\_SelectedTargetEAS API is not defined yet.

**3. Conclusions**

Define OpenAPI for Eees\_SelectedTargetEAS service.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.558 v1.0.0.

\*\*\* 1st Change \*\*\*

## A.m(new) Eees\_SelectedTargetEAS API

openapi: 3.0.0

info:

 title: EES SELECTED TARGET EAS\_API

 description: |

 API for EES SELECTED TARGET EAS.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: 1.0.0-alpha.1

externalDocs:

 description: 3GPP TS 29.558 V1.1.0 Enabling Edge Applications; Application Programming Interface (API) specification; Stage 3

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.558/

servers:

 - url: '{apiRoot}/eees-selected-target-eas/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 7.5 of 3GPP TS 29.558.

paths:

 /declare:

 post:

 summary: Declare the selected target EAS.

 operationId: DeclareTargetEAS

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SelectedEAS'

 responses:

 '204':

 description: No Content.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 schemas:

 SelectedEAS:

 description: Represents the selected target EAS information.

 type: object

 properties:

 easId:

 type: string

 description: Identifier of the selected target EAS.

 ueId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 endPt:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 required:

 - easId

 - ueId

 - endPt

\*\*\* End of Changes \*\*\*