**3GPP TSG-CT3 Meeting #119bis-e C3-220066**

**E-Meeting, 17th – 21st January 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.122** | **CR** | **0546** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Updating the AsSessionWithQoS API data types table |
|  |  |
| ***Source to WG:*** | KDDI, Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | NBI17 |  | ***Date:*** | 2022-01-10 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The data types re-used by the AsSessionWithQoS API are listed in table 5.14.2.1.1-1, but the API specific data types are not listed anywhere in the specification. TscPriorityLevel and TscPriorityLevelRm data types are not listed in table 5.14.2.1.1-1. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Add a table in clause 5.14.2.1.1 to list all the the AsSessionWithQoS API specific data types.
* Add TscPriorityLevel and TscPriorityLevelRm data types to table 5.14.2.1.1-1.
 |
|  |  |
| ***Consequences if not approved:*** | * The quality and readability of the specification are not improved.
 |
|  |  |
| ***Clauses affected:*** | 5.14.2.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact OpenAPI specification files defined in this specification. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* Start of changes \* \* \*

##### 5.14.2.1.1 Introduction

This clause defines data structures to be used in resource representations, including subscription resources.

Editor's Note: It is FFS to implement the individual alternative QoS parameters in this API according to stage 2 specs.

Table 5.14.2.1.1-1 specifies data types re-used by the AsSessionWithQoS API from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the AsSessionWithQoS API.

Table 5.14.2.1.1-1: AsSessionWithQoS API re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Dnn | 3GPP TS 29.571 [45] | Identifies a DNN. |
| EthFlowDescription | 3GPP TS 29.514 [52] | Defines a packet filter for an Ethernet flow.(NOTE 1) |
| IpAddr | 3GPP TS 29.571 [45] | UE IP Address. |
| MacAddr48 | 3GPP TS 29.571 [45] | MAC Address. |
| ReportingFrequency | 3GPP TS 29.512 [8] | Indicates the frequency for the reporting, such as event triggered, periodic, when the PDU Session is released, and/or any combination. (NOTE 2) |
| RequestedQosMonitoringParameter | 3GPP TS 29.512 [8] | Indicate the UL packet delay, DL packet delay or round trip packet delay between the UE and the UPF is to be monitored when the QoS Monitoring for URLLC is enabled for the service data flow. (NOTE 2) |
| Snssai | 3GPP TS 29.571 [45] | Identifies the S-NSSAI. |
| SupportedFeatures | 3GPP TS 29.571 [45] | Used to negotiate the applicability of the optional features defined in table 5.14.4-1. |
| TscaiInputContainer | 3GPP TS 29.514 [52] | TSCAI Input information container. |
| TscPriorityLevel | 3GPP TS 29.514 [52] | Represents priority of TSC Flows. |
| TscPriorityLevelRm | 3GPP TS 29.514 [52] | Represents the same way as the TscPriorityLevel data type, but with the OpenAPI "nullable: true" property. |
| NOTE 1: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange\_5G as specified in clause 5.14.4 shall be supported.NOTE 2: In order to support QoS Monitoring, feature QoSMonitoring\_5G as specified in clause 5.14.4 shall be supported. |

Table 5.14.2.1.1-2 specifies the data types defined for the AsSessionWithQoS API.

Table 5.14.2.1.1-2: AsSessionWithQoS API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| AsSessionWithQoSSubscription | 5.14.2.1.2 | Represents an individual AS session with required QoS subscription resource. |  |
| AsSessionWithQoSSubscriptionPatch | 5.14.2.1.3 | Represents parameters to modify an AS session with specific QoS subscription. |  |
| QosMonitoringInformation | 5.14.2.1.6 | Represents QoS monitoring information. | QoSMonitoring\_5G |
| QosMonitoringInformationRm | 5.14.2.1.7 | Represents the same as the QosMonitoringInformation data type but with the "nullable: true" property. | QoSMonitoring\_5G |
| QosMonitoringReport | 5.14.2.1.8 | Represents a QoS monitoring report. | QoSMonitoring\_5G |
| TscQosRequirement | 5.14.2.1.9 | Represents QoS requirements for time sensitive communication. | TSC\_5G |
| TscQosRequirementRm | 5.14.2.1.10 | Represents the same as the TscQosRequirement data type but with the "nullable: true" property. | TSC\_5G |
| UserPlaneEvent | 5.14.2.2.3 | Represents the user plane event. | enNB |
| UserPlaneEventReport | 5.14.2.1.5 | Represents an event report for user plane. | enNB |
| UserPlaneNotificationData | 5.14.2.1.4 | Represents the parameters to be conveyed in a user plane event(s) notification. | enNB |

\* \* \* End of changes \* \* \*