**TSG-CT WG3 Meeting #119bis-e *C3-220169***

**E-Meeting, 17th – 21st January 2022**

**Source: Huawei**

**Title: State of time synchronization Configuration**

**Spec: 3GPP TS 29.565 v1.0.0**

**Agenda item: 17.16**

**Document for: Decision**

**1. Introduction**

<Introduction part (optional)>

**2. Reason for Change**

As defined in clause 4.15.9.3.2 of 23.502,

1. The TSCTSF constructs PMIC(s) and UMIC to NW-TT to activate the time synchronization service in NW-TT in respect to the service parameters
2. Upon reception of responses from each DS-TT and NW-TT, the TSCTSF determines the state of the time synchronization configuration.
3. The TSCTSF constructs a PMIC to each DS-TT/UE to subscribe for the port management information changes in the DS-TT. The TSCTSF constructs PMIC(s) and UMIC to NW-TT to subscribe for the port management and user-plane management information changes in NW-TT.
4. The TSCTSF notifies the NEF (or AF) with the Ntsctsf\_TimeSynchronization\_ConfigUpdateNotify service operation, containing the time synchronization configuration Id and the current state of the time synchronization service configuration.

**3. Conclusions**

TSCTSF reports the state of configuration.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.565.

\* \* \* First Change \* \* \* \*

##### 5.2.2.8.2 Notifying the current state of an existing configuration

Figure 5.2.2.8.2-1 illustrates the notification about the current state of the time synchronization configuration.



Figure 5.2.2.8.2-1: Notification about the current state of the time synchronization configuration

When the TSFCST receives the notification for each DS-TT and NW-TT from the PCF, the TSCTSF shall determine the current state of the time synchronization configuration and sends an HTTP POST request with "{configNotifUri}", as previously provided by the NF service consumer within the corresponding configuration, as URI and the TimeSyncExposureConfigNotif data structure as request body, as shown in figure 5.2.2.8.2-1, step 1.

The TimeSyncExposureConfigNotif data structure as request body that shall include:

- Notification correlation ID provided by the NF service consumer during the configuration within "configNotifId" attribute;

- current state of the time synchronization configuration.

Editor's Note: Error/Redirect responses are FFS.

\* \* \* Next Change \* \* \* \*

##### 6.1.6.2.x1 Type: TimeSyncExposureConfigNotif

Table 6.1.6.2.x1-1: Definition of type TimeSyncExposureConfigNotif

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| configNotifId | string | M | 1 | Notification Correlation ID assigned by the NF service consumer. |  |
| stateOfConfig | StageOfConfiguration | M | 1 | Indicates the current state of time synchroniztion service configuration |  |

\* \* \* Next Change \* \* \* \*

##### 6.1.6.2.x2 Type: StageOfConfiguration

Table 6.1.6.2.x2-1: Definition of type TimeSyncExposureConfigNotif

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| state | boolean | M | 1 | When it is set to true, it indicates the states of configurations for NW-TT port and all DS-TT port are active.  When it is set to false, it indicates the state of configurations for NW-TT port or at least one of the DS-TT port are inactive. |  |
| inactiveNwtt | boolean | C | 0..1 | When it is included and set to true, it indicates the state of configuration for NW-TT port is inactive. It may be included when the "state" attribute is set to false. Default value is false. |  |
| inactiveDstts | array(Supi) | C | 1..N | Contains the UE identities. The states of configurations for DS-TT ports corresponding to these UEs are inactive. It may be included when the "state" attribute is set to false. |  |

\* \* \* Next Change \* \* \* \*

## A.2 Ntsctsf\_TimeSynchronization API

openapi: 3.0.0

info:

title: Ntsctsf\_TimeSynchronization Service API

version: 1.0.0-alpha.1

description: |

TSCTSF Time Synchronization Service.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.565 V1.0.0; 5G System; Time Sensitive Communication and Time Synchronization Function Services; Stage 3.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.565/'

#

servers:

- url: '{apiRoot}/ntsctsf-time-sync/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- ntsctsf-timesynchronization

paths:

/subscriptions:

post:

summary: Creates a new subscription to notification of capability of time synchronization service resource

operationId: TimeSynchronizationExposureSubscriptions

tags:

- Time Synchronization Exposure Subscriptions (Collection)

requestBody:

description: Contains the information for the creation the resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

responses:

'201':

description: Successful creation of the resource

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

headers:

Location:

description: 'Contains the URI of the created individual time synchronization exposure subscription resource, according to the structure: {apiRoot}/ntsctsf-time-sync/{apiVersion}/subscriptions/{subscriptionId}'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

subsEventNotification:

'{$request.body#/subsNotifUri':

post:

requestBody:

description: Notification of an event occurrence in the TSCTSF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsNotif'

responses:

'204':

description: The receipt of the notification is acknowledged

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

get:

summary: "Reads an existing Individual Time Synchronization Exposure Subscription"

operationId: GetIndividualTimeSynchronizationExposureSubscription

tags:

- Individual Time Synchronization Exposure Subscription (Document)

parameters:

- name: subscriptionId

description: string identifying an Individual Time Synchronization Exposure Subscription

in: path

required: true

schema:

type: string

responses:

'200':

description: A representation of the resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

operationId: DeleteIndividualTimeSynchronizationExposureSubscription

summary: Delete an Individual TimeSynchronization Exposure Subscription

tags:

- Individual Time Synchronization Exposure Subscription (Document)

parameters:

- name: subscriptionId

in: path

description: string identifying an Individual Time Synchronization Exposure Subscription

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was successfully deleted

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}/configurations:

post:

summary: "Craete a new Individual Time Synchronization Exposure Configuration"

operationId: CreateIndividualTimeSynchronizationExposureConfiguration

tags:

- Individual Time Synchronization Exposure Configuration (Document)

parameters:

- name: subscriptionId

description: string identifying an Individual Time Synchronization Exposure Subscription

in: path

required: true

schema:

type: string

requestBody:

description: Contains the information for the creation the resource

required: true

content:

application/json:

schema:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

responses:

'201':

description: Successful creation of the resource

content:

application/json:

schema:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

headers:

Location:

description: 'Contains the URI of the created individual time synchronization exposure configuration resource, according to the structure: {apiRoot}/ntsctsf-time-sync/{apiVersion}/subscriptions/{subscriptionId}/configurations/{configurationId}'

required: true

schema:

type: string

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

configEventNotification:

'{$request.body#/configNotifUri':

post:

requestBody:

description: Notification of an event occurrence in the TSCTSF.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfigNotif'

responses:

'204':

description: The receipt of the notification is acknowledged

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}/configurations/{configurationId}:

get:

summary: "Reads an existing Individual Time Synchronization Exposure Configuration"

operationId: GetIndividualTimeSynchronizationExposureConfiguration

tags:

- Individual Time Synchronization Exposure Configuration (Document)

parameters:

- name: subscriptionId

description: string identifying an Individual Time Synchronization Exposure Subscription

in: path

required: true

schema:

type: string

- name: configurationId

description: string identifying an Individual Time Synchronization Exposure Configuration

in: path

required: true

schema:

type: string

responses:

'200':

description: A representation of the resource is returned.

content:

application/json:

schema:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

operationId: ReplaceIndividualTimeSynchronizationExposureConfiguration

summary: Replace an individual Time Synchronization Exposure Configuration

tags:

- IndividualTimeSynchronizationExposureConfiguration (Document)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

parameters:

- name: subscriptionId

description: string identifying an Individual Time Synchronization Exposure Subscription

in: path

required: true

schema:

type: string

- name: configurationId

description: string identifying an Individual Time Synchronization Exposure Configuration

in: path

required: true

schema:

type: string

responses:

'200':

description: OK. Resource was successfully modified and representation is returned

content:

application/json:

schema:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/TimeSyncExposureConfig'

'204':

description: No Content. Resource was successfully modified

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

operationId: DeleteIndividualTimeSynchronizationExposureConfiguration

summary: Delete an Individual TimeSynchronization Exposure Configuration

tags:

- Individual Time Synchronization Exposure Configuration (Document)

parameters:

- name: subscriptionId

in: path

description: string identifying an Individual Time Synchronization Exposure Subscription

required: true

schema:

type: string

- name: configurationId

description: string identifying an Individual Time Synchronization Exposure Configuration

in: path

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was successfully deleted

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

ntsctsf-timesynchronization: Access to the Ntsctsf\_TimeSynchronization API

schemas:

TimeSyncExposureSubsc:

description: Contains the parameters for the subscription to notification of capability of time synchronization service.

type: object

properties:

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

interGrpId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

anyUeInd:

type: boolean

description: Identifies whether the request applies to any UE. This attribute shall set to "true" if applicable for any UE, otherwise, set to "false".

notifMethod:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

subscribedEvents:

type: array

items:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/SubscribedEvent'

minItems: 1

eventFilters:

type: array

items:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/EventFilter'

minItems: 1

subsNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

maxReportNbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- subsNotifUri

- subsNotifId

TimeSyncExposureSubsNotif:

description: Contains the notification of time synchronization service.

type: object

properties:

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

eventNotifs:

type: array

items:

$ref: '#/components/schemas/SubsEventNotification'

minItems: 1

SubsEventNotification:

description: Contains the notification of capability of time synchronization for a list of UEs.

type: object

properties:

event:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/SubscribedEvent'

timeSyncCapas:

type: array

items:

$ref: '#/components/schemas/TimeSyncCapability'

minItems: 1

TimeSyncCapability:

description: Contains the capability of time synchronization service

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

gmCapables:

type: array

items:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/GmCapable'

minItems: 1

ptpCapForUes:

type: object

additionalProperties:

$ref: '#/components/schemas/PtpCapabilitiesPerUe'

minProperties: 1

description: Contains the PTP capabilities supported by each of the UE(s). The key of the map is the supi.

required:

- upNodeId

- ptpCapForUes

PtpCapabilitiesPerUe:

description: Contains the supported PTP capabilities per UE.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

ptpCaps:

type: array

items:

$ref: 'TS29522\_TimeSyncExposure.yaml#/components/schemas/EventFilter'

minItems: 1

required:

- supi

- ptpCaps

TimeSyncExposureConfigNotif:

description: Contains the notification of time synchronization service state.

type: object

properties:

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

stateOfConfig:

$ref: '#/components/schemas/StageOfConfiguration'

required:

- configNotifId

- stateOfConfig

StageOfConfiguration:

description: Contains the state of the time synchronization configuration.

type: object

properties:

state:

type: boolean

description: When it is set to true, it indicates the states of configurations for NW-TT port and all DS-TT ports are active.

inactiveNwtt:

type: boolean

description: When it is included and set to true, it indicates the state of configuration for NW-TT port is inactive.

inactiveDstts:

description: Contains the UE identities. The states of configurations for DS-TT ports corresponding to these UEs are inactive.

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

required:

- state

\* \* \* End of Changes \* \* \* \*