**3GPP TSG-CT WG4 Meeting #101eC4-205**

**E-Meeting, 3rd – 13th November 2020 was C4-205235**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.500** | **CR** | **0186** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [*HE**LP*](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Too Many Requests |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2020-11-03 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | When the NF Service Producer receives too many requests, regardless whether this is caused by a single or by multiple NF Service Consumers, it may respond with a status code "429 Too Many Requests". |
|  |  |
| ***Summary of change:*** | Remove the restriction to send "429 Too Many Requests" only when the source of extensive traffic is a single NF Service Consumer.  |
|  |  |
| ***Consequences if not approved:*** | NF Service Producers may not be able to send "429 Too Many Requests" status codes.  |
|  |  |
| ***Clauses affected:*** | 6.4.2.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

#### 6.4.2.3 HTTP Status Code "429 Too Many Requests"

This status code may be sent, if supported by the server, when the NF Service Producer detects that NF Service Consumers are sending excessive traffic which, if continued over time, may lead to (or may increase) an overload situation in the NF Service Producer.

The HTTP header field "Retry-After" may be added in the response to indicate how long the NF Service Consumer has to wait before making a new request.

As for all 4xx status codes, this indicates a client-related issue (not limited to a specific HTTP method), and it indicates that the client seems to be misbehaving.

\* \* \* End Of Change \* \* \* \*