**3GPP TSG-CT WG4 Meeting #111-eC4-224**

**E-Meeting, 18th – 26th August 2022 revision of C4-224128**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.571** | **CR** | **0368** | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Spatial Validity Condition | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eEDGE\_5GC | | | | |  | ***Date:*** | | | 2022-08-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | According to 23.548 the Spatial Validity Condition may include a Geographical Service Area. See S2-2204737. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add attribute geographicalServiceArea to type SpatialValidityCond | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Misalignment with 23.548 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.4.4.74, 5.4.4.yy (new), A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible corrections to the following APIs:  TS29503\_Nudm\_PP.yaml  TS29503\_Nudm\_SDM.yaml  TS29504\_Nudr\_DR.yaml  TS29522\_EcsAddressProvision.yaml | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[3] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[4] IETF RFC 1166: "Internet Numbers".

[5] IETF RFC 5952: "A recommendation for IPv6 address text representation".

[6] IETF RFC 3986: "Uniform Resource Identifier (URI): Generic Syntax".

[7] 3GPP TS 23.003: "Numbering, addressing and identification".

[8] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[9] IETF RFC 7807: "Problem Details for HTTP APIs".

[10] IETF RFC 3339: "Date and Time on the Internet: Timestamps".

[11] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP) ".

[12] IETF RFC 6901: "JavaScript Object Notation (JSON) Pointer".

[13] 3GPP TS 24.007: "Mobile radio interface signalling layer 3; General aspects".

[14] IETF RFC 6902: "JavaScript Object Notation (JSON) Patch".

[15] IETF RFC 4122: "A Universally Unique IDentifier (UUID) URN Namespace".

[16] 3GPP TS 36.413: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 Application Protocol (S1AP)".

[17] IETF RFC 7042: "IANA Considerations and IETF Protocol and Documentation Usage for IEEE 802 Parameters".

[18] IETF RFC 6733: "Diameter Base Protocol".

[19] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[20] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[21] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[22] Void.

[23] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[24] ITU-T Recommendation Q.763 (1999): "Specifications of Signalling System No.7; Formats and codes".

[25] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[26] 3GPP TS 23.015: "Technical Realization of Operator Determined Barring".

[27] 3GPP TR 21.900: "Technical Specification Group working methods".

[28] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[29] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[30] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

[31] IEEE Std 802.11-2012: "IEEE Standard for Information technology - Telecommunications and information exchange between systems - Local and metropolitan area networks - Specific requirements - Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications".

[32] CableLabs WR-TR-5WWC-ARCH: "5G Wireless Wireline Converged Core Architecture".

[33] 3GPP TS 23.401: "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access; Stage 2".

[34] BBF TR-069: "CPE WAN Management Protocol".

[35] BBF TR-369: "User Services Platform (USP)".

[36] 3GPP TS 23.287: "Architecture enhancements for 5G System (5GS) to support Vehicle-to-Everything (V2X) services".

[37] BBF TR-470: "5G Wireless Wireline Convergence Architecture".

[38] IEEE "Guidelines for Use of Extended Unique Identifier (EUI), Organizationally Unique Identifier (OUI), and Company ID (CID)", <https://standards.ieee.org/content/dam/ieee-standards/standards/web/documents/tutorials/eui.pdf>

[39] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[40] IETF RFC 5580: "Carrying Location Objects in RADIUS and Diameter".

[41] BBF TR-456: "AGF Functional Requirements".

[42] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[43] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[44] ECMA-262: "ECMAScript® Language Specification", <https://www.ecma-international.org/ecma-262/5.1/>.

[45] 3GPP TS 33.246: "Security of Multimedia Broadcast/Multicast Service (MBMS)".

[46] 3GPP TS 33.501: "Security architecture and procedures for 5G system; Stage 2".

[xx] 3GPP TS 23.558: "Architecture for enabling Edge Applications (EA)".

\* \* \* Next Change \* \* \* \*

#### 5.4.4.74 Type: SpatialValidityCond

Table 5.4.4.74-1: Definition of type SpatialValidityCond

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| trackingAreaList | array(Tai) | C | 1..N | This IE shall be included if available.  When present, it shall contain the list of tracking areas identities. |
| countries | array(Mcc) | O | 1..N | When present, it shall contain the list of Mobile Country Codes. |
| geographicalServiceArea | GeoServiceArea | O | 0..1 | Geographical Service Area; see 3GPP TS 23.558 [xx] clause 7.3.3.3 |

\* \* \* Next Change \* \* \* \*

#### 5.4.4.yy Type: GeoServiceArea

Table 5.4.4.yy-1: Definition of type GeoServiceArea

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| geographicAreaList | array(GeographicArea) | O | 1..N | Identifies a list of geographic area specified by different shapes. |
| civicAddressList | Array(CivicAddress) | O | 1..N | Identifies a list of civic address. |

\* \* \* Next Change \* \* \* \*

# A.2 Data related to Common Data Types

openapi: 3.0.0

\*\*\*\*\*\*\*\*\*\*\*text not shown for clarity\*\*\*\*\*\*\*\*\*\*

SpatialValidityCond:

description: Contains the Spatial Validity Condition.

type: object

properties:

trackingAreaList:

type: array

items:

$ref: '#/components/schemas/Tai'

minItems: 1

countries:

type: array

items:

$ref: '#/components/schemas/Mcc'

minItems: 1

geographicalServiceArea:

$ref: '#/components/schemas/GeoServiceArea'

GeoServiceArea:

description: List of geographic area or list of civic address info

type: object

properties:

geographicAreaList:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

minItems: 1

civicAddressList:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

minItems: 1

\*\*\*\*\*\*\*\*\*\*\*text not shown for clarity\*\*\*\*\*\*\*\*\*\*

\* \* \* End Of Change \* \* \* \*