**3GPP TSG-CT WG4 Meeting #111-eC4-224269**

**E-Meeting, 18th – 26th August 2022 *was C4-224269***

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | TEI17, 5GS\_Ph1-CT |  | ***Date:*** | 2022-08-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | 3GPP TS 29.510 has specified that the NF (Service) instance can register default notification subscription in NF profile to receive notifications with implicit subscriptions. Within the default notification subscriptions, it is possible to indicate the supported API versions for the corresponding service of the NF (Service) instance acting as the NF service consumer. The producer then compose the notification accordingly.However, the default notification with same notification type may come from different service, e.g. for LOCATION\_NOTIFICATION, the notification may be generated by AMF (Namf\_Location\_EventNotify) or LMF (Nmlf\_Location\_EventNotify). If the supported API versions of the AMF API and LMF API may be different by the NF consumer, it is not possible to clearly identify the supported API version accordingly.**NOTE**: In Rel-17 the supported features for the default notification subscription is also service specific. |
|  |  |
| ***Summary of change:*** | 1/ Define new data type for service specific information for default notification subscription.2/ Add new IE as map of service specific information in default notification subscription.3/ Update OpenAPI accordingly |
|  |  |
| ***Consequences if not approved:*** | When default notification for one notification type can be generated by multiple services, NF consumer cannot indicate the supported API versions per service. Notification will fail if NF producer compose the notification with unsupported API version. |
|  |  |
| ***Clauses affected:*** | 6.1.6.1, 6.1.6.2.4, 6.1.6.2.x, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduce backward compatible corrections on Nnrf\_NFManagement and Nnrf\_NFDiscovery APIs. |
|  |  |
| ***This CR's revision history:*** | Rev1:* Change Category to "Cat F"
* Define the service name as specified in the ServiceName data type as the map keys
* Give an example for LOCATION\_NOTIFICATION type
* Editorial corrections
 |

\* \* \* First Change \* \* \* \*

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nnrf\_NFManagement service-based interface protocol.

Table 6.1.6.1-1: Nnrf\_NFManagement specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| NFProfile | 6.1.6.2.2 | Information of an NF Instance registered in the NRF. |
| NFService | 6.1.6.2.3 | Information of a given NF Service Instance; it is part of the NFProfile of an NF Instance. |
| DefaultNotificationSubscription | 6.1.6.2.4 | Data structure for specifying the notifications the NF service subscribes by default along with callback URI. |
| IpEndPoint | 6.1.6.2.5 | IP addressing information of a given NFService; it consists on, e.g. IP address, TCP port, transport protocol... |
| UdrInfo | 6.1.6.2.6 | Information of an UDR NF Instance. |
| UdmInfo | 6.1.6.2.7 | Information of an UDM NF Instance. |
| AusfInfo | 6.1.6.2.8 | Information of an AUSF NF Instance. |
| SupiRange | 6.1.6.2.9 | A range of SUPIs (subscriber identities), either based on a numeric range, or based on regular-expression matching. |
| IdentityRange | 6.1.6.2.10 | A range of subscriber identities, either based on a numeric range, or based on regular-expression matching. |
| AmfInfo | 6.1.6.2.11 | Information of an AMF NF Instance. |
| SmfInfo | 6.1.6.2.12 | Information of an SMF NF Instance. |
| UpfInfo | 6.1.6.2.13 | Information of an UPF NF Instance. |
| SnssaiUpfInfoItem | 6.1.6.2.14 | Set of parameters supported by UPF for a given S-NSSAI. |
| DnnUpfInfoItem | 6.1.6.2.15 | Set of parameters supported by UPF for a given DNN. |
| SubscriptionData | 6.1.6.2.16 | Information of a subscription to notifications to NRF events, included in subscription requests and responses. |
| NotificationData | 6.1.6.2.17 | Data sent in notifications from NRF to subscribed NF Instances. |
| NFServiceVersion | 6.1.6.2.19 | Contains the version details of an NF service. |
| PcfInfo | 6.1.6.2.20 | Information of a PCF NF Instance. |
| BsfInfo | 6.1.6.2.21 | Information of a BSF NF Instance. |
| Ipv4AddressRange | 6.1.6.2.22 | Range of IPv4 addresses. |
| Ipv6PrefixRange | 6.1.6.2.23 | Range of IPv6 prefixes. |
| InterfaceUpfInfoItem | 6.1.6.2.24 | Information of a given IP interface of an UPF. |
| UriList | 6.1.6.2.25 | Set of URIs following 3GPP hypermedia format (containing a "\_links" attribute). |
| N2InterfaceAmfInfo | 6.1.6.2.26 | AMF N2 interface information |
| TaiRange | 6.1.6.2.27 | Range of TAIs (Tracking Area Identities). |
| TacRange | 6.1.6.2.28 | Range of TACs (Tracking Area Codes). |
| SnssaiSmfInfoItem | 6.1.6.2.29 | Set of parameters supported by SMF for a given S-NSSAI. |
| DnnSmfInfoItem | 6.1.6.2.30 | Set of parameters supported by SMF for a given DNN. |
| NrfInfo | 6.1.6.2.31 | Information of an NRF NF Instance, used in hierarchical NRF deployments. |
| ChfInfo | 6.1.6.2.32 | Information of a CHF NF Instance. |
| PlmnRange | 6.1.6.2.34 | Range of PLMN IDs. |
| SubscrCond | 6.1.6.2.35 | Condition to determine the set of NFs to monitor under a certain subscription in NRF. |
| NfInstanceIdCond | 6.1.6.2.36 | Subscription to a given NF Instance Id. |
| NfTypeCond | 6.1.6.2.37 | Subscription to a set of NFs based on their NF Type. |
| ServiceNameCond | 6.1.6.2.38 | Subscription to a set of NFs based on their support for a given Service Name. |
| AmfCond | 6.1.6.2.39 | Subscription to a set of AMFs, based on AMF Set Id and/or AMF Region Id. |
| GuamiListCond | 6.1.6.2.40 | Subscription to a set of AMFs, based on their GUAMIs. |
| NetworkSliceCond | 6.1.6.2.41 | Subscription to a set of NFs, based on the slices (S-NSSAI and NSI) they support . |
| NfGroupCond | 6.1.6.2.42 | Subscription to a set of NFs based on their Group Id. |
| NotifCondition | 6.1.6.2.43 | Condition (list of attributes in the NF Profile) to determine whether a notification must be sent by NRF. |
| PlmnSnssai | 6.1.6.2.44 | List of network slices (S-NSSAIs) for a given PLMN ID. |
| NwdafInfo | 6.1.6.2.45 | Information of a NWDAF NF Instance. |
| LmfInfo | 6.1.6.2.46 | Information of an LMF NF Instance. |
| GmlcInfo | 6.1.6.2.47 | Information of a GMLC NF Instance. |
| NefInfo | 6.1.6.2.48 | Information of an NEF NF Instance. |
| PfdData | 6.1.6.2.49 | List of Application IDs and/or AF IDs managed by a given NEF Instance. |
| AfEventExposureData | 6.1.6.2.50 | AF Event Exposure data managed by a given NEF Instance. |
| WAgfInfo | 6.1.6.2.51 | Information of the W-AGF endpoints. |
| TngfInfo | 6.1.6.2.52 | Information of the TNGF endpoints. |
| PcscfInfo | 6.1.6.2.53 | Information of a P-CSCF NF Instance. |
| NfSetCond | 6.1.6.2.54 | Subscription to a set of NFs based on their Set Id. |
| NfServiceSetCond | 6.1.6.2.55 | Subscription to a set of NFs based on their Service Set Id. |
| NfInfo | 6.1.6.2.56 | Information of a generic NF Instance. |
| HssInfo | 6.1.6.2.57 | Information of an HSS NF Instance. |
| ImsiRange | 6.1.6.2.58 | A range of IMSIs (subscriber identities), either based on a numeric range, or based on regular-expression matching. |
| InternalGroupIdRange | 6.1.6.2.59 | A range of Group IDs (internal group identities), either based on a numeric range, or based on regular-expression matching. |
| UpfCond | 6.1.6.2.60 | Subscription to a set of NF Instances (UPFs), able to serve a certain service area (i.e. SMF serving area or TAI list). |
| TwifInfo | 6.1.6.2.61 | Addressing information (IP addresses, FQDN) of the TWIF. |
| VendorSpecificFeature | 6.1.6.2.62 | Information about a vendor-specific feature |
| UdsfInfo | 6.1.6.2.63 | Information related to UDSF |
| ScpInfo | 6.1.6.2.65 | Information of an SCP Instance |
| ScpDomainInfo | 6.1.6.2.66 | SCP domain information |
| ScpDomainCond | 6.1.6.2.67 | Subscription to an SCP domain  |
| OptionsResponse | 6.1.6.2.68 | Communication options of the NRF |
| NwdafCond | 6.1.6.2.69 | Subscription to a set of NF Instances (NWDAFs), identified by Analytics ID(s), S-NSSAI(s) or NWDAF Serving Area information, i.e. list of TAIs for which the NWDAF can provide analytics. |
| NefCond | 6.1.6.2.70 | Subscription to a set of NF Instances (NEFs), identified by Event ID(s) provided by AF, S-NSSAI(s), AF Instance ID, Application Identifier, External Identifier, External Group Identifier, or domain name. |
| SuciInfo | 6.1.6.2.71 | SUCI information containing Routing Indicator and Home Network Public Key ID. |
| SeppInfo | 6.1.6.2.72 | Information of a SEPP Instance |
| AanfInfo | 6.1.6.2.73 | Information of an AAnF NF Instance. |
| 5GDdnmfInfo | 6.1.6.2.74 | Information of a 5G DDNMF NF Instance. |
| MfafInfo | 6.1.6.2.75 | Information of the MFAF NF Instance. |
| NwdafCapability | 6.1.6.2.76 | Indicates the capability supported by the NWDAF. |
| DccfInfo | 6.1.6.2.80 | Information of a DCCF NF Instance. |
| NsacfInfo | 6.1.6.2.81 | Information of an NSACF NF Instance. |
| NsacfCapability | 6.1.6.2.82 | NSACF service capability. |
| DccfCond | 6.1.6.2.83 | Subscription to a set of NF Instances (DCCFs), identified by NF types, NF Set Id(s) or DCCF Serving Area information, i.e. list of TAIs served by the DCCF. |
| MlAnalyticsInfo | 6.1.6.2.84 | ML Analytics Filter information supported by the Nnwdaf\_MLModelProvision service |
| MbSmfInfo | 6.1.6.2.85 | Information of a MB-SMF NF Instance |
| TmgiRange | 6.1.6.2.86 | Range of TMGIs |
| MbsSession | 6.1.6.2.87 | MBS Session served by an MB-SMF |
| SnssaiMbSmfInfoItem | 6.1.6.2.88 | Parameters supported by an MB-SMF for a given S-NSSAI |
| DnnMbSmfInfoItem | 6.1.6.2.89 | Parameters supported by an MB-SMF for a given DNN |
| TsctsfInfo | 6.1.6.2.91 | Information of a TSCTSF NF Instance. |
| SnssaiTsctsfInfoItem | 6.1.6.2.92 | Set of parameters supported by TSCTSF for a given S-NSSAI. |
| DnnTsctsfInfoItem | 6.1.6.2.93 | Set of parameters supported by TSCTSF for a given DNN. |
| MbUpfInfo | 6.1.6.2.94 | Information of a MB-UPF NF Instance. |
| UnTrustAfInfo | 6.1.6.2.95 | Information of a untrusted AF Instance. |
| TrustAfInfo | 6.1.6.2.96 | Information of a trusted AF Instance |
| SnssaiInfoItem | 6.1.6.2.97 | Set of parameters supported by NF for a given S-NSSAI. |
| DnnInfoItem | 6.1.6.2.98 | Set of parameters supported by NF for a given DNN. |
| CollocatedNfInstance | 6.1.6.2.99 | Information related to collocated NF type(s) and corresponding NF Instance(s) when the NF is collocated with NFs supporting other NF types. |
| ServiceNameListCond | 6.1.6.2.100 | Subscription to a set of NF Instances that offer a service name in the Service Name list. |
| NfGroupListCond | 6.1.6.2.101 | Subscription to a set of NF Instances, identified by a NF Group Identity in the NF Group Identity list. |
| PlmnOauth2 | 6.1.6.2.102 | Per PLMN Oauth2.0 indication. |
| V2xCapability | 6.1.6.2.103 | Indicate the supported V2X Capability by the PCF. |
| NssaafInfo | 6.1.6.2.104 | Information of a NSSAAF NF Instance. |
| ProSeCapability | 6.1.6.2.105 | Indicate the supported ProSe Capability by the PCF. |
| SharedDataIdRange | 6.1.6.2.106 |  |
| SubscriptionContext | 6.1.6.2.107 | Context data related to a created subscription, to be included in notifications sent by NRF. |
| IwmscInfo | 6.1.6.2.108 | Information of a SMS-IWMSC NF Instance. |
| MnpfInfo | 6.1.6.2.109 | Information of an MNPF Instance. |
| DefSubServiceInfo | 6.1.6.2.x | Service Specific Information for Default Notification Subscription. |
| NefId | 6.1.6.3.2 | Identity of the NEF. |
| VendorId | 6.1.6.3.2 | Vendor ID of the NF Service instance (Private Enterprise Number assigned by IANA) |
| WildcardDnai | 6.1.6.3.2 | Wildcard DNAI |
| NFType | 6.1.6.3.3 | NF types known to NRF. |
| NotificationType | 6.1.6.3.4 | Types of notifications used in Default Notification URIs in the NF Profile of an NF Instance. |
| TransportProtocol | 6.1.6.3.5 | Types of transport protocol used in a given IP endpoint of an NF Service Instance. |
| NotificationEventType | 6.1.6.3.6 | Types of events sent in notifications from NRF to subscribed NF Instances. |
| NFStatus | 6.1.6.3.7 | Status of a given NF Instance stored in NRF. |
| DataSetId | 6.1.6.3.8 | Types of data sets stored in UDR. |
| UPInterfaceType | 6.1.6.3.9 | Types of User-Plane interfaces of the UPF. |
| ServiceName | 6.1.6.3.11 | Service names known to NRF. |
| NFServiceStatus | 6.1.6.3.12 | Status of a given NF Service Instance of an NF Instance stored in NRF. |
| AnNodeType | 6.1.6.3.13 | Access Network Node Type (gNB, ng-eNB...). |
| ConditionEventType | 6.1.6.3.14 | Indicates whether a notification is due to the NF Instance to start or stop being part of a condition for a subscription to a set of NFs |
| IpReachability | 6.1.6.3.15 | Indicates the type(s) of IP addresses reachable via an SCP. |
| CollocatedNfType | 6.1.6.3.17 | Possible NF types supported by a collocated NF. |

Editor's Note: A general solution of NRF handling towards absent attributes (not registered by the NF or not supported by NF with early version) is FFS.

Table 6.1.6.1-2 specifies data types re-used by the Nnrf\_NFManagement service-based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nnrf\_NFManagement service-based interface.

Table 6.1.6.1-2: Nnrf\_NFManagement re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| N1MessageClass | 3GPP TS 29.518 [6] | The N1 message type |
| N2InformationClass | 3GPP TS 29.518 [6] | The N2 information type |
| IPv4Addr | 3GPP TS 29.571 [7] |  |
| IPv6Addr | 3GPP TS 29.571 [7] |  |
| IPv6Prefix | 3GPP TS 29.571 [7] |  |
| Uri | 3GPP TS 29.571 [7] |  |
| Dnn | 3GPP TS 29.571 [7] |  |
| SupportedFeatures | 3GPP TS 29.571 [7] |  |
| Snssai | 3GPP TS 29.571 [7] |  |
| PlmnId | 3GPP TS 29.571 [7] |  |
| Guami | 3GPP TS 29.571 [7] |  |
| Tai | 3GPP TS 29.571 [7] |  |
| NfInstanceId | 3GPP TS 29.571 [7] |  |
| LinksValueSchema | 3GPP TS 29.571 [7] | 3GPP Hypermedia link |
| UriScheme | 3GPP TS 29.571 [7] |  |
| AmfName | 3GPP TS 29.571 [7] |  |
| DateTime | 3GPP TS 29.571 [7] |  |
| Dnai | 3GPP TS 29.571 [7] |  |
| ChangeItem | 3GPP TS 29.571 [7] |  |
| DiameterIdentity | 3GPP TS 29.571 [7] |  |
| AccessType | 3GPP TS 29.571 [7] |  |
| NfGroupId | 3GPP TS 29.571 [7] | Network Function Group Id |
| AmfRegionId | 3GPP TS 29.571 [7] |  |
| AmfSetId | 3GPP TS 29.571 [7] |  |
| PduSessionType | 3GPP TS 29.571 [7] |  |
| AtsssCapability | 3GPP TS 29.571 [7] | Capability to support procedures related to Access Traffic Steering, Switching, Splitting. |
| Nid | 3GPP TS 29.571 [7] |  |
| PlmnIdNid | 3GPP TS 29.571 [7] |  |
| NfSetId | 3GPP TS 29.571 [7] | NF Set ID (see clause 28.12 of 3GPP TS 23.003 [12]) |
| NfServiceSetId | 3GPP TS 29.571 [7] | NF Service Set ID (see clause 28.13 of 3GPP TS 23.003 [12]) |
| GroupId | 3GPP TS 29.571 [7] | Internal Group Identifier |
| RatType | 3GPP TS 29.571 [7] | RAT Type |
| DurationSec | 3GPP TS 29.571 [7] |  |
| RedirectResponse | 3GPP TS 29.571 [7] | Response body of the redirect response message. |
| ExtSnssai | 3GPP TS 29.571 [7] |  |
| AreaSessionId | 3GPP TS 29.571 [7] | Area Session Identifier used for an MBS session with location dependent content |
| MbsSessionId | 3GPP TS 29.571 [7] | MBS Session Identifier |
| MbsServiceArea | 3GPP TS 29.571 [7] | MBS Service Area |
| IpAddr | 3GPP TS 29.571 [7] | IP Address |
| MbsServiceAreaInfo | 3GPP TS 29.571 [7] | MBS Service Area Information for Location dependent MBS session |
| Fqdn | 3GPP TS 29.571 [7] | Fully Qualified Domain Name |
| EventId | 3GPP TS 29.520 [32] | Defined in Nnwdaf\_AnalyticsInfo API. |
| NwdafEvent | 3GPP TS 29.520 [32] | Defined in Nnwdaf\_EventsSubscription API. |
| ExternalClientType | 3GPP TS 29.572 [33] |  |
| LMFIdentification | 3GPP TS 29.572 [33] | LMF Identification |
| AfEvent | 3GPP TS 29.517 [35] | Defined in Naf\_EventExposure API |
| SupportedGADShapes | 3GPP TS 29.572 [33] | Supported GAD Shapes |
| NetworkNodeDiameterAddress | 3GPP TS 29.503 [36] | Diameter Address of a Network Node |

\* \* \* Next Change \* \* \* \*

##### 6.1.6.2.4 Type: DefaultNotificationSubscription

Table 6.1.6.2.4-1: Definition of type DefaultNotificationSubscription

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| notificationType | NotificationType | M | 1 | Type of notification for which the corresponding callback URI is provided. |
| callbackUri | Uri | M | 1 | This attribute contains a default notification endpoint to be used by a NF Service Producer towards an NF Service Consumer that has not registered explicitly a callback URI in the NF Service Producer (e.g. as a result of an implicit subscription). |
| n1MessageClass | N1MessageClass | C | 0..1 | If the notification type is N1\_MESSAGES, this IE shall be present and shall identify the class of N1 messages to be notified.  |
| n2InformationClass | N2InformationClass | C | 0..1 | If the notification type is N2\_INFORMATION, this IE shall be present and shall identify the class of N2 information to be notified.  |
| versions | array(string) | O | 1..N | API versions (e.g. "v1") supported for the default notification type. (NOTE x) |
| binding | string | O | 0..1 | When present, this IE shall contain the value of the Binding Indication for the default subscription notification (i.e. the value part of "3gpp-Sbi-Binding" header), as specified in clause 6.12.4 of 3GPP TS 29.500 [4]. (NOTE 1) |
| acceptedEncoding | string | O | 0..1 | Content encodings that are accepted by a NF Service Consumer when receiving a notification related to a default notification subscription.The value of this attribute shall be formatted as the value of the Accept-Encoding header defined in IETF RFC 7231 [40] clause 5.3.4 (e.g. acceptedEncoding: "gzip;q=1.0, identity;q=0.5, \*;q=0")The absence of this IE shall not be interpreted as indicating that no specific encodings isare supported, but the NF Service Consumer did not register the encodings it may support. |
| supportedFeatures | SupportedFeatures | O | 0..1 | When present, this attribute shall indicate the features of the service corresponding to the subscribed default notification, which are supported by the NF (Service) instance acting as NF service consumer. (NOTE 2, NOTE x) |
| serviceInfoList | map(DefSubServiceInfo) | O | 1..N | This IE may be present when the notification request of the notification type may be generated by multiple services, i.e. notifications from different services may be received by the subscription.When present, this IE shall contain a map of service specific information. The name of the corresponding service (as specified in ServiceName data type, see clause 6.1.6.3.11) is the key of the map and the value of the map is the specific information for the indicated service supported by the NF (Service) instance acting as NF service consumer.For example, when the NF subscribes to default notification of "LOCATION\_NOTIFICATION" type which may be sent by Namf\_Location service and Nlmf\_Location service, the NF may provide service specific information as below:{ "namf-loc" : { "versions" : [ "v1" ], "supportedFeatures" : "AB"  }, "nlmf-loc" : { "versions" : [ "v1" ], "supportedFeatures" : "12"  }} (NOTE x, NOTE y) |
| NOTE 1: The binding indication for default subscription may be used by a NF service producer to reselect an alternative NF service consumer instance, when delivering a notification for a default subscription towards a specific NF consumer but the latter is not reachable. E.g. an AMF notifies corresponding uplink LPP/NRPPa messages via default subscription, to the LMF instance who previously sent downlink LPP/NRPPa message during a location procedure, If the original LMF instance is not reachable, the AMF selects an alternative LMF instance using the binding indication and delivers the notification towards the selected LMF instance.NOTE 2: When sending notifications towards the subscribed NF service consumer, the NF service producer shall generate the default notifications according to the supported features indicated in this attribute, e.g. to include the attributes or enumerated values related to particular features only if the corresponding features are supported, as specified in clause 6.6.2 of 3GPP TS 29.500 [4].NOTE x: When the serviceInfoList IE is present, the versions IE and the supportedFeatures IE shall be absent.NOTE y: When the serviceInfoList IE is present, the NF producer shall determine whether the service of the default notification is supported, i.e. whether the service is listed in the map keys. If supported, the NF producer shall generate the default notification according to the specific information of the service, i.e. the corresponding map value. |

\* \* \* Next Change \* \* \* \*

##### 6.1.6.2.x Type: DefSubServiceInfo

Table 6.1.6.2.x-1: Definition of type DefSubServiceInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| versions | array(string) | O | 1..N | When present, this attribute shall indicate the API version (e.g. "v1") of the indicated service which are supported by the NF (Service) instance acting as NF service consumer. |
| supportedFeatures | SupportedFeatures | O | 0..1 | When present, this attribute shall indicate the features of the indicated service which are supported by the NF (Service) instance acting as NF service consumer. |

\* \* \* Next Change \* \* \* \*

# A.2 Nnrf\_NFManagement API

openapi: 3.0.0

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Text Skipped for Clarity \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

 DefaultNotificationSubscription:

 description: >

 Data structure for specifying the notifications the NF service subscribes by default,

 along with callback URI

 type: object

 required:

 - notificationType

 - callbackUri

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 callbackUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 n1MessageClass:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N1MessageClass'

 n2InformationClass:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InformationClass'

 versions:

 type: array

 items:

 type: string

 minItems: 1

 binding:

 type: string

 acceptedEncoding:

 type: string

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 serviceInfoList:

 description: >

 A map of service specific information. The name of the corresponding service (as

 specified in ServiceName data type) is the key.

 type: object

 additionalProperties:

 $ref: '#/components/schemas/DefSubServiceInfo'

 minProperties: 1

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Text Skipped for Clarity \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

 MnpfInfo:

 description: Information of an MNPF Instance

 type: object

 properties:

 msisdnRanges:

 type: array

 items:

 $ref: '#/components/schemas/IdentityRange'

 minItems: 1

 required:

 - msisdnRanges

 DefSubServiceInfo:

 description: Service Specific information for Default Notification Subscription.

 type: object

 properties:

 versions:

 type: array

 items:

 type: string

 minItems: 1

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

\* \* \* End of Changes \* \* \* \*