**3GPP TSG-CT4 Meeting #97e *C4-202088***

**E-Meeting, 15th – 24th April 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **29.544** | **CR** | **0001** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification on Secured Packet format provided by SP-AF |
|  |  |
| ***Source to WG:*** | THALES |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5GS\_OTAF |  | ***Date:*** | 2020-04-02 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The clause 7.1.1.1a in TS 31.111 describes the procedure between the ME and the USIM to support SoR and Routing ID update. This clause states that the ME shall receive a secure packet constructed as an SMS-Deliver as specified in 3GPP TS 23.040. This secured packet shall be constructed by the SP-AF. But in current version of TS 29.544, there is no reference to TS 23.040, there is only a reference to TS 31.115. And TS 31.115 just describes a subpart of SMS-Deliver element as specified in TS 23.040. |
|  |  |
| ***Summary of change:*** | Specify that the secured packet provided by the SP-AF shall be constructed as an SMS-Deliver as specified in 3GPP TS 23.040. |
|  |  |
| ***Consequences if not approved:*** | The USIM cannot perform SoR or Routing ID update  |
|  |  |
| ***Clauses affected:*** | 2; 6.1.3.2.4.2.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not make any changes to the OpenAPI  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* First Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 7807: "Problem Details for HTTP APIs".

[14] 3GPP TS 29.503: "Unified Data Management Services".

[15] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces Stage 3".

[16] 3GPP TS 31.115: "Secured packet structure for (Universal) Subscriber Identity Module (U)SIM Toolkit applications".

[17] 3GPP TS 29.509: "Authentication Server Services; Stage 3".

[xx] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)"

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Next Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

6.1.3.2.4.2.1 Description

This custom operation is used by the NF service consumer (e.g. UDM) to request a secured packet for the SUPI containing the presented UICC configuration parameter. The secure packet shall be constructed as an SMS-Deliver as specified in 3GPP TS 23.040 [xx] and protected as specified in 3GPP TS 31.115 [16].

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*