**3GPP TSG-CT WG4 Meeting #99eC4-204abc**

**E-Meeting, 18th – 28th April 2020 *was* C4-204289**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **23.003** | **CR** | **0596** | **rev** | **1** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction on Truncated 5G-S-TMSI |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT4 |
|  |  |
| ***Work item code:*** | 5G\_CIoT |  | ***Date:*** | 2020-08-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Keep in line with stage 2 TS23.501, In current solution in stage 2, the Truncated 5G-S-TMSI Configuration to UE will be configured by AMF, not by RAN any more, see TS 23.501 clause 5.31.4.3, and in addition there is a note as below in TS 23.501 clause 5.31.4.3*NOTE: Network sharing default configuration of the sizes of the truncated components is described in TS 23.003 [19].*How to cofigure the sizes of the truncated components should be added in 23.003. |
|  |  |
| ***Summary of change:*** | 1. Correct the way of Truncated 5G-S-TMSI Configuration to UE.
2. Add the text to describe how to configure and distribute m and n in network sharing scenario.
 |
|  |  |
| ***Consequences if not approved:*** | Misalignment with stage 2. |
|  |  |
| ***Clauses affected:*** | 2.12 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev1：1. Corrected reference typos on cover page
2. Added "3GPP" before reference TS 24.501 in new text in clause 2.12.
 |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The start of changes\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 2.12 Structure of the Truncated 5G-S-Temporary Mobile Subscriber Identity (Truncated 5G-S-TMSI)

The Truncated 5G-S-TMSI is a 40 bit UE identifier constructed from the 5G-S-TMSI. It is used in RRC Connection Re-Establishment for the control plane for NB-IoT as described in 3GPP TS 36.300 [91]. The Truncated 5G-S-TMSI shall be constructed from the Truncated AMF set ID, the Truncated AMF Pointer and the Truncated 5G-TMSI:

<Truncated 5G-S-TMSI> = <Truncated AMF set ID><Truncated AMF Pointer><Truncated 5G-TMSI>

Truncated AMF set ID is n least significant bits of AMF Set ID, where n is no greater than 10 bits.

Truncated AMF Pointer is m least significant bits of AMF Pointer, where m is no greater than 6 bits.

Truncated 5G-TMSI is (40-n-m) least significant bits of 5G-TMSI.

The values n and m are configurable based on network deployment. The value n+m shall be larger or equal to 8 bits.

NOTE: Depending on network deployment it is up to operator configuration to ensure that Truncated AMF Set ID and Truncated AMF Pointer identify the AMF uniquely, and that Truncated 5G-TMSI identifies the UE uniquely within the serving AMF.

The NG-RAN and AMF are configured with the values n and m respectively, and NG-RAN is configured with how to recreate AMF Set ID from Truncated AMF Set ID, AMF Pointer from Truncated AMF Pointer, and 5G-TMSI from Truncated 5G-TMSI. The configuration of these parameters are specific to each PLMN.

The AMF configures the UE with the Truncated 5G-S-TMSI Configuration that provides the sizes of the components of the Truncated 5G-S-TMSI as described in 3GPP TS 24.501 [125] during the Registration and UE Configuration Update procedures.

For Network Sharing, the sharing NG-RAN is configured with the respective values n and m that are specific to each PLMN, and AMF is configured with the same values n and m as ones configured on NG-RAN per PLMN. The AMF configures the UE with the corresponding values n and m according to the PLMN which the UE accesses to during the Registration procedure.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*The end of changes\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*