**3GPP TSG-CT WG1 Meeting #123-eC1-20xxxx**

**Electronic meeting, 16-24 April 2020**

**Title:** ReplyLS on Manual CAG ID selection and granularity of UAC parameters for PNI-NPNs

**Response to:** R2-2002417

**Release:** Release 16

**Work Item:** Vertical\_LAN

**Source:** TSG CT WG1

**To:** RAN2

**Cc:** RAN3, SA1, SA2

**Contact Person:**

#### Name: Vishnu Preman

E-mail Address: vishnu(dot)preman(at)huawei(dot)com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** -

**1. Overall Description:**

CT1 would like to thank RAN2 for the questions for clarification on the manual CAG selection.

As CT1 is responsible for the stage 2 work for NAS IDLE mode procedures, including manual CAG selection and the network selection, CT1 thinks that it will be appropriate for CT1 to reply to Questions1.2.

**Question 1.2; TO: SA2; CC: CT1**Shall a UE prioritize for cell reselection the cells supporting the manually selected CAG ID over other suitable cells that do not support the manually selected CAG ID after a successful registration?

* **Answer 1.2**: *No.*

**Question 1.3; TO: CT1:**It is RAN2 understanding that the UE NAS provide the manually selected CAG ID to UE AS. Is the manually selected CAG ID provided as part of the allowed CAG list, or as a separate element?

* **Answer 1.3**: *Manually selected CAG ID will be provided as a separate element.*

**Question 2.2; TO: CT1, SA1:**If there is a requirement to enable PNI-NPN (CAG ID) specific access control in cells that are shared among PNI-NPNs belonging to the same PLMN, then is it sufficient to broadcast the Unified Access Control (UAC) parameters per PLMN (assuming that using the operator-defined access categories with access category criteria type set to the S-NSSAI used for PNI-NPN is sufficient to provide CAG specific UAC) or there is need to enable the broadcast of CAG ID specific configuration of UAC parameters?

* **Answer 2.2;** *As this question is dependent on service requirements which do not exist yet, this question can be answered only if and when the service requirements are specified by SA1.*

**2. Actions:**

**To RAN2 group.**

**ACTION:** CT1 respectfully asks RAN2 to take the above answers into consideration.

**3. Date of Next TSG-CT WG1 Meetings:**

3GPP CT1#124 25 – 30 May 2020 electronic