**3GPP TSG-CT WG1 Meeting #123-eC1-202xxx**

**E-Meeting, 24-28 February 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **24.519** | **CR** | **0001** | **rev** | **1** | **Current version:** | **16.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction of the abnormal case in NW-TT-initiated Ethernet port management procedure |
|  |  |
| ***Source to WG:*** | vivo |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | Vertical\_LAN |  | ***Date:*** | 2020-04-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In the NW-TT-initiated Ethernet port management procedure, the NW-TT will not sent ETHERNET PORT MANAGEMENT NOTIFY COMPLETE message, therefore the abnormal case of bullet b) in 6.2.2.5, i.e, the transmission failure of the ETHERNET PORT MANAGEMENT NOTIFY COMPLETE message will not happen, the corresponding abnormal case handling is not needed. |
|  |  |
| ***Summary of change:*** | It is proposed to delete the bullet b) in 6.2.2.5. |
|  |  |
| ***Consequences if not approved:*** | The abnormal case of bullet b) in 6.2.2.5 is incorrect. |
|  |  |
| ***Clauses affected:*** | 6.2.2.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First change \*\*\*

6.2.2.5 Abnormal cases in the NW-TT

The following abnormal cases can be identified:

a) T35zz expired.

 The NW-TT shall, on the first expiry of the timer T35zz, retransmit the ETHERNET PORT MANAGEMENT NOTIFY message and shall reset and start timer T35zz. This retransmission is repeated four times, i.e. on the fifth expiry of timer T35zz, the NW-TT shall abort the procedure.

\*\*\* End of changes \*\*\*