**3GPP TSG-CT WG1 Meeting #133-bis-eC1-220059**

**E-meeting, 17-21 January 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.501** | **CR** | **3841** | **rev** | **1** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification of including Service-level-AA container in PDU SESSION MODIFICATION REQUEST message |
|  |  |
| ***Source to WG:*** | SHARP |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | ID\_UAS |  | ***Date:*** | 2022-01-07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)...Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In clause 6.4.2.2 of current TS 24.501, it is described as follows:*The UE shall include the Service-level-AA container IE in the PDU SESSION MODIFICATION REQUEST message, when requesting to modify an established PDU session for C2 communication.*However, in clause 8.3.7.1, the above content is not reflected at table 8.3.7.1.1. |
|  |  |
| ***Summary of change:*** | Add a row of Service-level-AA container IE in PDU session modification request message content. |
|  |  |
| ***Consequences if not approved:*** | The specification has an inconsistency. |
|  |  |
| ***Clauses affected:*** | 8.3.7.1, 8.3.7.x (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\* 1st change \*\*\*\*\*

#### 8.3.7.1 Message definition

The PDU SESSION MODIFICATION REQUEST message is sent by the UE to the SMF to request a modification of a PDU session. See table 8.3.7.1.1.

Message type: PDU SESSION MODIFICATION REQUEST

Significance: dual

Direction: UE to network

Table 8.3.7.1.1: PDU SESSION MODIFICATION REQUEST message content

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| IEI | Information Element | Type/Reference | Presence | Format | Length |
|  | Extended protocol discriminator | Extended protocol discriminator9.2 | M | V | 1 |
|  | PDU session ID | PDU session identity9.4 | M | V | 1 |
|  | PTI | Procedure transaction identity9.6 | M | V | 1 |
|  | PDU SESSION MODIFICATION REQUEST message identity | Message type9.7 | M | V | 1 |
| 28 | 5GSM capability | 5GSM capability9.11.4.1 | O | TLV | 3-15 |
| 59 | 5GSM cause | 5GSM cause9.11.4.2 | O | TV | 2 |
| 55 | Maximum number of supported packet filters | Maximum number of supported packet filters9.11.4.9 | O | TV | 3 |
| B- | Always-on PDU session requested | Always-on PDU session requested9.11.4.4 | O | TV | 1 |
| 13 | Integrity protection maximum data rate | Integrity protection maximum data rate9.11.4.7 | O | TV | 3 |
| 7A | Requested QoS rules | QoS rules9.11.4.13 | O | TLV-E | 7-65538 |
| 79 | Requested QoS flow descriptions | QoS flow descriptions9.11.4.12 | O | TLV-E | 6-65538 |
| 75 | Mapped EPS bearer contexts | Mapped EPS bearer contexts9.11.4.8 | O | TLV-E | 7-65538 |
| 7B | Extended protocol configuration options | Extended protocol configuration options9.11.4.6 | O | TLV-E | 4-65538 |
| 74 | Port management information container | Port management information container9.11.4.27 | O | TLV-E | 4-65538 |
| 66 | IP header compression configuration | Header compression configuration9.11.4.24 | O | TLV | 5-257 |
| 1F | Ethernet header compression configuration | Ethernet header compression configuration9.11.4.28 | O | TLV | 3 |
| 23 | Requested MBS container | Requested MBS container9.11.4.30 | O | TLV | 7-n |
| 7C | Service-level-AA container | Service-level-AA container9.11.2.10 | O | TLV-E | 6-n |

NOTE: It is possible for UEs compliant with version 15.2.1 or earlier versions of this specification to send the Mapped EPS bearer contexts IE with IEI of value "7F" for this message.

Editor's note: The maximum length of the Requested MBS container IE is FFS.

\*\*\*\*\* 2nd change \*\*\*\*\*

#### 8.3.7.x Service-level-AA container

This IE shall be included in the message when the UE needs to modify an established PDU session for C2 communication.

\*\*\*\*\* end of change \*\*\*\*\*