**3GPP TSG-CT WG1 Meeting #134-eC1-221092-r1**

**E-Meeting, 17th – 25th February 2022**

**Source: Huawei, HiSilicon**

**Title: Minor corrections on Message Type**

**Spec: 3GPP TS 24.538**

**Agenda item: 17.2.30**

**Document for: Approval**

**1. Introduction**

This pCR is to correct some typos in clause 7.1.

**2. Reason for Change**

Types need to be corrected.

**3. Conclusions**

<Conclusion part (optional)>

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 24.538 v0.3.0.

\* \* \* First Change \* \* \* \*

## 7.1 General

This clause contains the information elements coding for the messages used in the procedures described in the present document.

In order to identify the usage of messages, in addition to the information elements specified in 3GPP TS 23.554 [2], a "Message Type" element shall be added to each message. The possible values of "Message Type" element are listed below:

a) "CONF" refers to Configuration;

b) "REG" refers to Registration;

c) "DEREG" refers to de-registration;

d) "TOPSUB" refers to Messaging Topic Subscription;

e) "MSG" refers to MSGin5G message;

f) "MSGRESP" refers to message response;

g) "IMDN" refers to MSGin5G delivery status report";

h) "SEGREC" refers to segments recovery; and

i) "SEGCONFIR" refers to message segments received confirmation.

\* \* \* End of Changes \* \* \* \*