**3GPP TSG-CT WG1 Meeting #136-eC1-223383**

**E-Meeting, 12th – 20th May 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **554** | **CR** |  | **rev** | **-** | **Current version:** | **.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update to configuration by application server | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | CATT | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_ProSe | | | | |  | ***Date:*** | | | 2022-05-05 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | As specified in TS 33.503, the PCF provisions the PC5 security policies to the 5G ProSe Remote UE and the UE-to-Network Relay respectively per 5G ProSe UE-to-Network Relay service.  The ProSe application server does not provision PC5 security policies to the UE. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clarify that security policies for 5G ProSe UE-to-network relay is not provisioned by the ProSe application server.  Remove the redundant description of "security related content" for 5G ProSe UE-to-network relay. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | How security policies for 5G ProSe UE-to-network relay is provisioned is unclear. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2.2, 5.2.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

### 5.2.2 Precedence of 5G ProSe configuration information

The 5G ProSe configuration information for 5G ProSe direct discovery, 5G ProSe direct communication, 5G ProSe UE-to-network relay and 5G ProSe usage reporting configuration and rules can be:

a) pre-configured in the ME;

b) configured in the UICC;

c) provided as a ProSeP by PCF;

d) provided by a ProSe application server via PC1 reference point except:

1) the authorization policy for 5G ProSe direct discovery and restricted ProSe discovery UE ID for restricted direct discovery in parameters for 5G ProSe direct discovery;

2) the authorization policy in parameters for 5G ProSe direct communication;

3) the following parameters for the role of a 5G ProSe UE-to-network relay UE:

i) authorization policy for acting as a 5G ProSe layer-3 and/or layer-2 UE-to-network relay when "served by NG-RAN";

ii) QoS mapping rules for 5G ProSe layer-3 ProSe UE-to-network relay; and

iii) a mapping of ProSe identifier(s) to ProSe application server address information for 5G ProSe layer-3 UE-to-network relay to relay Ethernet or Unstructured traffic from Remote UE by using IP type PDU session;

4) the following parameters for the role of a remote UE:

i) authorization policy for using a 5G ProSe layer-3 and/or layer-2 UE-to-network relay; and

5) the following parameters for the role of a 5G ProSe UE-to-network relay as well as for the role of a 5G ProSe remote UE:

i) radio parameters for 5G ProSe relay discovery when the UE is not "served by NG-RAN ";

ii) radio parameters for 5G ProSe relay communication when the UE is not "served by NG-RAN"; and

iii) security policies for 5G ProSe UE-to-network relay; or

e) a combination of case a), b), c) or d) above.

The UE should not request or accept any 5G ProSe configuration information from PCF when the UE is working as a remote UE using a 5G ProSe layer-3 ProSe UE-to-network relay without involving N3IWF.

The UE shall use the 5G ProSe configuration information in the following order of decreasing precedence:

a) the 5G ProSe configuration information provided as a ProSeP by PCF;

b) the 5G ProSe configuration information provided by a ProSe application server via PC1 reference point;

c) the 5G ProSe configuration information configured in the UICC; and

d) the 5G ProSe configuration information pre-configured in the ME.

\* \* \* Next Change \* \* \* \*

### 5.2.5 Configuration parameters for 5G ProSe UE-to-network relay

The configuration parameters for the role of a ProSe UE-to-network relay UE over PC5 reference point consist of:

a) a validity timer for the validity of the configuration parameter for 5G ProSe UE-to-network relay over PC5 interface;

b) a list of PLMNs in which the UE is authorised to relay traffic for 5G ProSe layer-3 remote UEs when the UE is served by NG-RAN, and in each PLMN;

c) a list of PLMNs in which the UE is authorised to relay traffic for 5G ProSe layer-2 remote UEs when the UE is served by NG-RAN, and in each PLMN;

d) the default destination layer-2 ID(s) for sending the discovery signalling for announcement and additional information, and for receiving the discovery signalling for solicitation;

NOTE 1: Which default destination layer-2 ID is selected is up to UE implementation when there are more than one default destination layer-2 ID.

e) a User info ID for the UE-to-network relay discovery;

f) one or more relay service code(s) for the UE-to-network relay discovery, and for each relay service code:

1) void;

2) an indication of whether the relay service code is offering 5G ProSe layer-2 or layer-3 UE-to-network relay service; and

3) for 5G ProSe layer-3 UE-to-network relay UE, a set of PDU session parameters:

i) PDU Session type;

ii) optionally, DNN;

iii) optionally, SSC Mode;

iv) optionally, S-NSSAI; and

v) optionally, access type preference;

4) for 5G ProSe layer-3 UE-to-network relay UE, security policies for UE-to-network relay direct communication:

i) the signalling integrity protection policy;

ii) the signalling ciphering policy;

iii) the user plane integrity protection policy; and

iv) the user plane ciphering policy;

g) for 5G ProSe layer-3 UE-to-network relay UE, QoS mapping rules including:

1) a mapping between a 5QI value and a 5G ProSe PQI value over PC5 for traffic relayed over the PC5 interface;

2) a PDB adjustment factor of the standardized PDB identified by the PQI; and

3) optionally, the relay service code(s) associated with the QoS mapping rule;

h) the radio parameters of the 5G ProSe UE-to-network relay discovery applicable per geographical area with an indication of whether these radio parameters are "operator managed" or "non-operator managed" when the UE is not served by NG-RAN;

i) for 5G ProSe layer-3 UE-to-network relay UE, for Ethernet and Unstructured traffic using IP type PDU session, a list of ProSe identifier(s) to ProSe application server address mapping rule. Each mapping rule contains one or more ProSe identifier(s) and IP address/FQDN and transport layer port number; and

j) the radio parameters of the 5G ProSe direct communication applicable per geographical area with an indication of whether these radio parameters are "operator managed" or "non-operator managed" when the UE is not served by NG-RAN; and

k) optionally, the ProSe key management function (PKMF) address.

The configuration parameters for the role of a 5G ProSe remote UE consist of:

a) a validity timer for the validity of the configuration parameters for 5G ProSe remote UE;

b) an indication whether the UE is authorized to use a 5G ProSe layer-3 UE-to-network relay UE;

c) a list of PLMNs in which the UE is authorized to use a 5G ProSe layer-2 UE-to-network relay UE;

d) default destination layer-2 ID(s) for sending the discovery signalling for solicitation, and for receiving the discovery signalling for announcement and additional information;

NOTE 2: Which default destination layer-2 ID is selected is up to UE implementation when there are more than one default destination layer-2 ID.

e) a User info ID for the UE-to-network relay discovery;

f) one or more relay service code(s) for the UE-to-network relay discovery, and for each relay service code:

1) void;

2) an indication of whether the relay service code is offering 5G ProSe layer-2 or layer-3 UE-to-network relay service; and

3) for 5G ProSe remote UE using 5G ProSe layer-3 UE-to-network relays, one of the following:

i) a set of PDU session parameters for the relayed traffic without using N3IWF access:

A) PDU Session type;

B) optionally, DNN;

C) optionally, SSC Mode;

D) optionally, S-NSSAI; and

E) optionally, access type preference; or

ii) an indication of using N3IWF access for the relayed traffic;

4) for 5G ProSe remote UE using 5G ProSe layer-3 UE-to-network relays, security policies for UE-to-network relay direct communication:

i) the signalling integrity protection policy;

ii) the signalling ciphering policy;

iii) the user plane integrity protection policy; and

iv) the user plane ciphering policy;

g) the radio parameters of the 5G ProSe Relay Discovery applicable per geographical area with an indication of whether these radio parameters are "operator managed" or "non-operator managed" when the UE is not served by NG-RAN;

h) the radio parameters of the 5G ProSe direct communication applicable per geographical area with an indication of whether these radio parameters are "operator managed" or "non-operator managed" when the UE is not served by NG-RAN;

NOTE 3: Whether a frequency band is "operator managed" or "non-operator managed" in a given Geographical Area is defined by local regulations.

i) the N3IWF selection information for 5G ProSe layer-3 remote UE:

1) N3IWF identifier configuration (either FQDN or IP address); and

2) 5G ProSe layer-3 UE-to-network relays, access node selection information consists of a prioritized list of PLMNs for N3IWF selection and an indication that the selection of an N3IWF in a PLMN should be based on Tracking Area Identity FQDN or on Operator Identifier FQDN; and

j) optionally, the PKMF address.

\* \* \* End of Changes \* \* \* \*