**3GPP TSG-CT WG1 Meeting #136-eC1-223424**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **24.379** | **CR** | **0808** | **rev** | **-** | **Current version:** | **14.14.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections to private call without floor control using pre-established session |
|  |  |
| ***Source to WG:*** | Samsung, FirstNet |
| ***Source to TSG:*** | C1 |
|  |  |
| ***Work item code:*** | MCImp-eMCPTT-CT |  | ***Date:*** | 05-05-2022 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | *Rel-14* |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The condition to determine a private call or first-to-answer without floor control on receipt of a "SIP REFER request for a pre-established session" is erroneously checking in the recieved SDP offer not including a media-level section for media plane control messages with the 'fmtp' attribute containing a value of "mc\_no\_floor\_ctrl" as specified in 3GPP TS 24.380 [5] clause 14. This erroneous check results into condition failure and the participating function will fail to initiate call further. Background: During #133-e meeting, a set of CRs (C1-217319 & its siblings) are proposed to fix non availability of the media control channel for transporting the call control messages while initiating a call without floor control using pre-established session and all the set of CRs were agreed. The proposal has an erroneous text which will result into original issue to be persisted without providing a fix. Hence phrase of text needs to replaced from “SDP offer not including media-level…” to “SDP offer ~~not~~ including media-level…” to fix the issue in the clause 11.1.2.3.1. |
|  |  |
| ***Summary of change:*** | The condition to determine a private call or first-to-answer without floor control on receipt of a "SIP REFER request for a pre-established session" is corrected.Changes: A phrase of text is replaced from “SDP offer not including media-level…” to “SDP offer ~~not~~ including media-level…” to fix the issue in the clause 11.1.2.3.1. |
|  |  |
| ***Consequences if not approved:*** | The origional issue will continue to persist even though a solution is implemented |
|  |  |
| ***Clauses affected:*** | 11.1.2.3.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**\*\*\*\*\*\*\***

\* \* \* First Change \* \* \* \*

##### 11.1.2.3.1 Originating procedures

Upon receipt of a "SIP INVITE request for originating participating MCPTT function" for a private call or first-to-answer call with an SDP offer not including a media-level section for media plane control messages, the participating MCPTT function shall consider it as a request for a private call without floor control or first-to-answer call without floor control and shall follow the procedures as specified in clause 11.1.1.3.1.1 for an on-demand session.

Upon receipt of a "SIP REFER request for a pre-established session" for a private call or first-to-answer call with an SDP offer including a media-level section for media plane control messages with the 'fmtp' attribute containing a value of "mc\_no\_floor\_ctrl" as specified in 3GPP TS 24.380 [5] clause 14, the participating MCPTT function shall consider it as a request for a private call without floor control or first-to-answer call without floor control and shall follow the procedures as specified in clause 11.1.1.3.1.2 for initiation using a pre-established session.

\* \* \* End of Changes \* \* \* \*