**3GPP TSG-CT WG1 Meeting #135-eC1-224209**

**E-Meeting, 6th – 12th April 2022**

Title: LS on name of the interface for usage information collection

Response to: -

Release: Rel-17

Work Item: 5G\_ProSe

Source: CT1

To: SA5

Cc: SA2

**Contact Person:**

Name: Xiaoyan Duan

E-mail Address: duanxiaoyan@catt.cn

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

Attachments: None

**1. Overall Description:**

CT1 discussed the usage information report for charging in 5G ProSe. According to TS 32.277, the 5G DDNMF takes the role of "ProSe Function"; while CT1 has defined the interface between the UE and 5G DDNMF as PC3a, see TS 24.554. So CT1 wonders whether the interface between the UE and 5G DDNMF CTF (ADF) for usage information collection should be named as PC3ach, instead of PC3ch which is the interface between the UE and ProSe Function CTF(ADF) in 4G.

**2. Actions:**

**To SA2 group.**

**ACTION:** CT1 kindly asks SA5 to clarify the name for the interface between the UE and 5G DDNMF CTF (ADF).

**3. Date of Next CT1 Meetings:**

CT1#137e 18th - 26th August 2022 e-meeting

CT1#138e 10th - 14th October 2022 e-meeting