**3GPP TSG-CT WG1 Meeting #149C1-243960**

**Hyderabad, India, 27-31 May 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **24.559** | **CR** | **????** | **rev** | **-** | **Current version:** | **18.0.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update info and externalDocs fields | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Lenovo | | | | | | | | | |
| ***Source to TSG:*** | C1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI18 | | | | |  | ***Date:*** | | | 2024-06-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CRs modifying ADAE\_ServiceConfiguration API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, clause 4.3.1.  The following agreed CRs update the ADAE\_ServiceConfiguration API for the present release:  - TS 24.559 CR #0001 is a backward compatible correction in Rel-18.  - TS 24.559 CR #0002 is a backward compatible correction in Rel-18.  - TS 24.559 CR #0004 is a backward compatible correction in Rel-18.  - TS 24.559 CR #0005 is a backward compatible correction in Rel-18.  As the present release will be frozen for OpenAPI, and a draft version number was already assigned, only the additional Pre-Release version field needs to be removed.  Since a new TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The ADAE\_ServiceConfiguration API version number set to value "1.1.0".  The TS version number in the "description" field of the "externalDocs" object is changed to "18.1.0". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\* First Change \*\*\*

# A.2 ADAE\_ServiceConfiguration API

openapi: 3.0.0

info:

title: ADAE\_ServiceConfiguration

version: 1.0.0

description: |

API for ADAE service configuration.

© 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 24.559 V18.1.0 Appliction Data Analytics Enablement Service; Stage 3.

url: https://www.3gpp.org/ftp/Specs/archive/24\_series/24.559/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/adae-sc/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

paths:

/application-performance:

post:

description: >

Creates a new individual VAL performance analytics event subscription.

operationId: VALPerformanceSubscription

tags:

- VAL performance event subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: VAL performance event subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_VALPerformanceAnalytics.yaml#/components/schemas/AppPerfSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/application-performance/{appPerfId}:

delete:

description: Deletes an individual VAL performance event subscription.

operationId: DeleteIndValPerfEventSubsc

tags:

- Individual VAL performance event subscription

parameters:

- name: appPerfId

in: path

description: Identifier of an individual VAL performance event subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The individual VAL performance subscription matching the appPerfId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/ue2ue-session-performance/fetch:

post:

description: >

Obtain the UE-to-UE session performance analytics.

operationId: FetchUe2UeSessionPerformance

tags:

- Fetch UE-to-UE session performance analytics

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/Ue2UePerfReq'

responses:

'200':

description: >

Successful case. The UE-to-UE session performance information is returned in

the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/Ue2UePerfResp'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/edge-load:

post:

description: >

Creates a new individual edge load data collection event subscription.

operationId: EdgeLoadDataCollectionSubscription

tags:

- Edge load data collection event subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

callbacks:

notificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeNotif'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Edge load data collection event subscription resource created successfully.

content:

application/json:

schema:

$ref: 'TS29549\_SS\_ADAE\_EdgeLoadAnalytics.yaml#/components/schemas/EdgeSub'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/edge-load/{edgeLdId}:

delete:

description: Deletes an individual edge load data collection event subscription.

operationId: DeleteIndEdgeLdDataCollectEventSubsc

tags:

- Individual edge load data collection event subscription

parameters:

- name: edgeLdId

in: path

description: Identifier of an individual edge load data collection event subscription.

required: true

schema:

type: string

responses:

'204':

description: >

The individual edge load data collection subscription matching the edgeLdId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/service-experience:

post:

description: >

Configures the ADAEC triggers for service experience reporting.

operationId: ConfigTriggerServExpReporting

tags:

- Configuration for service experience reporting (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ConfigRepTrigger'

callbacks:

serExpNotificationUri:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SrvExpInfoRep'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Triggers for service experience reporting configured successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/ConfigRepTrigger'

headers:

Location:

description: Contains the URI of the newly created resource.

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/service-experience/{srvTrigId}:

delete:

description: Abolish configured triggers for service experience reporting.

operationId: DeleteTriggerSrvExpReporting

tags:

- Individual configured trigger for service experience reporting

parameters:

- name: srvTrigId

in: path

description: Identifier of an individual triger-configured service experience reporting.

required: true

schema:

type: string

responses:

'204':

description: >

The individual trigger-configured service experiment reporting matching

the srvTrigId is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/service-experience/push:

post:

description: >

Configure ADAE client to push service experience report to the ADAE server.

operationId: PushSrvExpReport

tags:

- Push service experienec report

requestBody:

required: true

content:

application/json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

responses:

'200':

description: >

Successful case. The ADAE client pushes service experience reporting to the ADAE server.

content:

application/json:

schema:

$ref: '#/components/schemas/SrvExpInfoRep'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/service-experience/pull:

post:

description: >

ADAE server pulls service experience report from the ADAE client.

operationId: PullSrvExpReport

tags:

- Pull service experienec report

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PullSrvExpInfo'

responses:

'200':

description: >

Successful case. The ADAE client provides service experience reporting to

the ADAE server.

content:

application/json:

schema:

$ref: '#/components/schemas/SrvExpInfoRep'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

Ue2UePerfReq:

description: ADAES requests ADAEC for the UE-to-UE session performance analytics.

type: object

properties:

serverId:

type: string

description: String identifying the ADAE server

analyticsId:

type: string

description: String identifying the UE-to-UE session analytics

valUeIds:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

description: >

One or more VAL UE IDs whose UE-to-UE session performance is requested.

pc5Qos:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Pc5QoSPara'

reportConfig:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

area:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

timeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

required:

- serverId

- analyticsId

- valUeIds

- pc5Qos

Ue2UePerfResp:

description: >

ADAEC responds to ADAES with the UE-to-UE session performance analytics information.

type: object

properties:

dataOutputs:

type: array

items:

type: string

minItems: 1

description: >

UE-to-UE session performance analytics for prediction or statistics.

valUeIds:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

description: >

One or more VAL UE IDs whose UE-to-UE session performance has been requested.

analyticsId:

type: string

description: String identifying the UE-to-UE session analytics

required:

- dataOutputs

- valUeIds

- analyticsId

ConfigRepTrigger:

description: Configures the ADAEC triggers for service experience reporting.

type: object

properties:

valServSpecCrit:

$ref: '#/components/schemas/ValServSpecCrit'

commonTriggCrit:

$ref: '#/components/schemas/SrvExpRepCrit'

srvExpMeas:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

notifyTarget:

type: string

description: the target address which is notified.

required:

- valServSpecCrit

ValServSpecCrit:

description: String identifying the ADAE server.

type: object

properties:

valServerIds:

type: array

description: VAL servers for which configuration of service experience report applies.

items:

type: string

minItems: 1

triggCrit:

$ref: '#/components/schemas/SrvExpRepCrit'

required:

- valServerIds

- triggCrit

PullSrvExpInfo:

description: Contains VAL server and service identities.

type: object

properties:

valServerId:

type: string

valServiceId:

type: string

required:

- valServerId

SrvExpInfoRep:

description: Allows ADAEC to provide the service experience report to the ADAES.

type: object

properties:

valUeId:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

valServerId:

type: string

description: String identifying the VAL server the service experience report applies.

valServiceId:

type: string

description: String identifying the VAL service

timeStamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

valSrvExpRep:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

required:

- valUeId

- valServerId

# Simple data types and Enumerations

SrvExpRepCrit:

anyOf:

- type: string

enum:

- TRIGGER\_CRITERIA

- COMMON\_TRIGGER\_CRITERIA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: |

Represents information criteria to trigger service experience reporting.

Possible values are:

- TRIGGER\_CRITERIA: Information criteria that can trigger service experience

reporting to a VAL server.

- COMMON\_TRIGGER\_CRITERIA: Information criteria that can trigger service experience

reporting to all VAL servers.

\*\*\* End of Change \*\*\*