**TSG-CT WG3 Meeting #108-e *C3-201xyz***

**E-Meeting, 19th – 28th February 2020 (Revision of C3-201295)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | **0143** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | AnalyticsExposure API, Support of abnormal behaviour | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | eNA | | | | |  | ***Date:*** | | | 2020-02-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The AnalyticsExposure API is used by the AF to request the NWDAF via the NEF to report the analytics results. However, the data type for Abnormal behaviour analytics is not defined yet. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Complete the abnormal behaviour definition of AnalyticsExposure API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incomplete specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.6.3.2; 5.6.3.3.4; 5.6.3.3.14; 5.6.3.3.x (new); A.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible feature into the OpenAPI file for AnalyticsExposure API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 5.6.3.2 Reused data types

The data types reused by the AnalytcisExposure API from other specifications are listed in table 5.6.3.2-1.

Table 5.6.3.2-1: Re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| AdditionalMeasurement | 3GPP TS 29.520 [27] |  |
| AnalyticsReportingRequirement | 3GPP TS 29.520 [27] | Describes the analytics reporting requirement information. |
| DateTime | 3GPP TS 29.122 [4] |  |
| DurationSec | 3GPP TS 29.122 [4] | Seconds of duration. |
| ExternalGroupId | 3GPP TS 29.122 [4] | External Group Identifier for a user group. |
| Gpsi | 3GPP TS 29.571 [8] | Identifies a GPSI. |
| NotificationMethod | 3GPP TS 29.508 [26] | Represents the Notification Method. |
| EventReportingRequirement | 3GPP TS 29.520 [27] |  |
| SamplingRatio | 3GPP TS 29.571 [8] | Indicates Sampling Ratio. |
| ScheduledCommunicationTime | 3GPP TS 29.122 [4] |  |
| SupportedFeatures | 3GPP TS 29.571 [8] | Used to negotiate the applicability of the optional features defined in table 5.6.4-1. |
| TargetUeInformation | 3GPP TS 29.520 [27] |  |
| Uinteger | 3GPP TS 29.571 [8] | Unsigned integer. |
| Uri | 3GPP TS 29.571 [8] | Identifies a referenced resource. |
| WebsockNotifConfig | 3GPP TS 29.122 [4] | Contains the configuration parameters to set up notification delivery over Websocket protocol. |
| LocationArea5G | 3GPP TS 29.122 [4] |  |
| Communication | 3GPP TS 29.520 [27] |  |

\*\*\* Next Change \*\*\*

##### 5.6.3.3.4 Type: AnalyticsEventNotif

Table 5.6.3.3.4-1: Definition of type AnalyticsEventNotif

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| analyEvent | AnalyticsEvent | M | 1 | Detected analytics event. |  |
| timeStamp | DateTime | M | 1 | Time at which the event is observed. |  |
| ueMobilityInfos | array(UeMobilityExposure) | C | 1..N | Contains the UE mobility information.  Shall be present if the "analyEvent" attribute sets to "UE\_MOBILITY" | Ue\_Mobility |
| ueCommInfos | array(UeCommunicationExposure) | C | 1..N | Contains the application communication information.  Shall be present if the "analyEvent" attribute sets to "UE\_COMM" | Ue\_Communication |
| abnormalInfos | array(AbnormalExposure) | C | 1..N | Contains the user’s abnormal behavior information.  Shall be present if the "analyEvent" attribute sets to "ABNORMAL\_BEHAVIOR" | Abnormal\_Behavior |
| congestInfo | CongestInfo | C | 0..1 | Contains the UE’s user data congestion information.  Shall be present if the "analyEvent" attribute sets to "CONGESTION" | Congestion |

Editor’s Note: The definition of AbnormalInfo and CongestInfo are FFS.

\*\*\* Next Change \*\*\*

##### 5.6.3.3.14 Type AnalyticsData

Table 5.6.3.3.14-1: Definition of type AnalyticsData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| ueMobilityInfos | array(UeMobilityExposure) | C | 1..N | Contains the UE mobility information.  Shall be present if the "analyEvent" attribute sets to "UE\_MOBILITY" | Ue\_Mobility |
| ueCommInfos | array(UeCommunicationExposure) | C | 1..N | Contains the application communication information.  Shall be present if the "analyEvent" attribute sets to "UE\_COMM" | Ue\_Communication |
| abnormalInfos | array(AbnormalExposure) | C | 1..N | Contains the user’s abnormal behavior information.  Shall be present if the "analyEvent" attribute sets to "ABNORMAL\_BEHAVIOR" | Abnormal\_Behavior |
| suppFeat | SupportedFeatures | M | 1 | Represents the features supported by the NF service consumer. |  |

\*\*\* Next Change \*\*\*

##### 5.6.3.3.x Type AbnormalExposure

Table 5.6.3.3.x-1: Definition of type AbnormalExposure

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| gpsis | array(Gpsi) | C | 1..N | Each element identifies a UE which is affected with the Exception.  Shall be present if the subscription request applies to more than one UE. |  |
| excep | Exception | M | 1 | Contains the exception information. |  |
| ratio | SamplingRatio | C | 0..1 | If the analytics result applies for a group of UEs or any UE, this attribute contains the percentage of UEs. The sum of all ratios on a given abnorBehavrs (which is of AbnormalBehaviour data type) is equal or less than 100%. |  |
| confidence | Uinteger | C | 0..1 | If the analytics result is a prediction, it indicates the confidence of the prediction. |  |
| addtMeasInfo | AdditionalMeasurement | O | 0..1 | Additional measurement. |  |

\*\*\* Next Change \*\*\*

# A.4 AnalyticsExposure API

openapi: 3.0.0

info:

title: 3gpp-analyticsexposure

version: 1.0.0.alpha-1

description: |

API for Analytics Exposure.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.522 V16.2.0; 5G System; Network Exposure Function Northbound APIs.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-analyticsexposure/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

tags:

- AF level GET Operation

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

minItems: 0

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

tags:

- subscription level POST Operation

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

callbacks:

notification:

'{request.body#/notifUri}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsEventNotification'

responses:

'204':

description: No Content (successful notification)

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'204':

description: Successful case. The resource has been successfully created and no additional content is to be sent in the response message.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

tags:

- Subscription level GET Operation

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource

tags:

- Subscription level PUT Operation

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

responses:

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsExposureSubsc'

'204':

description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

tags:

- Subscription level DELETE Operation

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/fetch:

post:

summary: Fetch analytics information

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsRequest'

responses:

'200':

description: The requested information was returned successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/AnalyticsData'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AnalyticsExposureSubsc:

type: object

properties:

analyEventsSubs:

type: array

items:

$ref: '#/components/schemas/AnalyticsEventSubsc'

minItems: 1

analyRepInfo:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/EventReportingRequirement'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

notifId:

type: string

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- analyEventsSubs

- analyRepInfo

- notifUri

- notifId

AnalyticsEventNotification:

type: object

properties:

notifId:

type: string

analyEventNotifs:

type: array

items:

$ref: '#/components/schemas/AnalyticsEventNotif'

minItems: 1

AnalyticsEventNotif:

type: object

properties:

analyEvent:

$ref: '#/components/schemas/AnalyticsEvent'

timeStamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

ueMobilityInfos:

type: array

items:

$ref: '#/components/schemas/UeMobilityExposure'

minItems: 1

ueCommInfos:

type: array

items:

$ref: '#/components/schemas/UeCommunicationExposure'

minItems: 1

abnormalInfos:

type: array

items:

$ref: '#/components/schemas/AbnormalExposure'

minItems: 1

congestInfo:

type: string

required:

- analyEvent

- timeStamp

AnalyticsEventSubsc:

type: object

properties:

analyEvent:

$ref: '#/components/schemas/AnalyticsEvent'

analyEventFilter:

$ref: '#/components/schemas/AnalyticsEventFilterSubsc'

required:

- analyEvent

AnalyticsEventFilterSubsc:

type: object

properties:

tgtUe:

$ref: '#/components/schemas/TargetUeId'

TargetUeId:

type: object

properties:

anyUeInd:

type: boolean

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

exterGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

UeMobilityExposure:

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ueTrajs:

type: array

items:

$ref: '#/components/schemas/UeTrajectoryInfo'

minItems: 1

required:

- ueTrajs

UeTrajectoryInfo:

type: object

properties:

ts:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

recurringTime:

$ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

duration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

locInfo:

type: array

items:

$ref: '#/components/schemas/UeLocationInfo'

minItems: 1

required:

- duration

- locInfo

UeLocationInfo:

type: object

properties:

loc:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

ratio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

confidence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

required:

- loc

UeCommunicationExposure:

type: object

properties:

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

comms:

type: array

items:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/Communication'

minItems: 1

required:

- comms

AnalyticsRequest:

type: object

properties:

analyEvent:

$ref: '#/components/schemas/AnalyticsEvent'

analyEventFilter:

$ref: '#/components/schemas/AnalyticsEventFilter'

analyRep:

$ref: 'TS29520\_Nnwdaf\_AnalyticsInfo.yaml#/components/schemas/AnalyticsReportingRequirement'

tgtUe:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/TargetUeInformation'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- analyEvent

- tgtUe

- suppFeat

AnalyticsEventFilter:

type: object

properties:

locArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

maxAnaEntry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

AnalyticsData:

type: object

properties:

ueMobilityInfos:

type: array

items:

$ref: '#/components/schemas/UeMobilityExposure'

minItems: 1

ueCommInfos:

type: array

items:

$ref: '#/components/schemas/UeCommunicationExposure'

minItems: 1

abnormalInfos:

type: array

items:

$ref: '#/components/schemas/AbnormalExposure'

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- suppFeat

AbnormalExposure:

type: object

properties:

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

excep:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/Exception'

ratio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

confidence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

addtMeasInfo:

$ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/AdditionalMeasurement'

required:

- excep

AnalyticsEvent:

anyOf:

- type: string

enum:

- UE\_MOBILITY

- UE\_COMM

- ABNORMAL\_BEHAVIOR

- CONGESTION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UE\_MOBILITY: The AF requests to be notified about analytics information of UE mobility.

- UE\_COMM: The AF requests to be notified about analytics information of UE communication.

- ABNORMAL\_BEHAVIOR: The AF requests to be notified about analytics information of UE’s abnormal behavior.

- CONGESTION: The AF requests to be notified about analytics information of user data congestion information.

\*\*\* End of Changes \*\*\*