**3GPP TSG-CT WG3 Meeting #109eC3-202343**

**E-Meeting, 16th – 24th April 2020**  (Revision of C3-202240)

**Source: Samsung**

**Title: Pseudo-CR on Location based group creation**

**Spec: 3GPP TS 29.549 v1.1.0**

**Agenda item: 16.27**

**Document for: Decision**

**1. Introduction**

As per Clause 10.3.7 of TS 23.434, VAL server sends group creation request to group management server with location criteria information. Group management server obtains the list of users or UEs from location management server based on the location information. This list is used in the creation of new VAL group.

**2. Reason for Change**

Stage 3 aspects of location based group creation is missing.

**3. Conclusions**

None.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TS 29.549 v1.1.0.

\* \* \* First Change \* \* \* \*

###### 5.3.1.2.4.2 VAL server creating new group using Create\_Group service operation

To create a VAL group, the VAL server shall send a HTTP POST message to the group management server. The body of the POST message shall include VAL group document information as specified in clause 7.2.1.2.2.3.1. Upon receiving HTTP POST message, the group management server shall

1. verify the identity of the VAL server and check if the VAL server is authorized to create VAL group document;

2. if the VAL group document information in the request includes location criteria, shall obtain the list of VAL users or VAL UEs within the requested location criteria information from the Location Management server and include them in VAL group members of the new VAL group;

3. if the VAL server is authorized to create VAL group document, shall create a new resource as defined in 7.2.1.2.2.3.1 and return the VAL group document and its Resource URI in the response message.

\* \* \* Next Change \* \* \* \*

##### 7.2.1.4.1 General

This clause specifies the application data model supported by the API. Data types listed in clause 6.2 apply to this API

Table 7.2.1.4.1-1 specifies the data types defined specifically for the SS\_GroupManagement API service.

Table 7.2.1.4.1-1: SS\_GroupManagement API specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| VALGroupDoument | 7.2.1.4.2.2 | VAL group document details. |  |

Table 7.2.1.4.1-2 specifies data types re-used by the SS\_GroupManagement API service.

Table 7.2.1.4.1-2: Re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| SupportedFeatures | 3GPP TS 29.571 [21] | Used to negotiate the applicability of optional features defined in table 7.2.1.6-1. |  |
| LocationInfo | 3GPP TS 29.122 [3] | The location information related to VAL group.  |  |

\* \* \* Next Change \* \* \* \*

###### 7.2.1.4.2.2 Type: VALGroupDocument

Table 7.2.1.4.2.2-1: Definition of type VALGroupDocument

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| valGroupId | string | M | 1 | This is VAL group identity (VAL group ID) as per TS 23.434 [2], which is a unique identifier within the VAL service that represents a VAL group, set of VAL users or VAL UEs according to the VAL service. |  |
| grpDesc | string | O | 0..1 | Text description of the VAL group. |  |
| membersList | array(string) | O | 1..N | List of VAL User IDs and VAL UE IDs, which are members of the VAL group. |  |
| valGrpConf | string | O | 0..1 | Configuration data for the VAL group.Shall be present in HTTP POST request message from VAL server to Group Management server. |  |
| valServiceIds | array(string) | O | 1..N | List of VAL services whose communications enabled on the group. |  |
| suppFeat | SupportedFeatures | O | 0..1 | Used to negotiate the supported optional features of the API as described in clause 6.8.This attribute shall be provided in the HTTP POST request and in the response of successful resource creation. |  |
| locInfo | LocationInfo | O | 0..1 | The location information related to the VAL group. This information is used to determine the members of the group. |  |

\* \* \* Next Change \* \* \* \*

## A.2 SS\_GroupManagement API

openapi: 3.0.0

info:

 title: SS\_GroupManagement

 description: |

 API for SEAL Group management.

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.0.0.alpha-1"

externalDocs:

 description: 3GPP TS 29.549 V1.1.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

servers:

 - url: '{apiRoot}/group-management/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /group-documents:

 post:

 description: Creates a new VAL group document.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 responses:

 '201':

 description: VAL group created sucessfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/group-management/v1/group-documents/{groupDocId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /group-documents/{groupDocId}:

 get:

 description: Retrieves VAL group information satisfying filter criteria

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 - name: group-members

 in: query

 description: When set to true indicates the group management server to send the members list information of the VAL group.

 schema:

 type: boolean

 - name: group-configuration

 in: query

 description: When set to true indicates the group management server to send the group configuration information of the VAL group.

 schema:

 type: boolean

 responses:

 '200':

 description: The VAL group information based on the request from the VAL server. Includes VAL group members list if group-members flag is set to true in the request, VAL group configuration information if the group-configuration flag is set to true in the request, VAL group identifier, whole VAL group document resource if both group-members and group-configuration flags are omitted/set to false in the request.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Updates an individual VAL group document.

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 requestBody:

 description: VAL group document to be updated in Group management server.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 responses:

 '200':

 description: VAL group document updated successfully

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Deletes a VAL Group.

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual VAL group matching groupDocId was deleted.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 schemas:

 VALGroupDocument:

 type: object

 properties:

 valGroupId:

 type: string

 description: The VAL group idenitity.

 grpDesc:

 type: string

 description: The text description of the VAL group.

 membersList:

 type: array

 description: The list of VAL User IDs and VAL UE IDs, which are members of the VAL group.

 items:

 type: string

 minItems: 1

 valGrpConf:

 type: string

 description: Configuration data for the VAL group.

 valServiceIds:

 type: array

 description: The list of VAL services enabled on the group.

 items:

 type: string

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 locInfo:

 $ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/LocationInfo'

 required:

 - valGroupId

\* \* \* End of Changes \* \* \* \*