**3GPP TSG-CT3 Meeting #112e C3-205063\_r1**

**E-Meeting, 04th – 13th November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.554** | **CR** | **0053** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Essential corrections and alignments |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc16 |  | ***Date:*** | 2020-10-?? |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The following corrections and alignments are necessary:* The "Resource URI" column of Table 5.3.1-1 should contain a "<relative URI below root>" instead of a full resource URI, as per the API TS skeleton provided in TS 29.501.
* The "Notifications overview" table needs to be updated to align with the SBI TS skeleton provided in TS 29.501.
 |
|  |  |
| ***Summary of change:*** | * Update the "Resource URI" column of Table 5.3.1-1 by replacing the full resource URI with the associated "<relative URI below root>", i.e. by removing the part "{apiRoot}/<apiName>/<apiVersion>".
* Update the "Notifications overview" table to align with the updated SBI TS skeleton provided in TS 29.501.
 |
|  |  |
| ***Consequences if not approved:*** | Necessary corrections are not applied. |
|  |  |
| ***Clauses affected:*** | 5.3.1, 5.5.1, 5.5.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact OpenAPI specification files. |
|  |  |
| ***This CR's revision history:*** | Rev 1: Additional changes to clause 5.5.2.2 to further align with the SBI TS Skeleton. |

\* \* \* Start of changes \* \* \* \*

5.3.1 Resource Structure

****

**Figure 5.3.1-1: Resource URI structure of the Npcf\_BDTPolicyControl API**

Table 5.3.1-1 provides an overview of the resources and applicable HTTP methods.

**Table 5.3.1-1: Resources and methods overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Resource name** | **Resource URI** | **HTTP method or custom operation** | **Description** |
| BDT policies | /bdtpolicies | POST | Npcf\_BDTPolicyControl\_Create. Creates a new Individual BDT policy resource. |
| Individual BDT policy | /bdtpolicies/{bdtPolicyId} | GET | Reads an Individual BDT policy resource. |
| PATCH | Npcf\_BDTPolicyControl\_Update.Modifies an existing Individual BDT policy resource by selecting or reselecting a transfer policy. |

\* \* \* Next changes \* \* \* \*

5.5.1 General

Notifications shall comply to subclause 6.2 of 3GPP TS 29.500 [6] and subclause 4.6.2.3 of 3GPP TS 29.501 [7].

**Table 5.5.1-1: Notifications overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Notification** | **Callback URI** | **HTTP method or custom operation** | **Description (service operation)** |
| BDT Notification | {notifUri} | POST | Provides BDT notification. |

\* \* \* Next changes \* \* \* \*

#### 5.5.2.2 Target URI

The Callback URI "**{notifUri}**" shall be used with the callback URI variables defined in table 5.5.2.2-1.

Table 5.5.2.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| notifUri | Uri | It contains the URI of the recipient of BDT notification as assigned by the NF service consumer during the Create service operation and described within the BdtReqData (see table 5.6.2.3-1). |

\* \* \* End of changes \* \* \* \*