**3GPP TSG-CT3 Meeting #112e C3-205065\_r1**

**E-Meeting, 04th – 13th November 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.594** | **CR** | **0061** | **rev** | **1** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Essential corrections and alignments |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc16 |  | ***Date:*** | 2020-10-?? |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The following corrections and alignments are necessary:* The "Resource URI" column of Table 5.3.1-1 should contain a "<relative URI below root>" instead of a full resource URI, as per the API TS skeleton provided in TS 29.501.
* The "Notifications overview" table needs to be updated to align with the SBI TS skeleton provided in TS 29.501.
 |
|  |  |
| ***Summary of change:*** | * Update the "Resource URI" column of Table 5.3.1-1 by replacing the full resource URI with the associated "<relative URI below root>", i.e. by removing the part "{apiRoot}/<apiName>/<apiVersion>".
* Update the "Notifications overview" table to align with the updated SBI TS skeleton provided in TS 29.501.
 |
|  |  |
| ***Consequences if not approved:*** | Necessary corrections are not applied. |
|  |  |
| ***Clauses affected:*** | 5.3.1, 5.5.1, 5.5.2.2, 5.5.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact OpenAPI specification files. |
|  |  |
| ***This CR's revision history:*** | Rev 1: Further align with the SBI TS Skeleton in clause 5.5.1 and add similar changes to clause 5.5.2.2 in clause 5.5.3.2.. |

\* \* \* Start of changes \* \* \* \*

5.3.1 Resource Structure

Figure 5.3.1-1 shows the resource structure of the Nchf\_SpendingLimitControl API.

****

**Figure 5.3.1-1: Resource URI structure of the** **Nchf\_SpendingLimitControl API**

Table 5.3.1-1 provides an overview of the resources and applicable HTTP methods.

**Table 5.3.1-1: Resources and methods overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Resource name** | **Resource URI** | **HTTP method or custom operation** | **Description** |
| Spending Limit Retrieval Subscriptions | /subscriptions | POST | Creates a new individual spending limit retrieval subscription. |
| Individual Spending Limit Retrieval Subscription | /subscriptions/{subscriptionId} | PUT | Modifies an existing subscription (e.g. addition of additional policy counters). |
| DELETE | Deletes an individual subscription. |

\* \* \* Next changes \* \* \* \*

5.5.1 General

Notification shall comply with subclause 6.2 of 3GPP TS 29.500 [4] and subclause 4.6.2.3 of 3GPP TS 29.501 [5].

**Table 5.5.1-1: Notifications overview**

|  |  |  |  |
| --- | --- | --- | --- |
| **Notification** | **Callback URI** | **HTTP method or custom operation** | **Description (service operation)** |
| Spending limit notification | {notifUri}/notify | notify (POST) | Counter Status changes notification. |
| Subscription Termination | {notifUri}/terminate | terminate (POST) | Indication of subscription termination. |

\* \* \* Next changes \* \* \* \*

5.5.2.2 Target URI

The Callback URI **{notifUri}/notify** shall be used with the callback URI variables defined in table 5.5.2.2-1.

**Table 5.5.2.2-1: Callback URI variables**

|  |  |  |
| --- | --- | --- |
| **Name** | **Data type** | **Definition** |
| notifUri | Uri | The Notification Uri as assigned by the NF service consumer during the subscription service operation and described within the SpendingLimitContext data type (see table 5.6.2.2-1). |

\* \* \* Next changes \* \* \* \*

#### 5.5.3.2 Target URI

The Callback URI **{notifUri}/terminate** shall be used with the callback URI variables defined in table 5.5.3.2-1.

Table 5.5.3.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| notifUri | Uri | The Notification Uri as assigned by the NF service consumer during the subscription service operation and described within the SpendingLimitContext data type (see table 5.6.2.2-1). |

\* \* \* End of changes \* \* \* \*