**3GPP TSG-CT3 Meeting #112eC3-205076-r1(C3-205371)**

**Online, , 4th Nov 2020 - 13th Nov 2020 (revision of …)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.508** | **CR** | **0104** | **rev** | **-** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Storage of YAML files in 3GPP Forge |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** | SBIProtoc16  |  | ***Date:*** | 2020-11-06 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16) Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | MCC shall store OpenAPI files extracted from 3GPP specifications at <https://forge.3gpp.org/rep/all/5G_APIs>.The storage at [https://www.3gpp.org/ftp/Specs/archive/OpenAPI/<Release>/](https://www.3gpp.org/ftp/Specs/archive/OpenAPI/%3CRelease%3E/)and [https://www.3gpp.org/ftp/Specs/<Plenary>/<Release>/OpenAPI/](https://www.3gpp.org/ftp/Specs/%3CPlenary%3E/%3CRelease%3E/OpenAPI/) is discontinued. |
|  |  |
| ***Summary of change:*** | Clarify in Annex A.1 the correct location where YAML files are stored, using the text agreed in the 3GPP TS template for 5GC APIs (see TS 29.501). |
|  |  |
| ***Consequences if not approved:*** | Incorrect information in the TS regarding the storage of YAML files. |
|  |  |
| ***Clauses affected:*** | A.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not change the OpenAPI file. |
|  |  |
| ***This CR's revision history:*** |  |

1st Change \*\*\*

Annex A (normative):
OpenAPI specification

# A.1 General

The present Annex contains an OpenAPI [10] specification of HTTP messages and content bodies used by the Nsmf\_EventExposure API.

This Annex shall take precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API.

NOTE: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification file contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see clause 5B of the 3GPP TR 21.900 [19] and subclause 5.3.1 of the 3GPP TS 29.501 [5] for further information).

\*\*\* End of Changes \*\*\*