**TSG-CT WG3 Meeting #112-e *C3-205xyz***

**E-Meeting, 4th – 13th November 2020 (Revision of C3-205275)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.520** | **CR** | **0232** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Error response for statistics request |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eNA |  | ***Date:*** | 2020-10-28 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | As agreed [S2-2006218](https://www.3gpp.org/ftp/tsg_sa/WG2_Arch/TSGS2_140e_Electronic/Docs/S2-2006218.zip) indicated, the NWDAF can send a error response when receiving a request or subscription for statistics while data in the past is unavailable. |
|  |  |
| ***Summary of change:*** | Define an application error for error response when receiving a request or subscription for statistics while data in the past is unavailable. |
|  |  |
| ***Consequences if not approved:*** | The behaviour of the NWDAF is unclear when the NWDAF receives a request or subscription for statistics while data in the past is unavailable. |
|  |  |
| ***Clauses affected:*** | 5.1.6.2.2; 5.1.6.2.x (new); 5.1.6.3.x (new); 5.1.7.3; 5.2.7.3; A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible corrections on the OpenAPI file for Nnwdaf\_EventsSubscription API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.1.6.2.2 Type NnwdafEventsSubscription

Table 5.1.6.2.2-1: Definition of type NnwdafEventsSubscription

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| eventSubscriptions | array(EventSubscription) | M | 1..N | Subscribed events |  |
| evtReq | ReportingInformation | O | 0..1 | Represents the reporting requirements of the event subscription. (NOTE 1, NOTE 2)If omitted, the default values within the ReportingInformation data type apply. |  |
| notificationURI | Uri | C | 0..1 | Identifies the recipient of Notifications sent by the NWDAF.This parameter shall be supplied by the NF service consumer in the HTTP POST requests that include an object of EventSubscription type. |  |
| eventNotifications | array(EventNotification) | C | 1..N | Notifications about Individual Events.Shall only be present if the immediate reporting indication in the "immRep" attribute within the "evtReq" attribute sets to true in the event subscription, and the reports are available. |  |
| failEventReports | array(FailureEventInfo) | O | 1..N | Supplied by the NWDAF and contains the event for which the subscription is not successful. The failure reason is also included.  |  |
| supportedFeatures | SupportedFeatures | C | 0..1 | List of Supported features used as described in subclause 5.1.8.This parameter shall be supplied by NF service consumer in the POST request that request the creation of an NWDAF Event Subscriptions resource, and shall be supplied by the NWDAF in the reply of corresponding request. |  |
| NOTE 1: If the "evtReq" attribute in the ReportingInformation data type is provided, the notification method indicated by the "notifMethod" attribute within the ReportingInformation data type takes preference over the notification method indicated by the "notificationMethod" attribute within the EventSubscription data type. NOTE 2: If the "evtReq" attribute in the ReportingInformation data type is provided, the periodic reporting time indicated by the "repPeriod" attribute in the ReportingInformation data type takes preference over the periodic reporting time indicated by the "repetitionPeriod" attributes in the EventSubscription data type. |

\*\*\* Next Change \*\*\*

##### 5.1.6.2.x Type FailureEventInfo

Table 5.1.6.2.x-1: Definition of type FailureEventInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| event | NwdafEvent | M | 1 | Event that is subscribed. |  |
| failureCode | NwdafFailureCode | M | 1 | Identifies the failure reason |  |

\*\*\* Next Change \*\*\*

##### 5.1.6.3.x Enumeration: NwdafFailureCode

Table 5.1.6.3.x-1: Enumeration NwdafFailureCode

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| UNAVAILABLE\_DATA | Indicates the requested statistics information for the event is rejected since necessary data to perform the service is unavailable. |  |

\*\*\* Next Change \*\*\*

#### 5.1.7.3 Application Errors

The application errors defined for the Nnwdaf\_EventsSubscription API are listed in table 5.1.7.3-1. The NWDAF shall include in the HTTP status code a "ProblemDetails" data structure with the "cause" attribute indicating the application error as listed in table 5.7.3-1.

Table 5.1.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| **Application Error** | **HTTP status code** | **Description** |
| SUBSCRIPTION\_NOT\_FOUND | 404 Not Found | Indicates that the modification or deletion has failed because the specified Individual NWDAF Event Subscription resource does not exist. (NOTE) |
| BOTH\_STAT\_PRED\_NOT\_ALLOWED | 400 Bad Request | For the requested observation period, the start time is in the past and the end time is in the future, which means the NF service consumer requested both statistics and prediction for the analytics. |
| UNAVAILABLE\_DATA | 500 Internal Server Error | Indicates the requested statistics in the past is rejected since necessary data to perform the service is unavailable. |
| NOTE: This application error is included in the responses to the GET and the DELETE requests. |

\*\*\* Next Change \*\*\*

#### 5.2.7.3 Application Errors

The application errors defined for the Nnwdaf\_AnalyticsInfo API are listed in table 5.2.7.3-1. The NWDAF shall include in the HTTP status code a "ProblemDetails" data structure with the "cause" attribute indicating the application error as listed in table 5.2.7.3-1.

Table 5.2.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| **Application Error** | **HTTP status code** | **Description** |
| BOTH\_STAT\_PRED\_NOT\_ALLOWED | 400 Bad Request | For the requested observation period, the start time is in the past and the end time is in the future, which means the NF service consumer requested both statistics and prediction for the analytics. |
| UNAVAILABLE\_DATA | 500 Internal Server Error | Indicates the requested statistics in the past is rejected since necessary data to perform the service is unavailable. |

\*\*\* Next Change \*\*\*

# A.2 Nnwdaf\_EventsSubscription API

openapi: 3.0.0

info:

 version: 1.2.0.alpha-1

 title: Nnwdaf\_EventsSubscription

 description: |

 Nnwdaf\_EventsSubscription Service API.

 © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V17.0.0; 5G System; Network Data Analytics Services.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/'

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

servers:

 - url: '{apiRoot}/nnwdaf-eventssubscription/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

 /subscriptions:

 post:

 summary: Create a new Individual NWDAF Events Subscription

 operationId: CreateNWDAFEventsSubscription

 tags:

 - NWDAF Events Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-eventssubscription/v1/subscriptions/{subscriptionId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notificationURI}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 responses:

 '204':

 description: The receipt of the Notification is acknowledged.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 delete:

 summary: Delete an existing Individual NWDAF Events Subscription

 operationId: DeleteNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF Event Subscription resource matching the subscriptionId was deleted.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Events Subscription

 operationId: UpdateNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The Individual NWDAF Event Subscription resource was modified successfully and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '204':

 description: The Individual NWDAF Event Subscription resource was modified successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-eventssubscription: Access to the Nnwdaf\_EventsSubscription API

 schemas:

 NnwdafEventsSubscription:

 type: object

 properties:

 eventSubscriptions:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationURI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 failEventReports:

 type: array

 items:

 $ref: '#/components/schemas/FailureEventInfo'

 minItems: 1

 required:

 - eventSubscriptions

 EventSubscription:

 type: object

 properties:

 anySlice:

 $ref: '#/components/schemas/AnySlice'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 description: Identification(s) of application to which the subscription applies.

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Identification(s) of DNN to which the subscription applies.

 dnais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 event:

 $ref: '#/components/schemas/NwdafEvent'

 extraReportReq:

 $ref: '#/components/schemas/EventReportingRequirement'

 loadLevelThreshold:

 type: integer

 description: Indicates that the NWDAF shall report the corresponding network slice load level to the NF service consumer where the load level of the network slice instance identified by snssais is reached.

 notificationMethod:

 $ref: '#/components/schemas/NotificationMethod'

 matchingDir:

 $ref: '#/components/schemas/MatchingDirection'

 nfLoadLvlThds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 description: Shall be supplied in order to start reporting when an average load level is reached.

 nfInstanceIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 nfSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 nfTypes:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nsiIdInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiIdInfo'

 minItems: 1

 nsiLevelThrds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 qosRequ:

 $ref: '#/components/schemas/QosRequirement'

 qosFlowRetThds:

 type: array

 items:

 $ref: '#/components/schemas/RetainabilityThreshold'

 minItems: 1

 ranUeThrouThds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minItems: 1

 repetitionPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 snssaia:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies. When subscribed event is "SLICE\_LOAD\_LEVEL", either information about slice(s) identified by snssai, or anySlice set to "TRUE" shall be included. It corresponds to snssais in the data model definition of 3GPP TS 29.520. When subscribed is “QOS\_SUSTAINABILITY”, the identifications of network slices is optional.

 tgtUe:

 $ref: '#/components/schemas/TargetUeInformation'

 congThresholds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 nwPerfRequs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfRequirement'

 minItems: 1

 bwRequs:

 type: array

 items:

 $ref: '#/components/schemas/BwRequirement'

 minItems: 1

 excepRequs:

 type: array

 items:

 $ref: '#/components/schemas/Exception'

 minItems: 1

 exptAnaType:

 $ref: '#/components/schemas/ExpectedAnalyticsType'

 exptUeBehav:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ExpectedUeBehaviourData'

 required:

 - event

 NnwdafEventsSubscriptionNotification:

 type: object

 properties:

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 subscriptionId:

 type: string

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required:

 - eventNotifications

 - subscriptionId

 EventNotification:

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeStampGen:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 nfLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NfLoadLevelInformation'

 minItems: 1

 nsiLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiLoadLevelInfo'

 minItems: 1

 sliceLoadLevelInfo:

 $ref: '#/components/schemas/SliceLoadLevelInformation'

 svcExps:

 type: array

 items:

 $ref: '#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 qosSustainInfos:

 type: array

 items:

 $ref: '#/components/schemas/QosSustainabilityInfo'

 minItems: 1

 ueComms:

 type: array

 items:

 $ref: '#/components/schemas/UeCommunication'

 minItems: 1

 ueMobs:

 type: array

 items:

 $ref: '#/components/schemas/UeMobility'

 minItems: 1

 userDataCongInfos:

 type: array

 items:

 $ref: '#/components/schemas/UserDataCongestionInfo'

 minItems: 1

 abnorBehavrs:

 type: array

 items:

 $ref: '#/components/schemas/AbnormalBehaviour'

 minItems: 1

 nwPerfs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfInfo'

 minItems: 1

 required:

 - event

 ServiceExperienceInfo:

 type: object

 properties:

 svcExprc:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/SvcExperience'

 svcExprcVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 required:

 - svcExprc

 BwRequirement:

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 required:

 - appId

 SliceLoadLevelInformation:

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription.

 required:

 - loadLevelInformation

 - snssais

 NsiLoadLevelInfo:

 description: Represents the slice instance and the load level information.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 required:

 - loadLevelInformation

 - snssai

 NsiIdInfo:

 description: Represents the S-NSSAI and the optionally associated Network Slice Instance(s).

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiIds:

 type: array

 items:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 minItems: 1

 required:

 - snssai

 EventReportingRequirement:

 type: object

 properties:

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 maxObjectNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 maxSupiNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeAnaNeeded:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 TargetUeInformation:

 type: object

 properties:

 anyUe:

 type: boolean

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 intGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 UeMobility:

 type: object

 properties:

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 durationVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 locInfos:

 type: array

 items:

 $ref: '#/components/schemas/LocationInfo'

 minItems: 1

 required:

 - duration

 - locInfos

 LocationInfo:

 type: object

 properties:

 loc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loc

 UeCommunication:

 type: object

 properties:

 commDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 commDurVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 perioTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 perioTimeVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 trafChar:

 $ref: '#/components/schemas/TrafficCharacterization'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - commDur

 - trafChar

 TrafficCharacterization:

 type: object

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 maxItems: 2

 ulVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 ulVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 dlVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 dlVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 UserDataCongestionInfo:

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 congestionInfo:

 $ref: '#/components/schemas/CongestionInfo'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 CongestionInfo:

 type: object

 properties:

 congType:

 $ref: '#/components/schemas/CongestionType'

 timeIntev:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 nsi:

 $ref: '#/components/schemas/ThresholdLevel'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - congType

 - timeIntev

 - nsi

 QosSustainabilityInfo:

 type: object

 properties:

 areaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qosFlowRetThd:

 $ref: '#/components/schemas/RetainabilityThreshold'

 ranUeThrouThd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 QosRequirement:

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 gfbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 gfbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 resType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

 pdb:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 per:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 ThresholdLevel:

 type: object

 properties:

 congLevel:

 type: integer

 nfLoadLevel:

 type: integer

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 NfLoadLevelInformation:

 type: object

 properties:

 nfType:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 nfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 nfStatus:

 $ref: '#/components/schemas/NfStatus'

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 nfLoadLevelAverage:

 type: integer

 nfLoadLevelpeak:

 type: integer

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nfType

 - nfInstanceId

 NfStatus:

 type: object

 properties:

 statusRegistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUnregistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUndiscoverable:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 AnySlice:

 type: boolean

 description: FALSE represents not applicable for all slices. TRUE represents applicable for all slices.

 LoadLevelInformation:

 type: integer

 description: Load level information of the network slice instance.

 AbnormalBehaviour:

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 excep:

 $ref: '#/components/schemas/Exception'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 addtMeasInfo:

 $ref: '#/components/schemas/AdditionalMeasurement'

 required:

 - excep

 Exception:

 type: object

 properties:

 excepId:

 $ref: '#/components/schemas/ExceptionId'

 excepLevel:

 type: integer

 excepTrend:

 $ref: '#/components/schemas/ExceptionTrend'

 required:

 - excepId

 AdditionalMeasurement:

 type: object

 properties:

 unexpLoc:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 unexpFlowTeps:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 unexpWakes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 1

 ddosAttack:

 $ref: '#/components/schemas/AddressList'

 wrgDest:

 $ref: '#/components/schemas/AddressList'

 circums:

 type: array

 items:

 $ref: '#/components/schemas/CircumstanceDescription'

 minItems: 1

 IpEthFlowDescription:

 type: object

 properties:

 ipTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 ethTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 AddressList:

 type: object

 properties:

 ipv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 CircumstanceDescription:

 type: object

 properties:

 freq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 tm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 locArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 vol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 RetainabilityThreshold:

 type: object

 properties:

 relFlowNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 relTimeUnit:

 $ref: '#/components/schemas/TimeUnit'

 relFlowRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 NetworkPerfRequirement:

 type: object

 properties:

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nwPerfType

 NetworkPerfInfo:

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - networkArea

 - nwPerfType

 FailureEventInfo:

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 failureCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 required:

 - event

 - failureCode

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - THRESHOLD

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PERIODIC: The subscribe of NWDAF Event is periodically. The periodic of the notification is identified by repetitionPeriod defined in subclause 5.1.6.2.3.

 - THRESHOLD: The subscribe of NWDAF Event is upon threshold exceeded. The threshold of the notification is identified by loadLevelThreshold defined in subclause 5.1.6.2.3.

 NwdafEvent:

 anyOf:

 - type: string

 enum:

 - SLICE\_LOAD\_LEVEL

 - NETWORK\_PERFORMANCE

 - NF\_LOAD

 - SERVICE\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMMUNICATION

 - QOS\_SUSTAINABILITY

 - ABNORMAL\_BEHAVIOUR

 - USER\_DATA\_CONGESTION

 - NSI\_LOAD\_LEVEL

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - SLICE\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice

 - NETWORK\_PERFORMANCE: Indicates that the event subscribed is network performance information.

 - NF\_LOAD: Indicates that the event subscribed is load level and status of one or several Network Functions.

 - SERVICE\_EXPERIENCE: Indicates that the event subscribed is service experience.

 - UE\_MOBILITY: Indicates that the event subscribed is UE mobility information.

 - UE\_COMMUNICATION: Indicates that the event subscribed is UE communication information.

 - QOS\_SUSTAINABILITY: Indicates that the event subscribed is QoS sustainability.

 - ABNORMAL\_BEHAVIOUR: Indicates that the event subscribed is abnormal behaviour.

 - USER\_DATA\_CONGESTION: Indicates that the event subscribed is user data congestion information.

 - NSI\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice and the optionally associated Network Slice Instance

 Accuracy:

 anyOf:

 - type: string

 enum:

 - LOW

 - HIGH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LOW: Low accuracy.

 - HIGH: High accuracy.

 CongestionType:

 anyOf:

 - type: string

 enum:

 - USER\_PLANE

 - CONTROL\_PLANE

 - USER\_AND\_CONTROL\_PLANE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - USER\_PLANE: The congestion analytics type is User Plane.

 - CONTROL\_PLANE: The congestion analytics type is Control Plane.

 - USER\_AND\_CONTROL\_PLANE: The congestion analytics type is User Plane and Control Plane.

 ExceptionId:

 anyOf:

 - type: string

 enum:

 - UNEXPECTED\_UE\_LOCATION

 - UNEXPECTED\_LONG\_LIVE\_FLOW

 - UNEXPECTED\_LARGE\_RATE\_FLOW

 - UNEXPECTED\_WAKEUP

 - SUSPICION\_OF\_DDOS\_ATTACK

 - WRONG\_DESTINATION\_ADDRESS

 - TOO\_FREQUENT\_SERVICE\_ACCESS

 - UNEXPECTED\_RADIO\_LINK\_FAILURES

 - PING\_PONG\_ACROSS\_CELLS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNEXPECTED\_UE\_LOCATION: Unexpected UE location

 - UNEXPECTED\_LONG\_LIVE\_FLOW: Unexpected long-live rate flows

 - UNEXPECTED\_LARGE\_RATE\_FLOW: Unexpected large rate flows

 - UNEXPECTED\_WAKEUP: Unexpected wakeup

 - SUSPICION\_OF\_DDOS\_ATTACK: Suspicion of DDoS attack

 - WRONG\_DESTINATION\_ADDRESS: Wrong destination address

 - TOO\_FREQUENT\_SERVICE\_ACCESS: Too frequent Service Access

 - UNEXPECTED\_RADIO\_LINK\_FAILURES: Unexpected radio link failures

 - PING\_PONG\_ACROSS\_CELLS: Ping-ponging across neighbouring cells

 ExceptionTrend:

 anyOf:

 - type: string

 enum:

 - UP

 - DOWN

 - UNKNOW

 - STABLE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UP: Up trend of the exception level.

 - DOWN: Down trend of the exception level.

 - UNKNOW: Unknown trend of the exception level.

 - STABLE: Stable trend of the exception level.

 TimeUnit:

 anyOf:

 - type: string

 enum:

 - MINUTE

 - HOUR

 - DAY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MINUTE: Time unit is per minute.

 - HOUR: Time unit is per hour.

 - DAY: Time unit is per day.

 NetworkPerfType:

 anyOf:

 - type: string

 enum:

 - GNB\_ACTIVE\_RATIO

 - GNB\_COMPUTING\_USAGE

 - GNB\_MEMORY\_USAGE

 - GNB\_DISK\_USAGE

 - NUM\_OF\_UE

 - SESS\_SUCC\_RATIO

 - HO\_SUCC\_RATIO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - GNB\_ACTIVE\_RATIO: Indicates that the network performance requirement is gNodeB active (i.e. up and running) rate. Indicates the ratio of gNB active (i.e. up and running) number to the total number of gNB

 - GNB\_COMPUTING\_USAGE: Indicates gNodeB computing resource usage.

 - GNB\_MEMORY\_USAGE: Indicates gNodeB memory usage.

 - GNB\_DISK\_USAGE: Indicates gNodeB disk usage.

 - NUM\_OF\_UE: Indicates number of UEs.

 - SESS\_SUCC\_RATIO: Indicates ratio of successful setup of PDU sessions to total PDU session setup attempts.

 - SESS\_SUCC\_RATIO: Indicates Ratio of successful handovers to the total handover attempts.

 ExpectedAnalyticsType:

 anyOf:

 - type: string

 enum:

 - MOBILITY

 - COMMUN

 - MOBILITY\_AND\_COMMUN

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MOBILITY: Mobility related abnormal behaviour analytics is expected by the consumer.

 - COMMUN: Communication related abnormal behaviour analytics is expected by the consumer.

 - MOBILITY\_AND\_COMMUN: Both mobility and communication related abnormal behaviour analytics is expected by the consumer.

 MatchingDirection:

 anyOf:

 - type: string

 enum:

 - ASCENDING

 - DESCENDING

 - CROSSED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - ASCENDING: Threshold is crossed in ascending direction.

 - DESCENDING: Threshold is crossed in descending direction.

 - CROSSED: Threshold is crossed either in ascending or descending direction.

 NwdafFailureCode:

 anyOf:

 - type: string

 enum:

 - UNAVAILABLE\_DATA

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNAVAILABLE\_DATA: Indicates the requested statistics information for the event is rejected since necessary data to perform the service is unavailable.

\*\*\* End of Changes \*\*\*