**3GPP TSG-CT WG3 Meeting #112e C3-205387**

**E-Meeting, 4th – 13th November 2020 (Revision of C3-205327)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.591** | **CR** | **0029** | **rev** | **-** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections to location information usage |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | eNA, TEI17 |  | ***Date:*** | 2020-10-18 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17) Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The NetworkAreaInfo data in NefEventFilter data, including the location information belong to EutraLocation data or NrLocation data in UserLocation data, does not include n3gaLocation data in UserLocation. Hence NEF shall map location data in UeTrajectoryInfo for UE Mobility accordingly. |
|  |  |
| ***Summary of change:*** | Add NOTE in Table 5.1.6.2.11-1 Only EutraLocation data or NrLocation data in UserLocation data is applicable in UeTrajectoryInfo data type. |
|  |  |
| ***Consequences if not approved:*** | NEF can not handle the correct mapping of user location related to n3gaLocation data, NWDAF also can not handle the n3gaLocation data for UE Mobility analytics. |
|  |  |
| ***Clauses affected:*** | 5.1.6.2.11 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI files. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

##### 5.1.6.2.11 Type: UeTrajectoryInfo

Table 5.1.6.2.11-1: Definition of type UeTrajectoryInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| ts | DateTime | M | 1 | Identifies the timestamp when the UE enters this area. |  |
| location | UserLocation | M | 1 | Includes the location of the UE. (NOTE) |  |
| NOTE: Only EutraLocation data or NrLocation data in UserLocation data is applicable. |

\*\*\* End of Changes \*\*\*