**3GPP TSG-CT WG3 Meeting #114eC3-211516**

**E-Meeting, 24th February– 5th March 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of OpenAPI version and TS version in externalDocs field | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** | C3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CRs modifying the Npcf\_PolicyAuthorization API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.  The following agreed CRs update the OpenAPI file for Npcf\_PolicyAuthorization for the present release:   * CR# 0286 impacts the OpenAPI file with a backwards compatible correction.   The API version needs to be upated from 1.0.4 to 1.0.5, and the TS version in the externalDocs field from 15.7.0 to 15.9.0. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Update of the API version number and TS version in externalDocs field for Npcf\_PolicyAuthorization API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and TS version in externalDocs field. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# A.2 Npcf\_PolicyAuthorization API

openapi: 3.0.0

info:

title: Npcf\_PolicyAuthorization Service API

version: 1.0.5

description: |

PCF Policy Authorization Service.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.514 V15.9.0; 5G System; Policy Authorization Service;Stage 3.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.514/'

#

servers:

- url: '{apiRoot}/npcf-policyauthorization/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- npcf-policyauthorization

paths:

/app-sessions:

post:

summary: Creates a new Individual Application Session Context resource

operationId: PostAppSessions

tags:

- Application Sessions (Collection)

requestBody:

description: Contains the information for the creation the resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

responses:

'201':

description: Successful creation of the resource

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

headers:

Location:

description: 'Contains the URI of the created individual application session context resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId} or the URI of the created events subscription sub-resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

required: true

schema:

type: string

'303':

description: See Other. The result of the HTTP POST request would be equivalent to the existing Application Session Context.

headers:

Location:

description: 'Contains the URI of the existing individual Application Session Context resource.'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

headers:

Retry-After:

description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

schema:

anyOf:

- type: integer

- type: string

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

terminationRequest:

'{$request.body#/ascReqData/notifUri}/terminate':

post:

requestBody:

description: Request of the termination of the Individual Application Session Context

content:

application/json:

schema:

$ref: '#/components/schemas/TerminationInfo'

responses:

'204':

description: The receipt of the notification is acknowledged.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

eventNotification:

'{$request.body#/ascReqData/evSubsc/notifUri}/notify':

post:

requestBody:

description: Notification of an event occurrence in the PCF.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/app-sessions/{appSessionId}:

get:

summary: "Reads an existing Individual Application Session Context"

operationId: GetAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: string identifying the resource

in: path

required: true

schema:

type: string

responses:

'200':

description: A representation of the resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: "Modifies an existing Individual Application Session Context"

operationId: ModAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: string identifying the resource

in: path

required: true

schema:

type: string

requestBody:

description: modification of the resource.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AppSessionContextUpdateData'

responses:

'200':

description: successful modification of the resource and a representation of that resource is returned

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'204':

description: The successful modification

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden

content:

application/problem+json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

headers:

Retry-After:

description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

schema:

anyOf:

- type: integer

- type: string

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

eventNotification:

'{$request.body#/evSubsc/notifUri}/notify':

post:

requestBody:

description: Notification of an event occurrence in the PCF.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

#

/app-sessions/{appSessionId}/delete:

post:

summary: "Deletes an existing Individual Application Session Context"

operationId: DeleteAppSession

tags:

- Individual Application Session Context (Document)

parameters:

- name: appSessionId

description: string identifying the Individual Application Session Context resource

in: path

required: true

schema:

type: string

requestBody:

description: deletion of the Individual Application Session Context resource, req notification

required: false

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscReqData'

responses:

'200':

description: The deletion of the resource is confirmed and a resource is returned

content:

application/json:

schema:

$ref: '#/components/schemas/AppSessionContext'

'204':

description: The deletion is confirmed without returning additional data.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

/app-sessions/{appSessionId}/events-subscription:

put:

summary: "creates or modifies an Events Subscription subresource"

operationId: updateEventsSubsc

tags:

- Events Subscription (Document)

parameters:

- name: appSessionId

description: string identifying the Events Subscription resource

in: path

required: true

schema:

type: string

requestBody:

description: Creation or modification of an Events Subscription resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscReqData'

responses:

'201':

description: The creation of the Events Subscription sub-resource is confirmed and its representation is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscPutData'

headers:

Location:

description: 'Contains the URI of the created Events Subscription resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

required: true

schema:

type: string

'200':

description: The modification of the Events Subscription sub-resource is confirmed and its representation is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsSubscPutData'

'204':

description: The modification of the Events Subscription subresource is confirmed without returning additional data.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

eventNotification:

'{$request.body#/notifUri}/notify':

post:

requestBody:

description: Contains the information for the notification of an event occurrence in the PCF.

content:

application/json:

schema:

$ref: '#/components/schemas/EventsNotification'

responses:

'204':

description: The receipt of the notification is acknowledged.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: deletes the Events Subscription subresource

operationId: DeleteEventsSubsc

tags:

- Events Subscription (Document)

parameters:

- name: appSessionId

description: string identifying the Individual Application Session Context resource

in: path

required: true

schema:

type: string

responses:

'204':

description: The deletion of the of the Events Subscription sub-resource is confirmed without returning additional data.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-policyauthorization: Access to the Npcf\_PolicyAuthorization API

schemas:

AppSessionContext:

description: Represents an Individual Application Session Context resource.

type: object

properties:

ascReqData:

$ref: '#/components/schemas/AppSessionContextReqData'

ascRespData:

$ref: '#/components/schemas/AppSessionContextRespData'

evsNotif:

$ref: '#/components/schemas/EventsNotification'

AppSessionContextReqData:

description: Identifies the service requirements of an Individual Application Session Context.

type: object

required:

- notifUri

- suppFeat

oneOf:

- required: [ueIpv4]

- required: [ueIpv6]

- required: [ueMac]

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirement'

aspId:

$ref: '#/components/schemas/AspId'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

evSubsc:

$ref: '#/components/schemas/EventsSubscReqData'

medComponents:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaComponent'

minProperties: 1

ipDomain:

type: string

mpsId:

description: indication of MPS service request

type: string

resPrio:

$ref: '#/components/schemas/ReservPriority'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

sliceInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

sponId:

$ref: '#/components/schemas/SponId'

sponStatus:

$ref: '#/components/schemas/SponsoringStatus'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

ueIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

AppSessionContextRespData:

description: Describes the authorization data of an Individual Application Session Context created by the PCF.

type: object

properties:

servAuthInfo:

$ref: '#/components/schemas/ServAuthInfo'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

AppSessionContextUpdateData:

description: Identifies the modifications to an Individual Application Session Context and may include the modifications to the sub-resource Events Subscription.

type: object

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirementRm'

aspId:

$ref: '#/components/schemas/AspId'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

evSubsc:

$ref: '#/components/schemas/EventsSubscReqDataRm'

medComponents:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaComponentRm'

minProperties: 1

mpsId:

description: indication of MPS service request

type: string

resPrio:

$ref: '#/components/schemas/ReservPriority'

sponId:

$ref: '#/components/schemas/SponId'

sponStatus:

$ref: '#/components/schemas/SponsoringStatus'

EventsSubscReqData:

description: Identifies the events the application subscribes to.

type: object

required:

- events

properties:

events:

type: array

items:

$ref: '#/components/schemas/AfEventSubscription'

minItems: 1

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

usgThres:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

EventsSubscReqDataRm:

description: this data type is defined in the same way as the EventsSubscReqData data type, but with the OpenAPI nullable property set to true.

type: object

required:

- events

properties:

events:

type: array

items:

$ref: '#/components/schemas/AfEventSubscription'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

usgThres:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

nullable: true

MediaComponent:

description: Identifies a media component.

type: object

required:

- medCompN

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirement'

contVer:

$ref: '#/components/schemas/ContentVersion'

codecs:

type: array

items:

$ref: '#/components/schemas/CodecData'

minItems: 1

maxItems: 2

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

medCompN:

type: integer

medSubComps:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaSubComponent'

minProperties: 1

medType:

$ref: '#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

resPrio:

$ref: '#/components/schemas/ReservPriority'

MediaComponentRm:

description: This data type is defined in the same way as the MediaComponent data type, but with the OpenAPI nullable property set to true

type: object

required:

- medCompN

properties:

afAppId:

$ref: '#/components/schemas/AfAppId'

afRoutReq:

$ref: '#/components/schemas/AfRoutingRequirementRm'

contVer:

$ref: '#/components/schemas/ContentVersion'

codecs:

type: array

items:

$ref: '#/components/schemas/CodecData'

minItems: 1

maxItems: 2

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

medCompN:

type: integer

medSubComps:

type: object

additionalProperties:

$ref: '#/components/schemas/MediaSubComponentRm'

minProperties: 1

medType:

$ref: '#/components/schemas/MediaType'

mirBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

mirBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

resPrio:

$ref: '#/components/schemas/ReservPriority'

nullable: true

MediaSubComponent:

description: Identifies a media subcomponent

type: object

required:

- fNum

properties:

ethfDescs:

type: array

items:

$ref: '#/components/schemas/EthFlowDescription'

minItems: 1

maxItems: 2

fNum:

type: integer

fDescs:

type: array

items:

$ref: '#/components/schemas/FlowDescription'

minItems: 1

maxItems: 2

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

tosTrCl:

$ref: '#/components/schemas/TosTrafficClass'

flowUsage:

$ref: '#/components/schemas/FlowUsage'

MediaSubComponentRm:

description: This data type is defined in the same way as the MediaSubComponent data type, but with the OpenAPI nullable property set to true. Removable attributes marBwDl and marBwUl are defined with the corresponding removable data type.

type: object

required:

- fNum

properties:

ethfDescs:

type: array

items:

$ref: '#/components/schemas/EthFlowDescription'

minItems: 1

maxItems: 2

nullable: true

fNum:

type: integer

fDescs:

type: array

items:

$ref: '#/components/schemas/FlowDescription'

minItems: 1

maxItems: 2

nullable: true

fStatus:

$ref: '#/components/schemas/FlowStatus'

marBwDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

marBwUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

tosTrCl:

$ref: '#/components/schemas/TosTrafficClassRm'

flowUsage:

$ref: '#/components/schemas/FlowUsage'

nullable: true

EventsNotification:

description: describes the notification of a matched event

type: object

required:

- evSubsUri

- evNotifs

properties:

accessType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

anGwAddr:

$ref: '#/components/schemas/AnGwAddress'

evSubsUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

evNotifs:

type: array

items:

$ref: '#/components/schemas/AfEventNotification'

minItems: 1

failedResourcAllocReports:

type: array

items:

$ref: '#/components/schemas/ResourcesAllocationInfo'

minItems: 1

plmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

qncReports:

type: array

items:

$ref: '#/components/schemas/QosNotificationControlInfo'

minItems: 1

ratType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

usgRep:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

AfEventSubscription:

description: describes the event information delivered in the subscription

type: object

required:

- event

properties:

event:

$ref: '#/components/schemas/AfEvent'

notifMethod:

$ref: '#/components/schemas/AfNotifMethod'

AfEventNotification:

description: describes the event information delivered in the notification

type: object

required:

- event

properties:

event:

$ref: '#/components/schemas/AfEvent'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

TerminationInfo:

description: indicates the cause for requesting the deletion of the Individual Application Session Context resource

type: object

required:

- termCause

- resUri

properties:

termCause:

$ref: '#/components/schemas/TerminationCause'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

AfRoutingRequirement:

description: describes the event information delivered in the subscription

type: object

properties:

appReloc:

type: boolean

routeToLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

spVal:

$ref: '#/components/schemas/SpatialValidity'

tempVals:

type: array

items:

$ref: '#/components/schemas/TemporalValidity'

minItems: 1

upPathChgSub:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

SpatialValidity:

description: describes explicitly the route to an Application location

type: object

required:

- presenceInfoList

properties:

presenceInfoList:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

SpatialValidityRm:

description: this data type is defined in the same way as the SpatialValidity data type, but with the OpenAPI nullable property set to true

type: object

required:

- presenceInfoList

properties:

presenceInfoList:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

minProperties: 1

nullable: true

AfRoutingRequirementRm:

description: this data type is defined in the same way as the AfRoutingRequirement data type, but with the OpenAPI nullable property set to true and the spVal and tempVals attributes defined as removable.

type: object

properties:

appReloc:

type: boolean

routeToLocs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

nullable: true

spVal:

$ref: '#/components/schemas/SpatialValidityRm'

tempVals:

type: array

items:

$ref: '#/components/schemas/TemporalValidity'

minItems: 1

nullable: true

upPathChgSub:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

nullable: true

AnGwAddress:

description: describes the address of the access network gateway control node

type: object

anyOf:

- required: [anGwIpv4Addr]

- required: [anGwIpv6Addr]

properties:

anGwIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

anGwIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

Flows:

description: Identifies the flows

type: object

required:

- medCompN

properties:

contVers:

type: array

items:

$ref: '#/components/schemas/ContentVersion'

minItems: 1

fNums:

type: array

items:

type: integer

minItems: 1

medCompN:

type: integer

EthFlowDescription:

description: Identifies an Ethernet flow

type: object

required:

- ethType

properties:

destMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

ethType:

type: string

fDesc:

$ref: '#/components/schemas/FlowDescription'

fDir:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowDirection'

sourceMacAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

vlanTags:

type: array

items:

type: string

minItems: 1

maxItems: 2

ResourcesAllocationInfo:

description: describes the status of the PCC rule(s) related to certain media components.

type: object

required:

- mcResourcStatus

properties:

mcResourcStatus:

$ref: '#/components/schemas/MediaComponentResourcesStatus'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

TemporalValidity:

description: Indicates the time interval(s) during which the AF request is to be applied

type: object

properties:

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

stopTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

QosNotificationControlInfo:

description: Indicates whether the QoS targets for a GRB flow are not guaranteed or guaranteed again

type: object

required:

- notifType

properties:

notifType:

$ref: '#/components/schemas/QosNotifType'

flows:

type: array

items:

$ref: '#/components/schemas/Flows'

minItems: 1

#

#

EventsSubscPutData:

description: Identifies the events the application subscribes to within an Events Subscription sub-resource data. It may contain the notification of the already met events

anyOf:

- $ref: '#/components/schemas/EventsSubscReqData'

- $ref: '#/components/schemas/EventsNotification'

#

#

# SIMPLE DATA TYPES

#

AfAppId:

description: Contains an AF application identifier.

type: string

AspId:

description: Contains an identity of an application service provider.

type: string

CodecData:

description: Contains codec related information.

type: string

ContentVersion:

description: Represents the content version of some content.

type: integer

FlowDescription:

description: Defines a packet filter of an IP flow.

type: string

SponId:

description: Contains an identity of a sponsor.

type: string

TosTrafficClass:

description: 2-octet string, where each octet is encoded in hexadecimal representation. The first octet contains the IPv4 Type-of-Service or the IPv6 Traffic-Class field and the second octet contains the ToS/Traffic Class mask field.

type: string

TosTrafficClassRm:

description: this data type is defined in the same way as the TosTrafficClass data type, but with the OpenAPI nullable property set to true

type: string

nullable: true

#

# ENUMERATIONS DATA TYPES

#

MediaType:

anyOf:

- type: string

enum:

- AUDIO

- VIDEO

- DATA

- APPLICATION

- CONTROL

- TEXT

- MESSAGE

- OTHER

- type: string

#

ReservPriority:

anyOf:

- type: string

enum:

- PRIO\_1

- PRIO\_2

- PRIO\_3

- PRIO\_4

- PRIO\_5

- PRIO\_6

- PRIO\_7

- PRIO\_8

- PRIO\_9

- PRIO\_10

- PRIO\_11

- PRIO\_12

- PRIO\_13

- PRIO\_14

- PRIO\_15

- PRIO\_16

- type: string

#

ServAuthInfo:

anyOf:

- type: string

enum:

- TP\_NOT\_KNOWN

- TP\_EXPIRED

- TP\_NOT\_YET\_OCURRED

- type: string

#

SponsoringStatus:

anyOf:

- type: string

enum:

- SPONSOR\_DISABLED

- SPONSOR\_ENABLED

- type: string

#

AfEvent:

anyOf:

- type: string

enum:

- ACCESS\_TYPE\_CHANGE

- FAILED\_RESOURCES\_ALLOCATION

- PLMN\_CHG

- QOS\_NOTIF

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- USAGE\_REPORT

- type: string

#

AfNotifMethod:

anyOf:

- type: string

enum:

- EVENT\_DETECTION

- ONE\_TIME

- type: string

#

QosNotifType:

anyOf:

- type: string

enum:

- GUARANTEED

- NOT\_GUARANTEED

- type: string

#

TerminationCause:

anyOf:

- type: string

enum:

- ALL\_SDF\_DEACTIVATION

- PDU\_SESSION\_TERMINATION

- type: string

#

MediaComponentResourcesStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

#

#

FlowUsage:

anyOf:

- type: string

enum:

- NO\_INFO

- RTCP

- type: string

FlowStatus:

anyOf:

- type: string

enum:

- ENABLED-UPLINK

- ENABLED-DOWNLINK

- ENABLED

- DISABLED

- REMOVED

- type: string

\*\*\* End of Changes \*\*\*