**3GPP TSG-CT3 Meeting #114e C3-211545**

**E-Meeting, 24th February – 05th March 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of OpenAPI version and TS version in externalDocs field | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | China Mobile Communications Group Co.,Ltd | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17 | | | | |  | ***Date:*** | | | 2021-03-09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CRs modifying Nbsf\_Management API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.  The following agreed CRs update the Nbsf\_Management API for the present release:  - TS 29.521 CR #0094 is a backward compatible corrrection in Rel-16.  - TS 29.521 CR #0097 is a backward compatible corrrection in Rel-17.  As some backward compatible correction (but no backward incompatible changes or backward compatible new features) are added of the new release, the minor version number and a draft field need to be assigned for the new release, and the draft version number will be assigned.  Since a new TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The Nnwdaf\_EventsSubscription API version incremented from value "1.1.0" to value "1.2.0-alpha.1".  The TS version number in the "description" field of the "externalDocs" object is changed to "17.0.0". | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible changes to Nbsf\_Management API | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# A.2 Nbsf\_Management API

openapi: 3.0.0

info:

version: 1.2.0-alpha.1

title: Nbsf\_Management

description: |

Binding Support Management Service API.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.521 V17.0.0; 5G System; Binding Support Management Service.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.521/'

servers:

- url: '{apiRoot}/nbsf-management/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

- {}

- oAuth2ClientCredentials:

- nbsf-management

paths:

/pcfBindings:

post:

summary: Create a new Individual PCF binding information

operationId: CreatePCFBinding

tags:

- PCF Bindings (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PcfBinding'

responses:

'201':

description: The creation of an individual PCF session binding.

content:

application/json:

schema:

$ref: '#/components/schemas/PcfBinding'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nbsf-management/v1/pcfBindings/{bindingId}'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: The existing PCF binding information stored in the BSF for the indicated combination is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ExtProblemDetails'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Read PCF Bindings information

operationId: GetPCFBindings

tags:

- PCF Bindings (Collection)

parameters:

- name: ipv4Addr

in: query

description: The IPv4 Address of the served UE.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

- name: ipv6Prefix

in: query

description: The IPv6 Address of the served UE. The NF service consumer shall append '/128' to the IPv6 address in the attribute value. E.g. '2001:db8:85a3::8a2e:370:7334/128'.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

- name: macAddr48

in: query

description: The MAC Address of the served UE.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

- name: dnn

in: query

description: DNN.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

- name: supi

in: query

description: Subscription Permanent Identifier.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

- name: gpsi

in: query

description: Generic Public Subscription Identifier

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

- name: snssai

in: query

description: The identification of slice.

required: false

content:

application/json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

- name: ipDomain

in: query

description: The IPv4 address domain identifier.

required: false

schema:

type: string

- name: supp-feat

in: query

description: To filter irrelevant responses related to unsupported features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The individual PCF session binding session binding information resource matching the query parameter(s) is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PcfBinding'

'204':

description: There is no PCF session binding information matching the query parameter(s).

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/pcfBindings/{bindingId}:

delete:

summary: Delete an existing Individual PCF Binding information

operationId: DeleteIndPCFBinding

tags:

- Individual PCF Binding (Document)

parameters:

- name: bindingId

in: path

description: Represents the individual PCF Session Binding.

required: true

schema:

type: string

responses:

'204':

description: No Content. The Individual PCF session binding information resource is deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Update an existing Individual PCF Binding information

operationId: UpdateIndPCFBinding

tags:

- Individual PCF Binding (Document)

parameters:

- name: bindingId

in: path

description: Represents the individual PCF Session Binding.

required: true

schema:

type: string

requestBody:

description: Parameters to update the existing session binding

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/PcfBindingPatch'

responses:

'200':

description: OK (Successful update of the session binding)

content:

application/json:

schema:

$ref: '#/components/schemas/PcfBinding'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nbsf-management: Access to the Nbsf\_Management API

schemas:

PcfBinding:

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Prefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

addIpv6Prefixes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

minItems: 1

description: The additional IPv6 Address Prefixes of the served UE.

ipDomain:

type: string

macAddr48:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

addMacAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

description: The additional MAC Addresses of the served UE.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

pcfFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

pcfIpEndPoints:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

minItems: 1

description: IP end points of the PCF hosting the Npcf\_PolicyAuthorization service.

pcfDiamHost:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DiameterIdentity'

pcfDiamRealm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DiameterIdentity'

pcfSmFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

pcfSmIpEndPoints:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

minItems: 1

description: IP end points of the PCF hosting the Npcf\_SMPolicyControl service.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

pcfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

pcfSetId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

recoveryTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

paraCom:

$ref: '#/components/schemas/ParameterCombination'

bindLevel:

$ref: '#/components/schemas/BindingLevel'

ipv4FrameRouteList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4AddrMask'

minItems: 1

ipv6FrameRouteList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

minItems: 1

required:

- dnn

- snssai

oneOf:

- anyOf:

- required: [ipv4Addr]

- required: [ipv6Prefix]

- required: [addIpv6Prefixes]

- anyOf:

- required: [macAddr48]

- required: [addMacAddrs]

anyOf:

- anyOf:

- required: [pcfFqdn]

- required: [pcfIpEndPoints]

- required: [pcfDiamHost, pcfDiamRealm]

PcfBindingPatch:

type: object

properties:

ipv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4AddrRm'

ipDomain:

type: string

nullable: true

ipv6Prefix:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6PrefixRm'

addIpv6Prefixes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

minItems: 1

description: The additional IPv6 Address Prefixes of the served UE.

nullable: true

macAddr48:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48Rm'

addMacAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

description: The additional MAC Addresses of the served UE.

nullable: true

pcfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

pcfFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

pcfIpEndPoints:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

minItems: 1

description: IP end points of the PCF hosting the Npcf\_PolicyAuthorization service.

pcfDiamHost:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DiameterIdentity'

pcfDiamRealm:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DiameterIdentity'

ParameterCombination:

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

ExtProblemDetails:

allOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/BindingResp'

BindingResp:

type: object

properties:

pcfSmFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

pcfSmIpEndPoints:

type: array

items:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

minItems: 1

description: IP end points of the PCF hosting the Npcf\_SMPolicyControl service.

BindingLevel:

anyOf:

- type: string

enum:

- NF\_SET

- NF\_INSTANCE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- "NF\_SET"

- "NF\_INSTANCE"

\*\*\* End of Changes \*\*\*