**3GPP TSG-CT3 Meeting #114e C3-211546**

**E-Meeting, 24th February – 05th March 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.549** | **CR** | **0018** | **rev** | - | **Current version:** | **16.2.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of OpenAPI version and TS version in externalDocs field | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17 | | | | |  | ***Date:*** | | | 2021-03-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | CR (CR#0015, TS 29.549, C3-211485) modifying the following APIs is agreed. The version number of the corresponding Open API files thus need to be updated following the rules in TS 29.501, clause 4.3.1.   * SS\_LocationReporting, SS\_GroupManagement, SS\_UserProfileRetrieval, SS\_NetworkResourceAdapatation, SS\_Events, SS\_KeyInfoRetrieval   The agreed CR introduces backward compatible changes to the above APIs and this is the first change introduced in Rel-17. Hence the 2nd minor version needs to be updated with “alpha.1” appended. The TS version number included in the "description" field of the "externalDocs" object also needs to be updated to Rel-17 version of the TS 29.549 where this CR will be applied, i.e. v17.0.0. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The SS\_LocationReporting API   * Version incremented from value "1.0.0" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   The SS\_GroupManagement API   * Version incremented from value "1.0.1" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   The SS\_UserProfileRetrieval API   * Version incremented from value "1.0.0" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   The SS\_NetworkResourceAdaptation API   * Version incremented from value "1.0.1" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   The SS\_Events API   * Version incremented from value "1.0.1" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   The SS\_KeyInfoRetrieval API   * Version incremented from value "1.0.1" to value "1.1.0-alpha.1". * TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”   Copyright year updated to 2021 for all the above updated OpenAPIs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect OpenAPI version and TS version in the OpenAPI file. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.2, A.3, A.4, A.5, A.6, A.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* First Change \* \* \* \*

## A.2 SS\_LocationReporting API

openapi: 3.0.0

info:

title: SS\_LocationReporting

description: |

API for SEAL Location Reporting Configuration.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: "1.1.0-alpha.1"

externalDocs:

description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-lr/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

/trigger-configurations:

post:

description: Creates a new location reporting configuration.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/LocationReportConfiguration'

responses:

'201':

description: location reporting confirguation resource is created sucessfully.

content:

application/json:

schema:

$ref: '#/components/schemas/LocationReportConfiguration'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/trigger-configurations/{configurationId}:

get:

description: Retrieves an individual SEAL location reporting configuration information

parameters:

- name: configurationId

in: path

description: String identifying an individual configuration resource

required: true

schema:

type: string

responses:

'200':

description: The location reporting configuration information.

content:

application/json:

schema:

$ref: '#/components/schemas/LocationReportConfiguration'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

description: Updates an individual SEAL location reporting configuration.

parameters:

- name: configurationId

in: path

description: String identifying an individual configuration resource

required: true

schema:

type: string

requestBody:

description: configuration information to be updated in location management server.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/LocationReportConfiguration'

responses:

'200':

description: the configuration is updated successfully

content:

application/json:

schema:

$ref: '#/components/schemas/LocationReportConfiguration'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

description: Deletes an individual SEAL location reporting configuration.

parameters:

- name: configurationId

in: path

description: String identifying an individual configuration resource

required: true

schema:

type: string

responses:

'204':

description: The individual configuration matching configurationId is deleted.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

LocationReportConfiguration:

type: object

properties:

valServerId:

type: string

valTgtUe:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

immRep:

type: boolean

monDur:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

accuracy:

$ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/Accuracy'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- valServerId

- valTgtUe

\* \* \* Next of Change \* \* \* \*

## A.3 SS\_GroupManagement API

openapi: 3.0.0

info:

title: SS\_GroupManagement

description: |

API for SEAL Group management.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: "1.1.0-alpha.1"

externalDocs:

description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-gm/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

/group-documents:

post:

description: Creates a new VAL group document.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/VALGroupDocument'

responses:

'201':

description: VAL group created sucessfully.

content:

application/json:

schema:

$ref: '#/components/schemas/VALGroupDocument'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

get:

description: Retrieves VAL group documents satisfying filter criteria

parameters:

- name: val-group-id

in: query

description: String identifying the VAL group.

schema:

type: string

- name: val-service-id

in: query

description: String identifying the Val service.

schema:

type: string

responses:

'200':

description: List of VAL group documents matching the query parameters in the request.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/VALGroupDocument'

minItems: 0

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/group-documents/{groupDocId}:

get:

description: Retrieves VAL group information satisfying filter criteria

parameters:

- name: groupDocId

in: path

description: String identifying an individual VAL group document resource

required: true

schema:

type: string

- name: group-members

in: query

description: When set to true indicates the group management server to send the members list information of the VAL group.

schema:

type: boolean

- name: group-configuration

in: query

description: When set to true indicates the group management server to send the group configuration information of the VAL group.

schema:

type: boolean

responses:

'200':

description: The VAL group information based on the request from the VAL server. Includes VAL group members list if group-members flag is set to true in the request, VAL group configuration information if the group-configuration flag is set to true in the request, VAL group identifier, whole VAL group document resource if both group-members and group-configuration flags are omitted/set to false in the request.

content:

application/json:

schema:

$ref: '#/components/schemas/VALGroupDocument'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

description: Updates an individual VAL group document.

parameters:

- name: groupDocId

in: path

description: String identifying an individual VAL group document resource

required: true

schema:

type: string

requestBody:

description: VAL group document to be updated in Group management server.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/VALGroupDocument'

responses:

'200':

description: VAL group document updated successfully

content:

application/json:

schema:

$ref: '#/components/schemas/VALGroupDocument'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

description: Deletes a VAL Group.

parameters:

- name: groupDocId

in: path

description: String identifying an individual VAL group document resource

required: true

schema:

type: string

responses:

'204':

description: The individual VAL group matching groupDocId was deleted.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

VALGroupDocument:

type: object

properties:

valGroupId:

type: string

description: The VAL group idenitity.

grpDesc:

type: string

description: The text description of the VAL group.

members:

type: array

description: The list of VAL User IDs or VAL UE IDs, which are members of the VAL group.

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

valGrpConf:

type: string

description: Configuration data for the VAL group.

valServiceIds:

type: array

description: The list of VAL services enabled on the group.

items:

type: string

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

locInfo:

$ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/LocationInfo'

addLocInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

required:

- valGroupId

\* \* \* Next of Change \* \* \* \*

## A.4 SS\_UserProfileRetrieval API

openapi: 3.0.0

info:

title: SS\_UserProfileRetrieval

description: |

API for SEAL User Profile Retrieval.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: "1.1.0-alpha.1"

externalDocs:

description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-upr/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

/val-services:

get:

description: Retrieve VAL User or VAL UE profile information.

parameters:

- name: val-service-id

in: query

description: String identifying an individual VAL service

required: false

schema:

type: string

- name: val-tgt-ue

in: query

description: Identifying a VAL target UE.

required: true

schema:

$ref: '#/components/schemas/ValTargetUe'

responses:

'200':

description: The Profile information of the VAL User or VAL UE.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ProfileDoc'

minItems: 0

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

ProfileDoc:

type: object

properties:

profileInformation:

type: string

description: Profile information associated with the valUserId or valUeId.

valTgtUe:

$ref: '#/components/schemas/ValTargetUe'

required:

- profileInformation

- valTgtUe

ValTargetUe:

type: object

properties:

valUserId:

type: string

description: Unique identifier of a VAL user.

valUeId:

type: string

description: Unique identifier of a VAL UE.

oneOf:

- required: [valUserId]

- required: [valUeId]

\* \* \* Next of Change \* \* \* \*

## A.5 SS\_NetworkResourceAdaptation API

openapi: 3.0.0

info:

version: 1.1.0-alpha.1

title: SS\_NetworkResourceAdaptation

description: |

SS Network Resource Adaptation Service.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.549 V17.0.0; Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-nra/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

paths:

/multicast-subscriptions:

post:

summary: Creates a new Individual Multicast Subscription resource

operationId: CreateMulticastSubscription

tags:

- Multicast Subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MulticastSubscription'

responses:

'201':

description: Success

content:

application/json:

schema:

$ref: '#/components/schemas/MulticastSubscription'

headers:

Location:

description: 'Contains the URI of the created individual multicast subscription resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

UserPlaneNotification:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotification'

responses:

'204':

description: No Content, Notification was succesfull

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/multicast-subscriptions/{multiSubId}:

get:

summary: "Reads an existing Individual Multicast Subscription"

operationId: GetMulticastSubscription

tags:

- Individual Multicast Subscription (Document)

parameters:

- name: multiSubId

in: path

description: Multicast Subscription ID

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/MulticastSubscription'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: "Delete an existing Individual Multicast Subscription"

operationId: DeleteMulticastSubscription

tags:

- Individual Multicast Subscription (Document)

parameters:

- name: multiSubId

in: path

description: Multicast Subscription ID

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was succesfully deleted

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/unicast-subscriptions:

post:

summary: Creates a new Individual Unicast Subscription resource

operationId: CreateUnicastSubscription

tags:

- Unicast Subscriptions (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UnicastSubscription'

responses:

'201':

description: Success

content:

application/json:

schema:

$ref: '#/components/schemas/UnicastSubscription'

headers:

Location:

description: 'Contains the URI of the created individual unicast subscription resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

UserPlaneNotification:

'{$request.body#/notifUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotification'

responses:

'204':

description: No Content, Notification was succesfull

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/unicast-subscriptions/{uniSubId}:

get:

summary: "Reads an existing Individual Unicast Subscription"

operationId: GetUnicastSubscription

tags:

- Individual Unicast Subscription (Document)

parameters:

- name: uniSubId

in: path

description: Unicast Subscription ID

required: true

schema:

type: string

responses:

'200':

description: OK. Resource representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/UnicastSubscription'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: "Delete an existing Individual Unicast Subscription"

operationId: DeleteUnicastSubscription

tags:

- Individual Unicast Subscription (Document)

parameters:

- name: uniSubId

in: path

description: Unicast Subscription ID

required: true

schema:

type: string

responses:

'204':

description: No Content. Resource was succesfully deleted

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

MulticastSubscription:

type: object

properties:

valGroupId:

type: string

anncMode:

$ref: '#/components/schemas/ServiceAnnoucementMode'

multiQosReq:

type: string

locArea:

$ref: 'TS29122\_GMDviaMBMSbyMB2.yaml#/components/schemas/MbmsLocArea'

duration:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

tmgi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

reqTestNotif:

type: boolean

wsNotifCfg:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

upIpv4Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

upIpv6Addr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

upPortNum:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

radioFreqs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

minItems: 1

required:

- valGroupId

- anncMode

- multiQosReq

- notifUri

UnicastSubscription:

type: object

properties:

valTgtUe:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

uniQosReq:

type: string

duration:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

reqTestNotif:

type: boolean

wsNotifCfg:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- valTgtUe

- notifUri

UserPlaneNotification:

type: object

properties:

notifId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

eventNotifs:

type: array

items:

$ref: '#/components/schemas/NrmEventNotification'

minItems: 1

required:

- notifId

- eventNotifs

NrmEventNotification:

type: object

properties:

event:

$ref: '#/components/schemas/NrmEvent'

ts:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

deliveryMode:

$ref: '#/components/schemas/DeliveryMode'

streamIds:

type: array

items:

type: string

minItems: 1

required:

- event

- ts

# Simple data types and Enumerations

ServiceAnnoucementMode:

anyOf:

- type: string

enum:

- NRM

- VAL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NRM: NRM server performs the service announcement.

- VAL: VAL server performs the service announcement.

DeliveryMode:

anyOf:

- type: string

enum:

- UNICAST

- MULTICAST

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UNICAST: Unicast delivery.

- MULTICAST: Multicast delivery.

NrmEvent:

anyOf:

- type: string

enum:

- UP\_DELIVERY\_MODE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UP\_DELIVERY\_MODE: User Plane delivery mode.

\* \* \* Next of Change \* \* \* \*

## A.6 SS\_Events API

openapi: 3.0.0

info:

title: SS\_Events

description: |

API for SEAL Events management.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: "1.1.0-alpha.1"

externalDocs:

description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-events/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

/subscriptions:

post:

description: Creates a new individual SEAL Event Subscription.

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SEALEventSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SEALEventNotification'

responses:

'204':

description: No Content (successful notification)

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: SEAL Events subscription resource created successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/SEALEventSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

delete:

description: Deletes an individual SEAL Event Subscription.

parameters:

- name: subscriptionId

in: path

description: Identifier of an individual Events Subscription

required: true

schema:

type: string

responses:

'204':

description: The individual SEAL Events Subscription matching the subscriptionId is deleted.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

SEALEventSubscription:

type: object

properties:

subscriberId:

type: string

description: String identifying the subscriber of the event.

eventSubs:

type: array

items:

$ref: '#/components/schemas/EventSubscription'

minItems: 1

description: Subscribed events.

eventReq:

$ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

requestTestNotification:

type: boolean

description: Set to true by Subscriber to request the SEAL server to send a test notification. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

eventDetails:

type: array

items:

$ref: '#/components/schemas/SEALEventDetail'

minItems: 1

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- subscriberId

- eventSubs

- eventReq

- notificationDestination

SEALEventNotification:

type: object

properties:

subscriptionId:

type: string

description: Identifier of the subscription resource.

eventDetails:

type: array

items:

$ref: '#/components/schemas/SEALEventDetail'

minItems: 1

description: Detailed notifications of individual events.

required:

- subscriptionId

- eventDetails

EventSubscription:

type: object

properties:

eventId:

$ref: '#/components/schemas/SEALEvent'

valGroups:

type: array

items:

$ref: '#/components/schemas/VALGroupFilter'

minItems: 1

description: Each element of the array represents the VAL group identifier(s) of a VAL service that the subscriber wants to know in the interested event.

identities:

type: array

items:

$ref: '#/components/schemas/IdentityFilter'

minItems: 1

description: Each element of the array represents the VAL User / UE IDs of a VAL service that the event subscriber wants to know in the interested event.

required:

- eventId

SEALEventDetail:

type: object

properties:

eventId:

$ref: '#/components/schemas/SEALEvent'

lmInfos:

type: array

items:

$ref: '#/components/schemas/LMInformation'

minItems: 1

valGroupDocuments:

type: array

items:

$ref: 'TS29549\_SS\_GroupManagement.yaml#/components/schemas/VALGroupDocument'

minItems: 1

description: The VAL groups documents with modified membership and configuration information.

profileDocs:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ProfileDoc'

minItems: 1

description: Updated profile information associated with VAL Users or VAL UEs.

required:

- eventId

VALGroupFilter:

type: object

properties:

valSvcId:

type: string

description: Identity of the VAL service

valGrpIds:

type: array

items:

type: string

minItems: 1

description: VAL group identifiers that event subscriber wants to know in the interested event.

required:

- valGrpIds

IdentityFilter:

type: object

properties:

valSvcId:

type: string

description: Identity of the VAL service

valTgtUes:

type: array

items:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

minItems: 1

description: VAL User IDs or VAL UE IDs that the event subscriber wants to know in the interested event.

LMInformation:

type: object

properties:

valTgtUe:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

locInfo:

$ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/LocationInfo'

required:

- locInfo

- valTgtUe

SEALEvent:

anyOf:

- type: string

enum:

- LM\_LOCATION\_INFO\_CHANGE

- GM\_GROUP\_INFO\_CHANGE

- CM\_USER\_PROFILE\_CHANGE

- GM\_GROUP\_CREATE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- LM\_LOCATION\_INFO\_CHANGE: Events related to the location information of VAL Users or VAL UEs from the Location Management Server.

- GM\_GROUP\_INFO\_CHANGE: Events related to the modification of VAL group membership and configuration information from the Group Management Server.

- CM\_USER\_PROFILE\_CHANGE: Events related to update of user profile information from the Configuration Management Server.

- GM\_GROUP\_CREATE: Events related to creation of new VAL groups from the Group Mananagement Server.

\* \* \* Next of Change \* \* \* \*

## A.7 SS\_KeyInfoRetrieval API

openapi: 3.0.0

info:

title: SS\_KeyInfoRetrieval

description: |

API for SEAL Key Information Retrieval.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

version: "1.1.0-alpha.1"

externalDocs:

description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/ss-kir/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

/key-records:

get:

description: Retrieve Key mamangement information specific to VAL service.

parameters:

- name: val-service-id

in: query

description: String identifying an individual VAL service

required: true

schema:

type: string

- name: val-tgt-ue

in: query

description: Identifying a VAL target.

required: false

schema:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

responses:

'200':

description: The key management information of the VAL service, VAL User or VAL UE.

content:

application/json:

schema:

$ref: '#/components/schemas/ValKeyInfo'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

ValKeyInfo:

type: object

properties:

userUri:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

skmsId:

type: string

description: String identifying the key management server.

valService:

type: string

description: Unique identifier of a VAL Service.

valTgtUe:

$ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

keyInfo:

type: string

description: Key management information specific to VAL service, VAL User or VAL UE.

required:

- userUri

- valService

- keyInfo

\* \* \* End of Changes \* \* \* \*