**3GPP TSG-CT3 Meeting #114e C3-211546**

**E-Meeting, 24th February – 05th March 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.549** | **CR** | **0018** | **rev** | - | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update of OpenAPI version and TS version in externalDocs field  |
|  |  |
| ***Source to WG:*** | Samsung |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2021-03-08 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CR (CR#0015, TS 29.549, C3-211485) modifying the following APIs is agreed. The version number of the corresponding Open API files thus need to be updated following the rules in TS 29.501, clause 4.3.1.* SS\_LocationReporting, SS\_GroupManagement, SS\_UserProfileRetrieval, SS\_NetworkResourceAdapatation, SS\_Events, SS\_KeyInfoRetrieval

The agreed CR introduces backward compatible changes to the above APIs and this is the first change introduced in Rel-17. Hence the 2nd minor version needs to be updated with “alpha.1” appended. The TS version number included in the "description" field of the "externalDocs" object also needs to be updated to Rel-17 version of the TS 29.549 where this CR will be applied, i.e. v17.0.0. |
|  |  |
| ***Summary of change:*** | The SS\_LocationReporting API * Version incremented from value "1.0.0" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

The SS\_GroupManagement API* Version incremented from value "1.0.1" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

The SS\_UserProfileRetrieval API* Version incremented from value "1.0.0" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

The SS\_NetworkResourceAdaptation API* Version incremented from value "1.0.1" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

The SS\_Events API* Version incremented from value "1.0.1" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

The SS\_KeyInfoRetrieval API* Version incremented from value "1.0.1" to value "1.1.0-alpha.1".
* TS version number in the "description" field of the "externalDocs" object is changed to “17.0.0”

Copyright year updated to 2021 for all the above updated OpenAPIs.  |
|  |  |
| ***Consequences if not approved:*** | Incorrect OpenAPI version and TS version in the OpenAPI file. |
|  |  |
| ***Clauses affected:*** | A.2, A.3, A.4, A.5, A.6, A.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* First Change \* \* \* \*

## A.2 SS\_LocationReporting API

openapi: 3.0.0

info:

 title: SS\_LocationReporting

 description: |

 API for SEAL Location Reporting Configuration.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.1.0-alpha.1"

externalDocs:

 description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-lr/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /trigger-configurations:

 post:

 description: Creates a new location reporting configuration.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/LocationReportConfiguration'

 responses:

 '201':

 description: location reporting confirguation resource is created sucessfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/LocationReportConfiguration'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /trigger-configurations/{configurationId}:

 get:

 description: Retrieves an individual SEAL location reporting configuration information

 parameters:

 - name: configurationId

 in: path

 description: String identifying an individual configuration resource

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The location reporting configuration information.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/LocationReportConfiguration'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Updates an individual SEAL location reporting configuration.

 parameters:

 - name: configurationId

 in: path

 description: String identifying an individual configuration resource

 required: true

 schema:

 type: string

 requestBody:

 description: configuration information to be updated in location management server.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/LocationReportConfiguration'

 responses:

 '200':

 description: the configuration is updated successfully

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/LocationReportConfiguration'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Deletes an individual SEAL location reporting configuration.

 parameters:

 - name: configurationId

 in: path

 description: String identifying an individual configuration resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual configuration matching configurationId is deleted.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 LocationReportConfiguration:

 type: object

 properties:

 valServerId:

 type: string

 valTgtUe:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 immRep:

 type: boolean

 monDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 accuracy:

 $ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/Accuracy'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - valServerId

 - valTgtUe

\* \* \* Next of Change \* \* \* \*

## A.3 SS\_GroupManagement API

openapi: 3.0.0

info:

 title: SS\_GroupManagement

 description: |

 API for SEAL Group management.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.1.0-alpha.1"

externalDocs:

 description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-gm/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /group-documents:

 post:

 description: Creates a new VAL group document.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 responses:

 '201':

 description: VAL group created sucessfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 get:

 description: Retrieves VAL group documents satisfying filter criteria

 parameters:

 - name: val-group-id

 in: query

 description: String identifying the VAL group.

 schema:

 type: string

 - name: val-service-id

 in: query

 description: String identifying the Val service.

 schema:

 type: string

 responses:

 '200':

 description: List of VAL group documents matching the query parameters in the request.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/VALGroupDocument'

 minItems: 0

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /group-documents/{groupDocId}:

 get:

 description: Retrieves VAL group information satisfying filter criteria

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 - name: group-members

 in: query

 description: When set to true indicates the group management server to send the members list information of the VAL group.

 schema:

 type: boolean

 - name: group-configuration

 in: query

 description: When set to true indicates the group management server to send the group configuration information of the VAL group.

 schema:

 type: boolean

 responses:

 '200':

 description: The VAL group information based on the request from the VAL server. Includes VAL group members list if group-members flag is set to true in the request, VAL group configuration information if the group-configuration flag is set to true in the request, VAL group identifier, whole VAL group document resource if both group-members and group-configuration flags are omitted/set to false in the request.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 description: Updates an individual VAL group document.

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 requestBody:

 description: VAL group document to be updated in Group management server.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 responses:

 '200':

 description: VAL group document updated successfully

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VALGroupDocument'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 description: Deletes a VAL Group.

 parameters:

 - name: groupDocId

 in: path

 description: String identifying an individual VAL group document resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual VAL group matching groupDocId was deleted.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 VALGroupDocument:

 type: object

 properties:

 valGroupId:

 type: string

 description: The VAL group idenitity.

 grpDesc:

 type: string

 description: The text description of the VAL group.

 members:

 type: array

 description: The list of VAL User IDs or VAL UE IDs, which are members of the VAL group.

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 minItems: 1

 valGrpConf:

 type: string

 description: Configuration data for the VAL group.

 valServiceIds:

 type: array

 description: The list of VAL services enabled on the group.

 items:

 type: string

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 resUri:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 locInfo:

 $ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/LocationInfo'

 addLocInfo:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

 required:

 - valGroupId

\* \* \* Next of Change \* \* \* \*

## A.4 SS\_UserProfileRetrieval API

openapi: 3.0.0

info:

 title: SS\_UserProfileRetrieval

 description: |

 API for SEAL User Profile Retrieval.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.1.0-alpha.1"

externalDocs:

 description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-upr/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /val-services:

 get:

 description: Retrieve VAL User or VAL UE profile information.

 parameters:

 - name: val-service-id

 in: query

 description: String identifying an individual VAL service

 required: false

 schema:

 type: string

 - name: val-tgt-ue

 in: query

 description: Identifying a VAL target UE.

 required: true

 schema:

 $ref: '#/components/schemas/ValTargetUe'

 responses:

 '200':

 description: The Profile information of the VAL User or VAL UE.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/ProfileDoc'

 minItems: 0

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 ProfileDoc:

 type: object

 properties:

 profileInformation:

 type: string

 description: Profile information associated with the valUserId or valUeId.

 valTgtUe:

 $ref: '#/components/schemas/ValTargetUe'

 required:

 - profileInformation

 - valTgtUe

 ValTargetUe:

 type: object

 properties:

 valUserId:

 type: string

 description: Unique identifier of a VAL user.

 valUeId:

 type: string

 description: Unique identifier of a VAL UE.

 oneOf:

 - required: [valUserId]

 - required: [valUeId]

\* \* \* Next of Change \* \* \* \*

## A.5 SS\_NetworkResourceAdaptation API

openapi: 3.0.0

info:

 version: 1.1.0-alpha.1

 title: SS\_NetworkResourceAdaptation

 description: |

 SS Network Resource Adaptation Service.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.549 V17.0.0; Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-nra/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

paths:

 /multicast-subscriptions:

 post:

 summary: Creates a new Individual Multicast Subscription resource

 operationId: CreateMulticastSubscription

 tags:

 - Multicast Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MulticastSubscription'

 responses:

 '201':

 description: Success

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MulticastSubscription'

 headers:

 Location:

 description: 'Contains the URI of the created individual multicast subscription resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 callbacks:

 UserPlaneNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UserPlaneNotification'

 responses:

 '204':

 description: No Content, Notification was succesfull

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /multicast-subscriptions/{multiSubId}:

 get:

 summary: "Reads an existing Individual Multicast Subscription"

 operationId: GetMulticastSubscription

 tags:

 - Individual Multicast Subscription (Document)

 parameters:

 - name: multiSubId

 in: path

 description: Multicast Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/MulticastSubscription'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: "Delete an existing Individual Multicast Subscription"

 operationId: DeleteMulticastSubscription

 tags:

 - Individual Multicast Subscription (Document)

 parameters:

 - name: multiSubId

 in: path

 description: Multicast Subscription ID

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was succesfully deleted

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /unicast-subscriptions:

 post:

 summary: Creates a new Individual Unicast Subscription resource

 operationId: CreateUnicastSubscription

 tags:

 - Unicast Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UnicastSubscription'

 responses:

 '201':

 description: Success

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UnicastSubscription'

 headers:

 Location:

 description: 'Contains the URI of the created individual unicast subscription resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 callbacks:

 UserPlaneNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UserPlaneNotification'

 responses:

 '204':

 description: No Content, Notification was succesfull

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /unicast-subscriptions/{uniSubId}:

 get:

 summary: "Reads an existing Individual Unicast Subscription"

 operationId: GetUnicastSubscription

 tags:

 - Individual Unicast Subscription (Document)

 parameters:

 - name: uniSubId

 in: path

 description: Unicast Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UnicastSubscription'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: "Delete an existing Individual Unicast Subscription"

 operationId: DeleteUnicastSubscription

 tags:

 - Individual Unicast Subscription (Document)

 parameters:

 - name: uniSubId

 in: path

 description: Unicast Subscription ID

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was succesfully deleted

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 MulticastSubscription:

 type: object

 properties:

 valGroupId:

 type: string

 anncMode:

 $ref: '#/components/schemas/ServiceAnnoucementMode'

 multiQosReq:

 type: string

 locArea:

 $ref: 'TS29122\_GMDviaMBMSbyMB2.yaml#/components/schemas/MbmsLocArea'

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tmgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqTestNotif:

 type: boolean

 wsNotifCfg:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 upIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 upIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 upPortNum:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

 radioFreqs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 minItems: 1

 required:

 - valGroupId

 - anncMode

 - multiQosReq

 - notifUri

 UnicastSubscription:

 type: object

 properties:

 valTgtUe:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 uniQosReq:

 type: string

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqTestNotif:

 type: boolean

 wsNotifCfg:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - valTgtUe

 - notifUri

 UserPlaneNotification:

 type: object

 properties:

 notifId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/NrmEventNotification'

 minItems: 1

 required:

 - notifId

 - eventNotifs

 NrmEventNotification:

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NrmEvent'

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 deliveryMode:

 $ref: '#/components/schemas/DeliveryMode'

 streamIds:

 type: array

 items:

 type: string

 minItems: 1

 required:

 - event

 - ts

# Simple data types and Enumerations

 ServiceAnnoucementMode:

 anyOf:

 - type: string

 enum:

 - NRM

 - VAL

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - NRM: NRM server performs the service announcement.

 - VAL: VAL server performs the service announcement.

 DeliveryMode:

 anyOf:

 - type: string

 enum:

 - UNICAST

 - MULTICAST

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNICAST: Unicast delivery.

 - MULTICAST: Multicast delivery.

 NrmEvent:

 anyOf:

 - type: string

 enum:

 - UP\_DELIVERY\_MODE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UP\_DELIVERY\_MODE: User Plane delivery mode.

\* \* \* Next of Change \* \* \* \*

## A.6 SS\_Events API

openapi: 3.0.0

info:

 title: SS\_Events

 description: |

 API for SEAL Events management.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.1.0-alpha.1"

externalDocs:

 description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-events/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /subscriptions:

 post:

 description: Creates a new individual SEAL Event Subscription.

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SEALEventSubscription'

 callbacks:

 notificationDestination:

 '{request.body#/notificationDestination}':

 post:

 requestBody: # contents of the callback message

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SEALEventNotification'

 responses:

 '204':

 description: No Content (successful notification)

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 responses:

 '201':

 description: SEAL Events subscription resource created successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/SEALEventSubscription'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 delete:

 description: Deletes an individual SEAL Event Subscription.

 parameters:

 - name: subscriptionId

 in: path

 description: Identifier of an individual Events Subscription

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The individual SEAL Events Subscription matching the subscriptionId is deleted.

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 SEALEventSubscription:

 type: object

 properties:

 subscriberId:

 type: string

 description: String identifying the subscriber of the event.

 eventSubs:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events.

 eventReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationDestination:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 requestTestNotification:

 type: boolean

 description: Set to true by Subscriber to request the SEAL server to send a test notification. Set to false or omitted otherwise.

 websockNotifConfig:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 eventDetails:

 type: array

 items:

 $ref: '#/components/schemas/SEALEventDetail'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - subscriberId

 - eventSubs

 - eventReq

 - notificationDestination

 SEALEventNotification:

 type: object

 properties:

 subscriptionId:

 type: string

 description: Identifier of the subscription resource.

 eventDetails:

 type: array

 items:

 $ref: '#/components/schemas/SEALEventDetail'

 minItems: 1

 description: Detailed notifications of individual events.

 required:

 - subscriptionId

 - eventDetails

 EventSubscription:

 type: object

 properties:

 eventId:

 $ref: '#/components/schemas/SEALEvent'

 valGroups:

 type: array

 items:

 $ref: '#/components/schemas/VALGroupFilter'

 minItems: 1

 description: Each element of the array represents the VAL group identifier(s) of a VAL service that the subscriber wants to know in the interested event.

 identities:

 type: array

 items:

 $ref: '#/components/schemas/IdentityFilter'

 minItems: 1

 description: Each element of the array represents the VAL User / UE IDs of a VAL service that the event subscriber wants to know in the interested event.

 required:

 - eventId

 SEALEventDetail:

 type: object

 properties:

 eventId:

 $ref: '#/components/schemas/SEALEvent'

 lmInfos:

 type: array

 items:

 $ref: '#/components/schemas/LMInformation'

 minItems: 1

 valGroupDocuments:

 type: array

 items:

 $ref: 'TS29549\_SS\_GroupManagement.yaml#/components/schemas/VALGroupDocument'

 minItems: 1

 description: The VAL groups documents with modified membership and configuration information.

 profileDocs:

 type: array

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ProfileDoc'

 minItems: 1

 description: Updated profile information associated with VAL Users or VAL UEs.

 required:

 - eventId

 VALGroupFilter:

 type: object

 properties:

 valSvcId:

 type: string

 description: Identity of the VAL service

 valGrpIds:

 type: array

 items:

 type: string

 minItems: 1

 description: VAL group identifiers that event subscriber wants to know in the interested event.

 required:

 - valGrpIds

 IdentityFilter:

 type: object

 properties:

 valSvcId:

 type: string

 description: Identity of the VAL service

 valTgtUes:

 type: array

 items:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 minItems: 1

 description: VAL User IDs or VAL UE IDs that the event subscriber wants to know in the interested event.

 LMInformation:

 type: object

 properties:

 valTgtUe:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 locInfo:

 $ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/LocationInfo'

 required:

 - locInfo

 - valTgtUe

 SEALEvent:

 anyOf:

 - type: string

 enum:

 - LM\_LOCATION\_INFO\_CHANGE

 - GM\_GROUP\_INFO\_CHANGE

 - CM\_USER\_PROFILE\_CHANGE

 - GM\_GROUP\_CREATE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LM\_LOCATION\_INFO\_CHANGE: Events related to the location information of VAL Users or VAL UEs from the Location Management Server.

 - GM\_GROUP\_INFO\_CHANGE: Events related to the modification of VAL group membership and configuration information from the Group Management Server.

 - CM\_USER\_PROFILE\_CHANGE: Events related to update of user profile information from the Configuration Management Server.

 - GM\_GROUP\_CREATE: Events related to creation of new VAL groups from the Group Mananagement Server.

\* \* \* Next of Change \* \* \* \*

## A.7 SS\_KeyInfoRetrieval API

openapi: 3.0.0

info:

 title: SS\_KeyInfoRetrieval

 description: |

 API for SEAL Key Information Retrieval.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

 version: "1.1.0-alpha.1"

externalDocs:

 description: 3GPP TS 29.549 V17.0.0 Service Enabler Architecture Layer for Verticals (SEAL); Application Programming Interface (API) specification; Stage 3.

 url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.549/

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/ss-kir/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 6.5 of 3GPP TS 29.549

paths:

 /key-records:

 get:

 description: Retrieve Key mamangement information specific to VAL service.

 parameters:

 - name: val-service-id

 in: query

 description: String identifying an individual VAL service

 required: true

 schema:

 type: string

 - name: val-tgt-ue

 in: query

 description: Identifying a VAL target.

 required: false

 schema:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 responses:

 '200':

 description: The key management information of the VAL service, VAL User or VAL UE.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ValKeyInfo'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 ValKeyInfo:

 type: object

 properties:

 userUri:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Uri'

 skmsId:

 type: string

 description: String identifying the key management server.

 valService:

 type: string

 description: Unique identifier of a VAL Service.

 valTgtUe:

 $ref: 'TS29549\_SS\_UserProfileRetrieval.yaml#/components/schemas/ValTargetUe'

 keyInfo:

 type: string

 description: Key management information specific to VAL service, VAL User or VAL UE.

 required:

 - userUri

 - valService

 - keyInfo

\* \* \* End of Changes \* \* \* \*