**TSG-CT WG3 Meeting #117-e *C3-214081***

**E-Meeting, 18th – 27th August 2021 (Revision of C3-214xyz)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.214** | **CR** | 1657 | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | 5GS-Level UE identities |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | en5GPccSer17 |  | ***Date:*** | 2021-08-18 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The AF may request the EPC-level identities by including the AF-Requested-Data AVP. But it is not defined how the PCF reports the 5GS-level identities in the case of interworking with 5GS via Rx interface.  |
|  |  |
| ***Summary of change:*** | Defines the procedure to preort the 5GS-Level identities. |
|  |  |
| ***Consequences if not approved:*** | The procedure of PCF reporting the 5GS-level identities in the case of interworking with 5GS via Rx interface is not defined. |
|  |  |
| ***Clauses affected:*** | E.x(new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# E.x 5GS-Level Identities report

The PCF provides 5GS-Level Identities as defined in annex A.1 and A.5 with the following differences:

- the IMSI is included within the Subscription-Id AVP if the IMSI is received within the "supi" attribute;

- the MSISDN is included within the Subscription-Id AVP if the MSISDN is received within the "gpsi" attribute;

- the IMEISV is included with the User-Equipment-Info AVP if the IMEISV is received within the "pei" attribute;

- the IMEI is included with the the User-Equipment-Info-Extension AVP if the User-Equipment-Info-Extension feature is supported and the IMEI is received within the "pei" attribute.

NOTE: UE identities for wireless and wireline convergence access are not considered to be used for the IMS.

Editor’s note: The reporting for NAI is FFS

\*\*\* End of Changes \*\*\*