**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Analytics subscription transfer operation data model and OpenAPI |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | TS 23.288 clause 6.1B has specified how to perform transfer of analytics subscriptions, with the respective functionality added via a new service operation (Nnwdaf\_AnalyticsSubscription\_Transfer, see TS 23.288 clause 7.2.5). This needs to be implemented by extending the Nnwdaf\_EventsSubscription API accordingly. |
|  |  |
| ***Summary of change:*** | Implemented the required data model and OpenAPI to enable analytics subscriptions transfer. |
|  |  |
| ***Consequences if not approved:*** | Stage 2 requirements not fulfilled. |
|  |  |
| ***Clauses affected:*** | 5.1.6.1, 5.1.6.2.XX (new subclause), 5.1.6.2.YY (new subclause), 5.1.6.2.MM (new subclause), 5.1.6.2.PP (new subclause), 5.1.6.2.LL (new subclause), 5.1.6.3.NN (new subclause), A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces a backwards compatible feature in the OpenAPI file of the Nnwdaf\_EventsSubscription API. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First change \* \* \* \*

#### 5.1.6.1 General

This subclause specifies the application data model supported by the API.

Table 5.1.6.1-1 specifies the data types defined for the Nnwdaf\_EventsSubscription service based interface protocol.

Table 5.1.6.1-1: Nnwdaf\_EventsSubscription specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AbnormalBehaviour | 5.1.6.2.15 | Represents the abnormal behaviour information. | AbnormalBehaviour |
| Accuracy | 5.1.6.3.5 | Represents the preferred level of accuracy of the analytics. |  |
| AdditionalMeasurement | 5.1.6.2.26 |  | AbnormalBehaviour |
| AddressList | 5.1.6.2.28 |  | AbnormalBehaviour |
| AnalyticsContextIdentifer | 5.1.6.2.PP | Contains information about available analytics contexts. | EneNA |
| AnalyticsMetadata | 5.1.6.3.14 | Represents the types of analytics metadata information that can be requested. | Aggregation |
| AnalyticsMetadataIndication | 5.1.6.2.36 | Contains analytics metadata values indicated to be used during analytics generation. | Aggregation |
| AnalyticsMetadataInfo | 5.1.6.2.37 | Contains analytics metadata information required for analytics aggregation. | Aggregation |
| AnalyticsSubscriptionsTransfer | 5.1.6.2.XX | Contains information about a request to transfer analytics subscriptions. | EneNA |
| AnySlice | 5.1.6.3.2 | Represents the any slices. |  |
| BwRequirement | 5.1.6.2.25 | Represents bandwidth requirement. | ServiceExperience |
| CircumstanceDescription | 5.1.6.2.29 |  | AbnormalBehaviour |
| CongestionInfo | 5.1.6.2.18 |  | UserDataCongestion |
| CongestionType | 5.1.6.3.8 |  | UserDataCongestion |
| DatasetStatisticalProperty | 5.1.6.3.15 | Dataset statistical properties of the data used to generate the analytics. | Aggregation |
| EventNotification | 5.1.6.2.5 | Describes Notifications about events that occurred. |  |
| EventReportingRequirement | 5.1.6.2.7 | Represents the type of reporting the subscription requires. |  |
| EventSubscription | 5.1.6.2.3 | Represents the subscription to a single event. |  |
| Exception | 5.1.6.2.16 | Describes the Exception information. | AbnormalBehaviour |
| ExceptionId | 5.1.6.3.6 | Describes the Exception Id. | AbnormalBehaviour |
| ExceptionTrend | 5.1.6.3.7 | Describes the Exception Trend. | AbnormalBehaviour |
| ExpectedAnalyticsType | 5.1.6.3.11 |  | AbnormalBehaviour |
| FailureEventInfo | 5.1.6.2.35 | Contains information on the event for which the subscription is not successful. |  |
| IpEthFlowDescription | 5.1.6.2.27 |  | AbnormalBehaviour |
| LoadLevelInformation | 5.1.6.3.2 | Represents load level information of the network slice and the optionally associated network slice instance. |  |
| LocationInfo | 5.1.6.2.11 |  | UeMobility |
| MatchingDirection | 5.1.6.3.12 | Defines the matching direction when crossing a threshold. | NfLoad, QoSSustainability, UserDataCongestion, NetworkPerformance |
| ModelInfo | 5.1.6.2.MM | Contains information about an ML model. | EneNA |
| NetworkPerfInfo | 5.1.6.2.23 |  | NetworkPerformance |
| NetworkPerfRequirement | 5.1.6.2.22 |  | NetworkPerformance |
| NetworkPerfType | 5.1.6.3.10 |  | NetworkPerformance |
| NfLoadLevelInformation | 5.1.6.2.31 | Represents load level information of a given NF instance. | NfLoad |
| NfStatus | 5.1.6.2.32 | Provides the percentage of time spent on various NF states. | NfLoad |
| NwdafEvent | 5.1.6.3.4 | Describes the NWDAF Events. |  |
| NnwdafEventsSubscription | 5.1.6.2.2 | Represents an Individual NWDAF Event Subscription resource. |  |
| NnwdafEventsSubscriptionNotification | 5.1.6.2.4 | Represents an Individual NWDAF Event Subscription Notification resource. |  |
| NwdafFailureCode | 5.1.6.3.13 | Identifies the failure reason. |  |
| NotificationMethod | 5.1.6.3.3 | Represents the notification methods that can be subscribed. |  |
| NsiIdInfo | 5.1.6.2.33 | Represents the S-NSSAI and the optionally associated Network Slice Instance Identifier(s). | ServiceExperienceNsiLoad NsiLoadExt |
| NsiLoadLevelInfo | 5.1.6.2.34 | Represents the load level information for an S-NSSAI and the optionally associated network slice instance. | NsiLoad NsiLoadExt |
| OutputStrategy | 5.1.6.3.16 | Represents the output strategy used for the reporting of the analytics. | Aggregation |
| QosRequirement | 5.1.6.2.20 |  | QoSSustainability |
| QosSustainabilityInfo | 5.1.6.2.19 | Represents the QoS Sustainability information. | QoSSustainability |
| RetainabilityThreshold | 5.1.6.2.21 |  | QoSSustainability |
| ServiceExperienceInfo | 5.1.6.2.24 | Represents the service experience information. | ServiceExperience |
| SliceLoadLevelInformation | 5.1.6.2.6 | Represents the slices and their load level information. |  |
| SubscriptionTransferInfo | 5.1.6.2.YY | Contains information about subscriptions that are requested to be transferred. | EneNA |
| TargetUeInformation | 5.1.6.2.8 | Identifies the target UE information. | ServiceExperienceNfLoadNetworkPerformanceUserDataCongestionUserDataCongestionExtUeMobilityUeCommunicationAbnormalBehaviourQoSSustainability |
| ThresholdLevel | 5.1.6.2.30 | Describe a threshold level. | UserDataCongestionNfLoad |
| TimeUnit | 5.1.6.3.9 |  | QoSSustainability |
| TrafficCharacterization | 5.1.6.2.14 |  | UeCommunication |
| TransferRequestType | 5.1.6.3.NN | Represents the type of a request for analytics subscription transfer. | EneNA |
| TopApplication | 5.1.6.2.39 | Top application that contributes the most to the traffic. | UserDataCongestionExt |
| UeAnalyticsContextDescriptor | 5.1.6.2.LL | Contains information about available UE related analytics contexts. | EneNA |
| UeCommunication | 5.1.6.2.13 |  | UeCommunication |
| UeMobility | 5.1.6.2.10 |  | UeMobility |
| UserDataCongestionInfo | 5.1.6.2.17 | Represents the user data congestion information. | UserDataCongestion |

Table 5.1.6.1-2 specifies data types re-used by the Nnwdaf\_EventsSubscription service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nnwdaf service based interface.

Table 5.1.6.1-2: Nnwdaf\_EventsSubscription re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| 5Qi | 3GPP TS 29.571 [8]  | Identifies the 5G QoS identifier | QoSSustainability |
| ApplicationId | 3GPP TS 29.571 [8] | Identifies the application identifier. | ServiceExperience UeCommunicationAbnormalBehaviour |
| BitRate | 3GPP TS 29.571 [8] | String representing a bit rate that shall be formatted as follows:pattern: "^\d+(\.\d+)? (bps|Kbps|Mbps|Gbps|Tbps)$"Examples: "125 Mbps", "0.125 Gbps", "125000 Kbps". | ServiceExperienceQoSSustainability |
| DateTime | 3GPP TS 29.571 [8] | Identifies the time. |  |
| Dnai | 3GPP TS 29.571 [8] | Identifies a user plane access to one or more DN(s). | ServiceExperience |
| Dnn | 3GPP TS 29.571 [8] | Identifies the DNN. | ServiceExperienceAbnormalBehaviourUeCommunication |
| DurationSec | 3GPP TS 29.571 [8] |  |  |
| EthFlowDescription | 3GPP TS 29.514 [21] |  | UeCommunicationAbnormalBehaviour |
| ExpectedUeBehaviourData | 3GPP TS 29.503 [23] |  | AbnormalBehaviour |
| Float | 3GPP TS 29.571 [8] |  |  |
| FlowDescription | 3GPP TS 29.514 [21] |  | UeCommunicationAbnormalBehaviour |
| FlowInfo | 3GPP TS 29.122 [19] |  | UserDataCongestionExt |
| GroupId | 3GPP TS 29.571 [8] | Identifies a group of UEs. | UeMobilityUeCommunication NetworkPerformance AbnormalBehaviourServiceExperience |
| Ipv4Addr | 3GPP TS 29.571 [8] |  |  |
| Ipv6Addr | 3GPP TS 29.571 [8] |  |  |
| NetworkAreaInfo | 3GPP TS 29.554 [18] | Identifies the network area. | ServiceExperienceQoSSustainabilityAbnormalBehaviourUeMobilityUserDataCongestionNetworkPerformance NsiLoadExt |
| NfInstanceId | 3GPP TS 29.571 [8] | Identifies an NF instance | NfLoad |
| NfSetId | 3GPP TS 29.571 [8] | Identifies an NF Set instance | NfLoad |
| NFType | 3GPP TS 29.510 [12] | Indentifies a type of NF | NfLoad |
| NsiId | 3GPP TS 29.531 [24] | Identifies a Network Slice Instance | ServiceExperienceNsiLoad NsiLoadExt |
| PacketDelBudget | 3GPP TS 29.571 [8] |  | QoSSustainability |
| PacketErrRate | 3GPP TS 29.571 [8] |  | QoSSustainability |
| ProblemDetails | 3GPP TS 29.571 [8] | Used in error responses to provide more detailed information about an error. |  |
| QosResourceType | 3GPP TS 29.571 [8] | Identifies the resource type in QoS characteristics. | QoSSustainability |
| RedirectResponse | 3GPP TS 29.571 [8] | Contains redirection related information. | ES3XX |
| ReportingInformation | 3GPP TS 29.523 [20] | Represents the type of reporting the subscription requires. |  |
| SamplingRatio | 3GPP TS 29.571 [8] |  |  |
| ScheduledCommunicationTime | 3GPP TS 29.122 [19] |  | UeMobility UeCommunication |
| Snssai | 3GPP TS 29.571 [8] | Identifies the S-NSSAI (Single Network Slice Selection Assistance Information). |  |
| Supi | 3GPP TS 29.571 [8] | The SUPI for an UE. | ServiceExperience,NfLoadNetworkPerformance,UserDataCongestionUeMobilityUeCommunicationAbnormalBehaviour |
| Gpsi | 3GPP TS 29.571 [8] | The GPSI for an UE. | UserDataCongestionExt |
| SupportedFeatures | 3GPP TS 29.571 [8] | Used to negotiate the applicability of the optional features defined in table 5.1.8-1. |  |
| SvcExperience | 3GPP TS 29.517 [22] |  | ServiceExperience |
| TimeWindow | 3GPP TS 29.122 [19] |  |  |
| Uinteger | 3GPP TS 29.571 [8] | Unsigned Integer, i.e. only value 0 and integers above 0 are permissible. |  |
| Uri | 3GPP TS 29.571 [8] |  |  |
| UserLocation | 3GPP TS 29.571 [8] |  | UeMobility  |
| Volume | 3GPP TS 29.122 [19] |  | UeCommunicationAbnormalBehaviour |
| FailureEventInfo | 5.1.6.2.35 | Represents the failure event and the corresponding failure reason. |  |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.2.XX Type AnalyticsSubscriptionsTransfer

Table 5.1.6.2.XX-1: Definition of type AnalyticsSubscriptionsTransfer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| subsTransInfos | array(SubscriptionTransferInfo) | M | 1..N | Contains information about the subscription(s) that are requested to be transferred. |  |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.2.YY Type SubscriptionTransferInfo

Table 5.1.6.2.YY-1: Definition of type SubscriptionTransferInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| transReqType | TranferRequestType | M | 1 | Indicates the type of the transfer request (i.e. if it is a request for transfer preparation or transfer execution) |  |
| nwdafEvSub | NnwdafEventsSubscription | M | 1 | Contains information about the analytics subscription that is to be transferred. |  |
| consumerId | NfInstanceId | M | 1 | NF instance identifer of the consumer of the analytics subscription that is to be transferred. |  |
| contextId | AnalyticsContextIdentifier | O | 0..1 | Identifier of analytics context information available at the NF service consumer. |  |
| sourceNfIds | array(NfInstanceId) | O | 1..N | NF instance identifer(s) of active data source(s) the NF service consumer is currently using for the analytics of the subscription that is to be transferred. |  |
| sourceSetIds | array(NfSetId) | O | 1..N | NF set identifer(s) of active data source(s) the NF service consumer is currently using for the analytics of the subscription that is to be transferred. |  |
| modelInfo | array(ModelInfo) | O | 1..N | Contains information identifying the ML model(s) that the NF service consumer is currently using for the analytics. |  |
| modelProvIds | array(NfInstanceId) | O | 1..N | NF instance identifer(s) of the ML model provider NWDAF(s) from which the NF service consumer currently subscribes to the ML model information used for the analytics. |  |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.2.MM Type ModelInfo

Table 5.1.6.2.MM-1: Definition of type ModelInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| analyticsId | NwdafEvent | M | 1 | Type of analytics for which this ML model is used. |  |
| mlFileAddr | Uri | M | 1 | Address of ML model file. |  |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.2.PP Type AnalyticsContextIdentifier

Table 5.1.6.2.PP-1: Definition of type AnalyticsContextIdentifier

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| subscriptionId | string | M | 1 | Identifies a subscription to the Nnwdaf\_EventsSubscription Service. |  |
| nfAnaCtxts | array(NwdafEvent) | O | 1..N | List of analytics types for which NF related analytics contexts can be retrieved. (NOTE) |  |
| ueAnaCtxts | array(UeAnalyticsContextDescriptor) | O | 1..N | List of objects that indicate for which SUPI and analytics types combinations analytics context can be retrieved. (NOTE) |  |
| NOTE: At least one of "nfAnaCtxt" and "ueAnaCtxt" shall be provided. |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.2.LL Type UeAnalyticsContextDescriptor

Table 5.1.6.2.LL-1: Definition of type UeAnalyticsContextDescriptor

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| supi | Supi | M | 1 | SUPI of the UE for which analytics context can be retrieved. |  |
| anaTypes | array(NwdafEvent) | M | 1..N | List of analytics types for which UE related analytics contexts can be retrieved. |  |

\* \* \* \* Next change \* \* \* \*

##### 5.1.6.3.NN Enumeration: TransferRequestType

Table 5.1.6.3.NN-1: Enumeration TransferRequestType

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| PREPARE | Indicates that the request is for analytics subscription transfer preparation. |  |
| TRANSFER | Indicates that the request is for analytics subscription transfer execution. |  |

\* \* \* \* Next change \* \* \* \*

# A.2 Nnwdaf\_EventsSubscription API

openapi: 3.0.0

info:

 version: 1.2.0-alpha.5

 title: Nnwdaf\_EventsSubscription

 description: |

 Nnwdaf\_EventsSubscription Service API.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.520 V17.4.0; 5G System; Network Data Analytics Services.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.520/'

security:

 - {}

 - oAuth2ClientCredentials:

 - nnwdaf-eventssubscription

servers:

 - url: '{apiRoot}/nnwdaf-eventssubscription/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

 /subscriptions:

 post:

 summary: Create a new Individual NWDAF Events Subscription

 operationId: CreateNWDAFEventsSubscription

 tags:

 - NWDAF Events Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-eventssubscription/v1/subscriptions/{subscriptionId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notificationURI}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/NnwdafEventsSubscriptionNotification'

 minItems: 1

 responses:

 '204':

 description: The receipt of the Notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subscriptionId}:

 delete:

 summary: Delete an existing Individual NWDAF Events Subscription

 operationId: DeleteNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF Event Subscription resource matching the subscriptionId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Events Subscription

 operationId: UpdateNWDAFEventsSubscription

 tags:

 - Individual NWDAF Events Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The Individual NWDAF Event Subscription resource was modified successfully and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 '204':

 description: The Individual NWDAF Event Subscription resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 description: The Individual NWDAF Event Subscription resource does not exist.

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers:

 post:

 summary: Provide information about requested analytics subscriptions transfer and potentially create a new Individual NWDAF Event Subscription Transfer resource.

 operationId: CreateNWDAFEventSubscriptionTransfer

 tags:

 - NWDAF Event Subscription Transfers (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 responses:

 '201':

 description: Create a new Individual NWDAF Event Subscription Transfer resource.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nnwdaf-eventssubscription/v1/transfers/{transferId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /transfers/{transferId}:

 delete:

 summary: Delete an existing Individual NWDAF Event Subscription Transfer

 operationId: DeleteNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 parameters:

 - name: transferId

 in: path

 description: String identifying a request for an analytics subscription transfer to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. The Individual NWDAF Event Subscription Transfer resource matching the transferId was deleted.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Update an existing Individual NWDAF Event Subscription Transfer

 operationId: UpdateNWDAFEventSubscriptionTransfer

 tags:

 - Individual NWDAF Event Subscription Transfer (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AnalyticsSubscriptionsTransfer'

 parameters:

 - name: transferId

 in: path

 description: String identifying a request for an analytics subscription transfer to the Nnwdaf\_EventsSubscription Service

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual NWDAF Event Subscription Transfer resource was modified successfully.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '501':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/501'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nnwdaf-eventssubscription: Access to the Nnwdaf\_EventsSubscription API

 schemas:

 NnwdafEventsSubscription:

 description: Represents an Individual NWDAF Event Subscription resource.

 type: object

 properties:

 eventSubscriptions:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 evtReq:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 notificationURI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 failEventReports:

 type: array

 items:

 $ref: '#/components/schemas/FailureEventInfo'

 minItems: 1

 required:

 - eventSubscriptions

 EventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 anySlice:

 $ref: '#/components/schemas/AnySlice'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 description: Identification(s) of application to which the subscription applies.

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Identification(s) of DNN to which the subscription applies.

 dnais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 event:

 $ref: '#/components/schemas/NwdafEvent'

 extraReportReq:

 $ref: '#/components/schemas/EventReportingRequirement'

 loadLevelThreshold:

 type: integer

 description: Indicates that the NWDAF shall report the corresponding network slice load level to the NF service consumer where the load level of the network slice identified by snssais is reached.

 notificationMethod:

 $ref: '#/components/schemas/NotificationMethod'

 matchingDir:

 $ref: '#/components/schemas/MatchingDirection'

 nfLoadLvlThds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 description: Shall be supplied in order to start reporting when an average load level is reached.

 nfInstanceIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 nfSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 nfTypes:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 minItems: 1

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 topAppListUlInd:

 type: boolean

 description: Indicates that the list of top applications that contribute the most to the traffic in Uplink direction is requested, if it is included and set to "true". Default value is "false".

 topAppListDlInd:

 type: boolean

 description: Indicates that the list of top applications that contribute the most to the traffic in Downlink direction is requested, if it is included and set to "true". Default value is "false".

 nsiIdInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiIdInfo'

 minItems: 1

 nsiLevelThrds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 qosRequ:

 $ref: '#/components/schemas/QosRequirement'

 qosFlowRetThds:

 type: array

 items:

 $ref: '#/components/schemas/RetainabilityThreshold'

 minItems: 1

 ranUeThrouThds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minItems: 1

 repetitionPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 snssaia:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies. It corresponds to snssais in the data model definition of 3GPP TS 29.520.

 tgtUe:

 $ref: '#/components/schemas/TargetUeInformation'

 congThresholds:

 type: array

 items:

 $ref: '#/components/schemas/ThresholdLevel'

 minItems: 1

 nwPerfRequs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfRequirement'

 minItems: 1

 bwRequs:

 type: array

 items:

 $ref: '#/components/schemas/BwRequirement'

 minItems: 1

 excepRequs:

 type: array

 items:

 $ref: '#/components/schemas/Exception'

 minItems: 1

 exptAnaType:

 $ref: '#/components/schemas/ExpectedAnalyticsType'

 exptUeBehav:

 $ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/ExpectedUeBehaviourData'

 required:

 - event

 NnwdafEventsSubscriptionNotification:

 description: Represents an Individual NWDAF Event Subscription Notification resource.

 type: object

 properties:

 eventNotifications:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 subscriptionId:

 type: string

 description: String identifying a subscription to the Nnwdaf\_EventsSubscription Service

 required:

 - eventNotifications

 - subscriptionId

 EventNotification:

 description: Represents a notification on events that occurred.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 start:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeStampGen:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 failNotifyCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 rvWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 anaMetaInfo:

 $ref: '#/components/schemas/AnalyticsMetadataInfo'

 nfLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NfLoadLevelInformation'

 minItems: 1

 nsiLoadLevelInfos:

 type: array

 items:

 $ref: '#/components/schemas/NsiLoadLevelInfo'

 minItems: 1

 sliceLoadLevelInfo:

 $ref: '#/components/schemas/SliceLoadLevelInformation'

 svcExps:

 type: array

 items:

 $ref: '#/components/schemas/ServiceExperienceInfo'

 minItems: 1

 qosSustainInfos:

 type: array

 items:

 $ref: '#/components/schemas/QosSustainabilityInfo'

 minItems: 1

 ueComms:

 type: array

 items:

 $ref: '#/components/schemas/UeCommunication'

 minItems: 1

 ueMobs:

 type: array

 items:

 $ref: '#/components/schemas/UeMobility'

 minItems: 1

 userDataCongInfos:

 type: array

 items:

 $ref: '#/components/schemas/UserDataCongestionInfo'

 minItems: 1

 abnorBehavrs:

 type: array

 items:

 $ref: '#/components/schemas/AbnormalBehaviour'

 minItems: 1

 nwPerfs:

 type: array

 items:

 $ref: '#/components/schemas/NetworkPerfInfo'

 minItems: 1

 required:

 - event

 ServiceExperienceInfo:

 description: Represents service experience information.

 type: object

 properties:

 svcExprc:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/SvcExperience'

 svcExprcVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 required:

 - svcExprc

 BwRequirement:

 description: Represents bandwidth requirements.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 required:

 - appId

 SliceLoadLevelInformation:

 description: Contains load level information applicable for one or several slices.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Identification(s) of network slice to which the subscription applies.

 required:

 - loadLevelInformation

 - snssais

 NsiLoadLevelInfo:

 description: Represents the network slice and optionally the associated network slice instance and the load level information.

 type: object

 properties:

 loadLevelInformation:

 $ref: '#/components/schemas/LoadLevelInformation'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiId:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 timePeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 numOfUes:

 $ref: '#/components/schemas/NumberAverage'

 numOfPduSess:

 $ref: '#/components/schemas/NumberAverage'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loadLevelInformation

 - snssai

 NsiIdInfo:

 description: Represents the S-NSSAI and the optionally associated Network Slice Instance(s).

 type: object

 properties:

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 nsiIds:

 type: array

 items:

 $ref: 'TS29531\_Nnssf\_NSSelection.yaml#/components/schemas/NsiId'

 minItems: 1

 required:

 - snssai

 EventReportingRequirement:

 description: Represents the type of reporting that the subscription requires.

 type: object

 properties:

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 maxObjectNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 maxSupiNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeAnaNeeded:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 anaMeta:

 type: array

 items:

 $ref: '#/components/schemas/AnalyticsMetadata'

 minItems: 1

 anaMetaInd:

 $ref: '#/components/schemas/AnalyticsMetadataIndication'

 TargetUeInformation:

 description: Identifies the target UE information.

 type: object

 properties:

 anyUe:

 type: boolean

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 intGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 UeMobility:

 description: Represents UE mobility information.

 type: object

 properties:

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 duration:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 durationVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 locInfos:

 type: array

 items:

 $ref: '#/components/schemas/LocationInfo'

 minItems: 1

 required:

 - duration

 - locInfos

 LocationInfo:

 description: Represents UE location information.

 type: object

 properties:

 loc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - loc

 UeCommunication:

 description: Represents UE communication information.

 type: object

 properties:

 commDur:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 commDurVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 perioTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 perioTimeVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 ts:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tsVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 recurringTime:

 $ref: 'TS29122\_CpProvisioning.yaml#/components/schemas/ScheduledCommunicationTime'

 trafChar:

 $ref: '#/components/schemas/TrafficCharacterization'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - commDur

 - trafChar

 TrafficCharacterization:

 description: Identifies the detailed traffic characterization.

 type: object

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 maxItems: 2

 ulVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 ulVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 dlVol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 dlVolVariance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 UserDataCongestionInfo:

 description: Represents the user data congestion information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 congestionInfo:

 $ref: '#/components/schemas/CongestionInfo'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 CongestionInfo:

 description: Represents the congestion information.

 type: object

 properties:

 congType:

 $ref: '#/components/schemas/CongestionType'

 timeIntev:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 nsi:

 $ref: '#/components/schemas/ThresholdLevel'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 topAppListUl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 topAppListDl:

 type: array

 items:

 $ref: '#/components/schemas/TopApplication'

 minItems: 1

 required:

 - congType

 - timeIntev

 - nsi

 TopApplication:

 description: Top application that contributes the most to the traffic.

 type: object

 properties:

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ipTrafficFilter:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 QosSustainabilityInfo:

 description: Represents the QoS Sustainability information.

 type: object

 properties:

 areaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 startTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTs:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qosFlowRetThd:

 $ref: '#/components/schemas/RetainabilityThreshold'

 ranUeThrouThd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 QosRequirement:

 description: Represents the QoS requirements.

 type: object

 properties:

 5qi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

 gfbrUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 gfbrDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 resType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

 pdb:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 per:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

 ThresholdLevel:

 description: Represents a threshold level.

 type: object

 properties:

 congLevel:

 type: integer

 nfLoadLevel:

 type: integer

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 NfLoadLevelInformation:

 description: Represents load level information of a given NF instance.

 type: object

 properties:

 nfType:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/NFType'

 nfInstanceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 nfStatus:

 $ref: '#/components/schemas/NfStatus'

 nfCpuUsage:

 type: integer

 nfMemoryUsage:

 type: integer

 nfStorageUsage:

 type: integer

 nfLoadLevelAverage:

 type: integer

 nfLoadLevelpeak:

 type: integer

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nfType

 - nfInstanceId

 NfStatus:

 description: Contains the percentage of time spent on various NF states.

 type: object

 properties:

 statusRegistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUnregistered:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 statusUndiscoverable:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 AnySlice:

 type: boolean

 description: FALSE represents not applicable for all slices. TRUE represents applicable for all slices.

 LoadLevelInformation:

 type: integer

 description: Load level information of the network slice and the optionally associated network slice instance.

 AbnormalBehaviour:

 description: Represents the abnormal behaviour information.

 type: object

 properties:

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 excep:

 $ref: '#/components/schemas/Exception'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ratio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 addtMeasInfo:

 $ref: '#/components/schemas/AdditionalMeasurement'

 required:

 - excep

 Exception:

 description: Represents the Exception information.

 type: object

 properties:

 excepId:

 $ref: '#/components/schemas/ExceptionId'

 excepLevel:

 type: integer

 excepTrend:

 $ref: '#/components/schemas/ExceptionTrend'

 required:

 - excepId

 AdditionalMeasurement:

 description: Represents additional measurement information.

 type: object

 properties:

 unexpLoc:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 unexpFlowTeps:

 type: array

 items:

 $ref: '#/components/schemas/IpEthFlowDescription'

 minItems: 1

 unexpWakes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 1

 ddosAttack:

 $ref: '#/components/schemas/AddressList'

 wrgDest:

 $ref: '#/components/schemas/AddressList'

 circums:

 type: array

 items:

 $ref: '#/components/schemas/CircumstanceDescription'

 minItems: 1

 IpEthFlowDescription:

 description: Contains the description of an Uplink and/or Downlink Ethernet flow.

 type: object

 properties:

 ipTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 ethTrafficFilter:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 AddressList:

 description: Represents a list of IPv4 and/or IPv6 addresses.

 type: object

 properties:

 ipv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 CircumstanceDescription:

 description: Contains the description of a circumstance.

 type: object

 properties:

 freq:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 tm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 locArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 vol:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Volume'

 RetainabilityThreshold:

 description: Represents a QoS flow retainability threshold.

 type: object

 properties:

 relFlowNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 relTimeUnit:

 $ref: '#/components/schemas/TimeUnit'

 relFlowRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 NetworkPerfRequirement:

 description: Represents a network performance requirement.

 type: object

 properties:

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - nwPerfType

 NetworkPerfInfo:

 description: Represents the network performance information.

 type: object

 properties:

 networkArea:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 nwPerfType:

 $ref: '#/components/schemas/NetworkPerfType'

 relativeRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 absoluteNum:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 confidence:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 required:

 - networkArea

 - nwPerfType

 FailureEventInfo:

 description: Contains information on the event for which the subscription is not successful.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/NwdafEvent'

 failureCode:

 $ref: '#/components/schemas/NwdafFailureCode'

 required:

 - event

 - failureCode

 AnalyticsMetadataIndication:

 description: Contains analytics metadata information requested to be used during analytics generation.

 type: object

 properties:

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 aggrNwdafIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 AnalyticsMetadataInfo:

 description: Contains analytics metadata information required for analytics aggregation.

 type: object

 properties:

 numSamples:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 dataWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 dataStatProps:

 type: array

 items:

 $ref: '#/components/schemas/DatasetStatisticalProperty'

 minItems: 1

 strategy:

 $ref: '#/components/schemas/OutputStrategy'

 accuracy:

 $ref: '#/components/schemas/Accuracy'

 NumberAverage:

 description: Represents average and variance information.

 type: object

 properties:

 number:

 type: integer

 variance:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 required:

 - number

 - variance

 AnalyticsSubscriptionsTransfer:

 description: Contains information about a request to transfer analytics subscriptions.

 type: object

 properties:

 subsTransInfos:

 type: array

 items:

 $ref: '#/components/schemas/SubscriptionTransferInfo'

 minItems: 1

 required:

 - subsTransInfos

 SubscriptionTransferInfo:

 description: Contains information about subscriptions that are requested to be transferred.

 type: object

 properties:

 transReqType:

 $ref: '#/components/schemas/TranferRequestType'

 nwdafEvSub:

 $ref: '#/components/schemas/NnwdafEventsSubscription'

 consumerId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 contextId:

 $ref: '#/components/schemas/AnalyticsContextIdentifier'

 sourceNfIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 sourceSetIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 minItems: 1

 modelInfo:

 type: array

 items:

 $ref: '#/components/schemas/ModelInfo'

 minItems: 1

 modelProvIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 minItems: 1

 required:

 - transReqType

 - nwdafEvSub

 - consumerId

 ModelInfo:

 description: Contains information about an ML model.

 type: object

 properties:

 analyticsId:

 $ref: '#/components/schemas/NwdafEvent'

 mlFileAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - analyticsId

 - mlFileAddr

 AnalyticsContextIdentifier:

 description: Contains information about available analytics contexts.

 type: object

 properties:

 subscriptionId:

 type: string

 description: The identifier of a subscription.

 nfAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: List of analytics types for which NF related analytics contexts can be retrieved.

 ueAnaCtxts:

 type: array

 items:

 $ref: '#/components/schemas/UeAnalyticsContextDescriptor'

 minItems: 1

 description: List of objects that indicate for which SUPI and analytics types combinations analytics context can be retrieved.

 allOf:

 - anyOf:

 - required: [nfAnaCtxts]

 - required: [ueAnaCtxts] - required: [subscriptionId]

 UeAnalyticsContextDescriptor:

 description: Contains information about available UE related analytics contexts.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 anaTypes:

 type: array

 items:

 $ref: '#/components/schemas/NwdafEvent'

 minItems: 1

 description: List of analytics types for which UE related analytics contexts can be retrieved.

 required:

 - supi

 - anaTypes

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - THRESHOLD

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PERIODIC: The subscribe of NWDAF Event is periodically. The periodic of the notification is identified by repetitionPeriod defined in subclause 5.1.6.2.3.

 - THRESHOLD: The subscribe of NWDAF Event is upon threshold exceeded. The threshold of the notification is identified by loadLevelThreshold defined in subclause 5.1.6.2.3.

 NwdafEvent:

 anyOf:

 - type: string

 enum:

 - SLICE\_LOAD\_LEVEL

 - NETWORK\_PERFORMANCE

 - NF\_LOAD

 - SERVICE\_EXPERIENCE

 - UE\_MOBILITY

 - UE\_COMMUNICATION

 - QOS\_SUSTAINABILITY

 - ABNORMAL\_BEHAVIOUR

 - USER\_DATA\_CONGESTION

 - NSI\_LOAD\_LEVEL

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - SLICE\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice

 - NETWORK\_PERFORMANCE: Indicates that the event subscribed is network performance information.

 - NF\_LOAD: Indicates that the event subscribed is load level and status of one or several Network Functions.

 - SERVICE\_EXPERIENCE: Indicates that the event subscribed is service experience.

 - UE\_MOBILITY: Indicates that the event subscribed is UE mobility information.

 - UE\_COMMUNICATION: Indicates that the event subscribed is UE communication information.

 - QOS\_SUSTAINABILITY: Indicates that the event subscribed is QoS sustainability.

 - ABNORMAL\_BEHAVIOUR: Indicates that the event subscribed is abnormal behaviour.

 - USER\_DATA\_CONGESTION: Indicates that the event subscribed is user data congestion information.

 - NSI\_LOAD\_LEVEL: Indicates that the event subscribed is load level information of Network Slice and the optionally associated Network Slice Instance

 Accuracy:

 anyOf:

 - type: string

 enum:

 - LOW

 - HIGH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LOW: Low accuracy.

 - HIGH: High accuracy.

 CongestionType:

 anyOf:

 - type: string

 enum:

 - USER\_PLANE

 - CONTROL\_PLANE

 - USER\_AND\_CONTROL\_PLANE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - USER\_PLANE: The congestion analytics type is User Plane.

 - CONTROL\_PLANE: The congestion analytics type is Control Plane.

 - USER\_AND\_CONTROL\_PLANE: The congestion analytics type is User Plane and Control Plane.

 ExceptionId:

 anyOf:

 - type: string

 enum:

 - UNEXPECTED\_UE\_LOCATION

 - UNEXPECTED\_LONG\_LIVE\_FLOW

 - UNEXPECTED\_LARGE\_RATE\_FLOW

 - UNEXPECTED\_WAKEUP

 - SUSPICION\_OF\_DDOS\_ATTACK

 - WRONG\_DESTINATION\_ADDRESS

 - TOO\_FREQUENT\_SERVICE\_ACCESS

 - UNEXPECTED\_RADIO\_LINK\_FAILURES

 - PING\_PONG\_ACROSS\_CELLS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNEXPECTED\_UE\_LOCATION: Unexpected UE location

 - UNEXPECTED\_LONG\_LIVE\_FLOW: Unexpected long-live rate flows

 - UNEXPECTED\_LARGE\_RATE\_FLOW: Unexpected large rate flows

 - UNEXPECTED\_WAKEUP: Unexpected wakeup

 - SUSPICION\_OF\_DDOS\_ATTACK: Suspicion of DDoS attack

 - WRONG\_DESTINATION\_ADDRESS: Wrong destination address

 - TOO\_FREQUENT\_SERVICE\_ACCESS: Too frequent Service Access

 - UNEXPECTED\_RADIO\_LINK\_FAILURES: Unexpected radio link failures

 - PING\_PONG\_ACROSS\_CELLS: Ping-ponging across neighbouring cells

 ExceptionTrend:

 anyOf:

 - type: string

 enum:

 - UP

 - DOWN

 - UNKNOW

 - STABLE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UP: Up trend of the exception level.

 - DOWN: Down trend of the exception level.

 - UNKNOW: Unknown trend of the exception level.

 - STABLE: Stable trend of the exception level.

 TimeUnit:

 anyOf:

 - type: string

 enum:

 - MINUTE

 - HOUR

 - DAY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MINUTE: Time unit is per minute.

 - HOUR: Time unit is per hour.

 - DAY: Time unit is per day.

 NetworkPerfType:

 anyOf:

 - type: string

 enum:

 - GNB\_ACTIVE\_RATIO

 - GNB\_COMPUTING\_USAGE

 - GNB\_MEMORY\_USAGE

 - GNB\_DISK\_USAGE

 - NUM\_OF\_UE

 - SESS\_SUCC\_RATIO

 - HO\_SUCC\_RATIO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - GNB\_ACTIVE\_RATIO: Indicates that the network performance requirement is gNodeB active (i.e. up and running) rate. Indicates the ratio of gNB active (i.e. up and running) number to the total number of gNB

 - GNB\_COMPUTING\_USAGE: Indicates gNodeB computing resource usage.

 - GNB\_MEMORY\_USAGE: Indicates gNodeB memory usage.

 - GNB\_DISK\_USAGE: Indicates gNodeB disk usage.

 - NUM\_OF\_UE: Indicates number of UEs.

 - SESS\_SUCC\_RATIO: Indicates ratio of successful setup of PDU sessions to total PDU session setup attempts.

 - SESS\_SUCC\_RATIO: Indicates Ratio of successful handovers to the total handover attempts.

 ExpectedAnalyticsType:

 anyOf:

 - type: string

 enum:

 - MOBILITY

 - COMMUN

 - MOBILITY\_AND\_COMMUN

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - MOBILITY: Mobility related abnormal behaviour analytics is expected by the consumer.

 - COMMUN: Communication related abnormal behaviour analytics is expected by the consumer.

 - MOBILITY\_AND\_COMMUN: Both mobility and communication related abnormal behaviour analytics is expected by the consumer.

 MatchingDirection:

 anyOf:

 - type: string

 enum:

 - ASCENDING

 - DESCENDING

 - CROSSED

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - ASCENDING: Threshold is crossed in ascending direction.

 - DESCENDING: Threshold is crossed in descending direction.

 - CROSSED: Threshold is crossed either in ascending or descending direction.

 NwdafFailureCode:

 anyOf:

 - type: string

 enum:

 - UNAVAILABLE\_DATA

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME

 - OTHER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNAVAILABLE\_DATA: Indicates the requested statistics information for the event is rejected since necessary data to perform the service is unavailable.

 - BOTH\_STAT\_PRED\_NOT\_ALLOWED: Indicates the requested analysis information for the event is rejected since the start time is in the past and the end time is in the future, which means the NF service consumer requested both statistics and prediction for the analytics.

 - UNSATISFIED\_REQUESTED\_ANALYTICS\_TIME: Indicates that the requested event is rejected since the analytics information is not ready when the time indicated by the "timeAnaNeeded" attribute (as provided during the creation or modification of subscription) is reached.

 - OTHER: Indicates the requested analysis information for the event is rejected due to other reasons.

 AnalyticsMetadata:

 anyOf:

 - type: string

 enum:

 - NUM\_OF\_SAMPLES

 - DATA\_WINDOW

 - DATA\_STAT\_PROPS

 - STRATEGY

 - ACCURACY

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - NUM\_OF\_SAMPLES: Number of data samples used for the generation of the output analytics.

 - DATA\_WINDOW: Data time window of the data samples.

 - DATA\_STAT\_PROPS: Dataset statistical properties of the data used to generate the analytics.

 - STRATEGY: Output strategy used for the reporting of the analytics.

 - ACCURACY: Level of accuracy reached for the analytics.

 DatasetStatisticalProperty:

 anyOf:

 - type: string

 enum:

 - UNIFORM\_DIST\_DATA

 - NO\_OUTLIERS

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNIFORM\_DIST\_DATA: Indicates the use of data samples that are uniformly distributed according to the different aspects of the requested analytics.

 - NO\_OUTLIERS: Indicates that the data samples shall disregard data samples that are at the extreme boundaries of the value range.

 OutputStrategy:

 anyOf:

 - type: string

 enum:

 - BINARY

 - GRADIENT

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - BINARY: Indicates that the analytics shall only be reported when the requested level of accuracy is reached within a cycle of periodic notification.

 - GRADIENT: Indicates that the analytics shall be reported according with the periodicity irrespective of whether the requested level of accuracy has been reached or not.

 TransferRequestType:

 anyOf:

 - type: string

 enum:

 - PREPARE

 - TRANSFER

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PREPARE: Indicates that the request is for analytics subscription transfer preparation.

 - TRANSFER: Indicates that the request is for analytics subscription transfer execution.

\* \* \* \* End of changes \* \* \* \*