**TSG-CT WG3 Meeting #118-e *C3-215078***

**E-Meeting, 11th – 15th October 2021 (Revision of C3-214xyz)**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | 0412 | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update of the time synchronization exposure capability notification |
|  |  |
| ***Source to WG:*** | Huawei, Nokia, Nokia Shanghai Bell, Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | IIoT |  | ***Date:*** | 2021-10-11 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | As defined in clause 5.2.6.25.8, the NEF privides the Time Synchronization capability event parameters as follows (S2-2106773):

|  |  |
| --- | --- |
| Time Synchronization event parameter | Description |
| List of User-Plane Node IDs  | Identifies the applicable NW-TT (NOTE). |
| **For each User-Plane Node ID** |
| (g)PTP grandmaster capable | Indicates separately whether User-Plane Node ID supports acting as a gPTP and/or PTP grandmaster. |
| List of UEs associated with the User-Plane Node ID |  |
| **For each UE** |
| UE identity | Identifies the UE to which the reported parameters below apply. |
| PTP instance types |  Supported PTP instance types as described in clause 5.27.1.4 in TS 23.501 [2]. |
| Transport protocols | Supported transport protocols for PTP as described in clause 5.27.1.4 in TS 23.501 [2]. |
| Supported PTP Profiles | Identifies the PTP profiles supported by 5GS for the reported UE. |
| NOTE: This is needed to limit the PTP instance into a single NW-TT. In this way the AF can know e.g. UE1/UE2/UE3 are served by NW-TT1, UE4/UE5/UE6 are served by NW-TT2. The AF can control the PTP instances per NW-TT. |

 |
|  |  |
| ***Summary of change:*** | Restruct the data types to align with stage 2 requirement. |
|  |  |
| ***Consequences if not approved:*** | Not aligned with stage 2 on Nnef\_TimeSynchronization\_CapsNotify operation supporting. |
|  |  |
| ***Clauses affected:*** | 4.4.24.1, 5.15.4.3.3, 5.15,4.3.8, 5.15.4.3.x1(new), A.13 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible feature to the OpenAPI file TimeSyncExposure API. |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 4.4.24.1 Subscription to notification of Time Synchronization Capabilites

The procedures are used by the AF to subscribe to notifications and to explicitly cancel a previous subscription for UE availability for the time synchronization service via the NEF.

In order to subscribe to the notification for UE availability for the time synchronization service, the AF shall send an HTTP POST rmessage to the NEF to the customized operation URI "{apiRoot}/3gpp-time-sync/v1/{afId}/subscriptions". The HTTP POST message shall include the TimeSyncExposureSubsc data structure as request body. The TimeSyncExposureSubsc data structure shall include:

- one of the indication of the UEs to which the time synchronization capabilities is requested via:

- identification of a list of individual UEs within a "gpsis" attribute;

- indication of any UE within the "anyUeInd" attribute if DNN and S-NSSAI are provisioned; or

- identification of a group of UE(s) via a "exterGroupId" attribute.

- subscription to event(s) notification as "evSubsc" attribute;

- notification URI within the "subsNotifUri" attribute;

- notification correlation Id within the "subsNotifId" attribute;

and may include:

* either the DNN within the "dnn" attribute and the "snssai" attribute or the AF Service Identifier within the "afServiceId" attribute;
* notification methods within the "notifMethods" attribute
* maximum number of reports within the "maxReportNbr" attribute;
* expiry time within the "expiry" attribute; and
* report period within the "repPeriod" attribute.

In order to delete an existing subscription, the AF shall send an HTTP DELETE message to the NEF targeting the resource "Individual Time Synchronization Exposure Subscription".

Upon the reception of an HTTP POST request, if the AF is authorized, the NEF shall interact with the UDM by using Nudm\_SubscriberDataManagement service as defined in 3GPP TS 29.503 [17] to translate the GPSI or external group identifier into the corresponding SUPI or internal group identifier. Then the NEF selects a TSCTSF and invokes the Ntsctsf\_TimeSynchronization\_CapsSubscribe request service operation to the selected TSCTSF. If the NEF receives an error code from the TSCTSF, the NEF shall not create or delete the resource and shall respond to the AF with a proper error status code.

After receiving a successful response from the TSCTSF, the NEF shall,

- for an HTTP POST request, create an "Individual Time Synchronization Exposure Subscription" resource which represents the time synchronization exposure subscription request, addressed by a URI that contains the AF Identifier and a NEF-created configuration identifier, and shall respond to the AF with a 201 Created status code, including a Location header field containing the URI for the created resource. The AF shall use the URI received in the Location header in subsequent requests to the NEF to refer to this Time Synchronization Exposure Subscription.

- when the NEF receives the notification of the time synchronization capability for a list of UE(s) from the TSCSF by Ntsctsf\_TimeSynchronization\_CapsNotify service operation defined in 3GPP TS 29.565 [50], the NEF shall provide a notification to AF by sending HTTP POST message that include the TimeSyncExposureSubsNotif data structure in the request body. Upon receipt of the notification, the AF shall respond with a "204 No Content" status code to confirm the received notification.

- for an HTTP DELETE request, remove all properties of the resource and delete the corresponding active "Individual Time Synchronization Exposure Subscription" resource, then respond to the AF with a 204 No Content status code.

\*\*\* Next change \*\*\*

##### 5.15.4.3.3 Type: TimeSyncCapability

Table 5.15.4.3.3-1: Definition of type TimeSyncCapability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| upNodeId | Uint64 | M | 1 | Identifies the applicable NW-TT. Contains a TSC user plane node Id. If integrated with TSN, the user plane node Id is a bridge Id defined in IEEE 802.1Q [51] clause 14.2.5. |  |
|  |  |  |  |  |  |
| gmCapables | array(GmCapable) | O | 1..N | Indicates whether user plane node supports acting as a gPTP and/or PTP grandmaster. |  |
|  |  |  |  |  |  |
| ptpCapForUes | map(PtpCapabilitiesPerUe) | M | 1..N | Contains the PTP capabilities supported by the list of UE(s). The key of the map is the gpsi. |  |

\*\*\* Next change \*\*\*

##### 5.15.4.3.8 Type SubsEventNotification

Table 5.15.4.3.8-1: Definition of type SubsEventNotification

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| event | SubscribedEvent | M | 1 | Subscribed events. |  |
| timeSyncCapas | array(TimeSyncCapability) | O | 1..N | Contains a list of time synchronization capabilities for the UE(s). |  |

\*\*\* Next change \*\*\*

##### 5.15.4.3.x1 Type: PtpCapabilitiesPerUe

Table 5.15.4.4.x1-1: Definition of type PtpCapabilitiesPerUe

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| gpsi | Gpsi | M | 1 | Identifies the UE to which the reported PTP instance below apply. |  |
| ptpCaps | array(EventFilter) | M | 1..N | Contains the reported PTP capabilities for the UE. |  |

\*\*\* Next change \*\*\*

# A.13 TimeSyncExposure API

openapi: 3.0.0

info:

 title: 3gpp-time-sync-exposure

 version: 1.0.0-alpha.2

 description: |

 API for time synchronization exposure.

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.522 V17.3.0; 5G System; Network Exposure Function Northbound APIs.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

 - {}

 - oAuth2ClientCredentials: []

servers:

 - url: '{apiRoot}/3gpp-time-sync/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

 /{afId}/subscriptions:

 get:

 summary: read all of the active subscriptions for the AF

 tags:

 - Time Synchronization Exposure Subscriptions

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get all of the active subscriptions for the AF)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 minItems: 0

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 post:

 summary: Creates a new subscription resource

 tags:

 - Time Synchronization Exposure Subscriptions

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 requestBody:

 description: new subscription creation

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 responses:

 '201':

 description: Created (Successful creation)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 callbacks:

 timeSyncSubsNotification:

 '{$request.body#/subsNotifUri}':

 post:

 requestBody:

 description: Notification for Time Synchronization Capability for a list of UEs.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsNotif'

 responses:

 '204':

 description: Expected response to a successful callback processing without a body

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{afId}/subscriptions/{subscriptionId}:

 get:

 summary: read an active subscription for the AF and the subscription Id

 tags:

 - Individual Time Synchronization Exposure Subscription

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get the active subscription)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureSubsc'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Deletes an already existing subscription

 tags:

 - Individual Time Synchronization Exposure Subscription

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content (Successful deletion of the existing subscription)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{afId}/subscriptions/{subscriptionId}/configurations:

 get:

 summary: read all of the active configurations for the AF

 tags:

 - Time Synchronization Exposure Configurations

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 description: String identifying the individual synchronization Exposure Subscription resource in the NEF

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get all of the active configurations for the AF)

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 minItems: 0

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 post:

 summary: Creates a new configuration resource

 tags:

 - Time Synchronization Exposure Configurations

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 description: String identifying the individual synchronization Exposure Subscription resource in the NEF

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: new configuration creation

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 responses:

 '201':

 description: Created (Successful creation)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 callbacks:

 timeSyncConfigNotification:

 '{$request.body#/configNotifUri}':

 post:

 requestBody:

 description: Notification for Time Synchronization Service status.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfigNotif'

 responses:

 '204':

 description: Expected response to a successful callback processing without a body

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{afId}/subscriptions/{subscriptionId}/configurations/{configurationId}:

 get:

 summary: read an active subscription for the AF and the subscription Id

 tags:

 - Individual Time Synchronization Exposure Subscription

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK (Successful get the active subscription)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 summary: Updates/replaces an existing configuration resource

 tags:

 - Individual Time Synchronization Exposure Configuration

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 requestBody:

 description: Parameters to update/replace the existing configuration

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 responses:

 '200':

 description: OK (Successful deletion of the existing configuration)

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TimeSyncExposureConfig'

 '204':

 description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Deletes an already existing configuration

 tags:

 - Individual Time Synchronization Exposure Configuration

 parameters:

 - name: afId

 in: path

 description: Identifier of the AF

 required: true

 schema:

 type: string

 - name: subscriptionId

 in: path

 description: Identifier of the subscription resource

 required: true

 schema:

 type: string

 - name: configurationId

 in: path

 description: Identifier of the configuration resource

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content (Successful deletion of the existing configuration)

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 TimeSyncExposureSubsc:

 description: Contains requested parameters for the subscription to the notification of time synchronization capability.

 type: object

 properties:

 exterGroupId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 description: Contains a list of UE for which the time synchronization capabilities is requested.

 anyUeInd:

 type: boolean

 description: Any UE indication. This IE shall be present if the event subscription is applicable to any UE. Default value "false" is used, if not present.

 afServiceId:

 type: string

 description: Identifies a service on behalf of which the AF is issuing the request.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 subsNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 subsNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 subscribedEvents:

 type: array

 items:

 $ref: '#/components/schemas/SubscribedEvent'

 minItems: 1

 description: Subscribed events

 notifMethod:

 $ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

 maxReportNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 requestTestNotification:

 type: boolean

 description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

 websockNotifConfig:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - subsNotifUri

 - subsNotifId

 TimeSyncCapability:

 description: Contains time synchronization capability.

 type: object

 properties:

 gpsis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 minItems: 1

 description: Contains a list of UEs associated with the user plane node..

 upNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 gmCapables:

 type: array

 items:

 $ref: '#/components/schemas/GmCapable'

 ptpCapForUes:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/PtpCapabilitiesPerUe'

 minProperties: 1

 description: Contains the PTP capabilities supported by each of the UE(s). The key of the map is the gpsi.

 required:

 - upNodeId

 - ptpCapForUes

 DistributionMethod:

 description: Contains the time synchronization distribution methods.

 type: object

 properties:

 1588mes:

 $ref: '#/components/schemas/1588Method'

 1asMe:

 type: boolean

 description: Indicates that the IEEE Std 802.1AS-2020 method is supported if it is included and set to true.

 5gClockMe:

 type: boolean

 description: Indicates that Access Stratum-based 5G clock sync is supported if it is included and set to true.

 1588Method:

 description: Contains time synchronization distribution methods defined in IEEE Std 1588-2019.

 type: object

 properties:

 op:

 $ref: '#/components/schemas/Operation'

 pro:

 $ref: '#/components/schemas/Protocol'

 required:

 - op

 - pro

 TimeSyncExposureConfig:

 description: Contains the Time Synchronization Configuration parameters.

 type: object

 properties:

 upNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 reqDisMethod:

 $ref: '#/components/schemas/DistributionMethod'

 gmEnable:

 type: boolean

 description: Indicates that the AF requests 5GS to act as a grandmaster for PTP or gPTP if it is included and set to true.

 gmPrio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 timeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 ptpProfiles:

 type: string

 description: Identifies the PTP profiles supported by 5GS for the reported UE.

 configNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 configNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 tempValidity:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

 required:

 - configNotifId

 - configNotifUri

 TimeSyncExposureSubsNotif:

 description: Contains the notification of time synchronization capability.

 type: object

 properties:

 subsNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/SubsEventNotification'

 minItems: 1

 required:

 - subsNotifId

 - eventNotifs

 SubsEventNotification:

 description: Notifications about subscribed Individual Events.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/SubscribedEvent'

 timeSyncCapas:

 type: array

 items:

 $ref: '#/components/schemas/TimeSyncCapability'

 minItems: 1

 required:

 - event

 TimeSyncExposureConfigNotif:

 description: Contains the notification of time synchronization service state.

 type: object

 properties:

 configNotifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 stateOfConfig:

 type: string

 required:

 - configNotifId

 - stateOfConfig

 PtpCapabilitiesPerUe:

 description: Contains the supported PTP capabilities per UE.

 type: object

 properties:

 gpsi:

 $ref: '#/components/schemas/Gpsi'

 ptpCaps:

 type: array

 items:

 $ref: '#/components/schemas/EventFilter'

 minItems: 1

 required:

 - gpsi

 - ptpCaps

 Operation:

 anyOf:

 - type: string

 enum:

 - BOUNDARY\_CLOCK

 - P2P\_TRANS\_CLOCK

 - E2E\_TRANS\_CLOCK

 - type: string

 description: >

 This string identifies supported operation.

 description: >

 Possible values are

 - BOUNDARY\_CLOCK: Boundary Clock is supported.

 - P2P\_TRANS\_CLOCK: Peer-to-peer Transparent Clock is supported.

 - E2E\_TRANS\_CLOCK: End-to-end Transparent Clock is supported.

 Protocol:

 anyOf:

 - type: string

 enum:

 - ETH

 - UDP\_IPV4

 - UDP\_IPV6

 - type: string

 description: >

 This string identifies supported protocol.

 description: >

 Possible values are

 - ETH: Ethernet is supported.

 - UDP\_IPV4: UDP over IPv4 is supported.

 - UDP\_IPV6: UDP over IPv6 is supported.

 GmCapable:

 anyOf:

 - type: string

 enum:

 - GPTP

 - PTP

 - type: string

 description: >

 This string identifies supported grandmaste.

 description: >

 Possible values are

 - GPTP: gPTP grandmaster is supported.

 - PTP: PTP grandmaste is supported.

 SubscribedEvent:

 anyOf:

 - type: string

 enum:

 - AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE

 - type: string

 description: >

 This string identifies supported event.

 description: >

 Possible values are

 - AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE: The UE is availability for time synchronization service.

\*\*\* End of Changes \*\*\*