**TSG-CT WG3 Meeting #118-e *C3-215079***

**E-Meeting, 11th – 15th October 2021 (Revision of C3-215xyz)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.522** | **CR** | 0413 | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of the Time Synchronization Exposure Configuration | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | IIoT | | | | |  | ***Date:*** | | | 2021-10-11 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The PTP instance Id is created by the NEF for the time synchronization exposure configuration.  As defined in clause 4.15.9.3, the NEF privides the T Time Synchronization service parameters as follows (S2-2106773):   |  |  | | --- | --- | | Time Synchronization Parameter | Description | | PTP instance type | Identifies the requested PTP instance type as described in clause 5.27.1.4 in TS 23.501 [2]. | | Transport protocol | Identifies the requested transport protocol for PTP instance as described in clause 5.27.1.4 in TS 23.501 [2]. | | PTP Profile | Identifies the PTP profile for the PTP instance as requested by AF. | | Grandmaster enabled | Indicates whether the AF requests the PTP instance in 5GS to be able to act as a grandmaster for PTP or gPTP (depending on the requested PTP instance type).  This is applicable for IEEE Std 1588 [76] or IEEE Std 802.1AS [75] operation.  [optional] | | Grandmaster priority | Indicates a priority used as defaultDS.priority1 when generating Announce message when 5GS acts as (g)PTP GM. Applicable only if the Grandmaster enabled = TRUE.  [optional] | | Time Domain | (g)PTP domain of the PTP instance as defined in IEEE Std 1588 [76].  [ | | Temporal Validity Condition | Indicates start-time and stop-time attributes that describe the time period when the time synchronization service for a PTP instance is active. [optional] | | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Restruct the data types to align with stage 2 requirement.  instanceId is used to identify the resource created by the Nnef\_TimeSynchronization\_ConfigCreate operation | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Not aligned with stage 2. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.4.24.2, 5.15.1.1, 5.15.1.4.3.3, 5.15.4.3.6, A.13 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backward compatible feature to the OpenAPI file of TimeSyncExposure API. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**Additional discussion(if needed):**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

#### 4.4.24.2 Time Synchronization Exposure Configuration

The procedures are used by the AF to activate, modify or deactivate the (g)PTP instances by performing the time synchronization configuration at the NEF.

In order to configure the time synchronization parameters, the AF shall initiate an HTTP POST request to the NEF for the "Time Synchronization Exposure Configurations" resource. The body of the HTTP POST message shall include the Time Synchronization related parameters within the TimeSyncExposureConfig data structure.

Upon receipt of the corresponding HTTP POST message and the request is authorized by the NEF, the NEF invokes the Ntsctsf\_TimeSynchronization\_ConfigCreate service operation with the corresponding TSCTSF as defined in 3GPP TS 29.565 [50]. After receiving a successful response from the TSCTSF, the NEF shall create a new resource and assign an identifier for the "Individual Time Synchronization Exposure Configuration" resource. Then the NEF shall send a HTTP "201 Created" response with TimeSyncExposureConfig data structure as response body and a Location header field containing the URI of the created individual resource.

In order to update an existing Individual Time Synchronization Exposure Configuration, the AF may send an HTTP PUT message to the resource "Individual Time Synchronization Exposure Configuration" requesting the NEF to change all properties in the existing resource. The body of the HTTP PUT request message shall include TimeSyncExposureConfig data type as defined in subclause 5.15.4.3.6. The user plane node Id shall remain unchanged from previous values.

Upon receipt of the corresponding HTTP PUT message and the request is authorized by the NEF, the NEF shall interact with the TSCTSF to modify an existing resource at the TSCTSF by using Ntsctsf\_TimeSynchronization\_ConfigUpdate service operation as defined in 3GPP TS 29.565 [50]. If the modification request is accepted by the TSCTSF and the TSCTSF informs the NEF with a successful response, the NEF shall update the existing resource for the "Individual Time Synchronization Exposure Configuration" resource. Then the NEF shall send a HTTP response including "200 OK" status code with TimeSyncExposureConfig data structure or "204 No Content" status code.

When the NEF receives the notification of the current state of time synchronization service configuration from the TSCSF by Ntsctsf\_TimeSynchronization\_ConfigUpdateNotify service operation defined in 3GPP TS 29.565 [50], the NEF shall provide a notification to AF by sending HTTP POST message that include the TimeSyncExposureConfigNotif data structure in the request body. Upon receipt of the notification, the AF shall respond with a "204 No Content" status code to confirm the received notification.

To delete an existing "Individual Time Synchronization Exposure Configuration", the AF shall initiate an HTTP DELETE request to the NEF for the "Individual Time Synchronization Exposure Subscription" resource.

Upon receipt of the corresponding HTTP DELETE message, if the AF is authorized, the NEF shall interact with the TSCTSF to delete an existing Individual Time Synchronization Exposure Configuration at the TSCTSF by using Ntsctsf\_TimeSynchronization\_ConfigDelete service operation as defined in 3GPP TS 29.565 [50]. If the request is accepted by the TSCTSF, the NEF shall delete the existing resource for the "Individual Time Synchronization Exposure Configuration" resource. Then the NEF shall send a HTTP "204 No Content" response.

\*\*\* Next change \*\*\*

#### 5.15.1.1 Overview

All resource URIs of this API should have the following root:

**{apiRoot}/3gpp-time-sync/v1**

"apiRoot" is set as described in subclause 5.2.4 in 3GPP TS 29.122 [4]. "apiName" shall be set to "**3gpp-time-sync**" and "apiVersion" shall be set to "v1" for the current version defined in the present document. All resource URIs in the subclauses below are defined relative to the above root URI.

This subclause describes the structure for the Resource URIs as shown in figure 5.15.1.1-1 and the resources and HTTP methods used for the TimeSyncExposure API.



Figure 5.15.1.1-1: Resource URI structure of the TimeSyncExposure API

Table 5.15.1.1-1 provides an overview of the resources and HTTP methods applicable for the TimeSyncExposure API.

Table 5.15.1.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method | Description |
| Time Synchronization Exposure Subscriptions | /{afId}/subscriptions | GET | Read all subscriptions for a given AF |
| POST | Create a new subscription to time synchronization exposure |
| Individual Time Synchronization Exposure Subscription | /{afId}/subscriptions/{subscriptionId} | GET | Read a subscription to time synchronization exposure |
| PUT | Modify all of the properties of an existing subscription to time synchronization exposure |
| DELETE | Delete a subscription to time synchronization exposure |
| Time Synchronization Exposure Configurations | /{afId}/subscriptions/{subscriptionId}/configurations | GET | Read all configurations for a given AF and subscription |
| POST | Create a new configuration to time synchronization exposure |
| Individual Time Synchronization Exposure Configuration | /{afId}/subscriptions/{subscriptionId}/configurations/{instanceId} | GET | Read a configuration to time synchronization exposure |
| PUT | Modify all of the properties of an existing configuration to time synchronization exposure |
| DELETE | Delete a configuration to time synchronization exposure |

\*\*\* Next change \*\*\*

###### 5.15.1.4.3.3 POST

The POST method creates a new configuration resource to activate time synchronization service for a given AF. The AF shall initiate the HTTP POST request message and the NEF shall respond to the message. The NEF shall construct the URI of the created resource.

This method shall support the request data structures specified in table 5.15.1.4.3.3-1 and the response data structures and response codes specified in table 5.15.1.4.3.3-2.

Table 5.15.1.4.3.3-1: Data structures supported by the POSTRequest Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| TimeSyncExposureConfig | M | 1 | Parameters to create a configuration and to activate time synchronization service. |

Table 5.15.1.2.4.3-2: Data structures supported by thePOST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| TimeSyncExposureConfig | M | 1 | 201 Created | The subscription was created successfully.  The URI of the created resource shall be returned in the "Location" HTTP header. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in table 5.2.6-1 of 3GPP TS 29.122 [4] also apply. | | | | |

Table 5.15.1.4.3.3-3: Headers supported by the 201 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/3gpp-time-sync/v1/{afId}/subscriptions/{subscriptionId}/configurations/{instanceId} |

\*\*\* Next change \*\*\*

##### 5.15.1.5.2 Resource Definition

Resource URI: **{apiRoot}/3gpp-time-sync/v1/{afId}/subscriptions/{subscriptionId}/configuration/{instanceId}**

This resource shall support the resource URI variables defined in table 5.15.1.5.2-1.

Table 5.15.1.5.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | Subclause 5.2.4 of 3GPP TS 29.122 [4]. |
| afId | string | Identifier of the AF. |
| subscriptionId | string | Identifier of the subscription resource. |
| instanceId | string | Identifier of the PTP instance resource |

\*\*\* Next change \*\*\*

##### 5.15.4.3.6 Type: TimeSyncExposureConfig

Table 5.15.4.3.6-1: Definition of type TimeSyncExposureConfig

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| upNodeId | Uint64 | M | 1 | Identifies the applicable NW-TT. Contains a TSC user plane node Id. If integrated with TSN, the user plane node Id is a bridge Id defined in IEEE 802.1Q [41] clause 14.2.5. |  |
| reqPtpIn | PtpInstance | M | 1 | Identifies the PtP instance requested by the AF. |  |
| gmEnable | boolean | O | 0..1 | Indicates that the AF requests 5GS to act as a grandmaster for PTP or gPTP if it is included and set to true. The default value "false" shall apply, if the attribute is not present. |  |
| gmPrio | Uinteger | C | 0..1 | Indicates a priority used as defaultDS.priority1 when generating Announce message when 5GS acts as (g)PTP GM. It may be present if the "gmEnable" is set to true. |  |
| timeDom | Uinteger | M | 1 | Indicate the (g)PTP domain that the (TSN)AF is located in. |  |
| tempValidity | TemporalValidity | O | 0..1 | Indicates the time period when the time synchronization service for a PTP instance is active |  |
| configNotifUri | Uri | M | 1 | Notification URI for configuration state reporting. |  |
| configNotifId | string | M | 1 | Notification Correlation ID assigned by the NF service consumer. |  |

Editor's note: How a clock accuracy parameter as well as other parameters for time synchronization can be supported is FFS.

\*\*\* Next change \*\*\*

# A.13 TimeSyncExposure API

openapi: 3.0.0

info:

title: 3gpp-time-sync-exposure

version: 1.0.0-alpha.2

description: |

API for time synchronization exposure.

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.522 V17.3.0; 5G System; Network Exposure Function Northbound APIs.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-time-sync/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{afId}/subscriptions:

get:

summary: read all of the active subscriptions for the AF

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active subscriptions for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource

tags:

- Time Synchronization Exposure Subscriptions

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

requestBody:

description: new subscription creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncSubsNotification:

'{$request.body#/subsNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Capability for a list of UEs.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}:

get:

summary: read an active subscription for the AF and the subscription Id

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureSubsc'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations:

get:

summary: read all of the active configurations for the AF

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: String identifying the individual synchronization Exposure Subscription resource in the NEF

in: path

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active configurations for the AF)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TimeSyncExposureConfig'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new configuration resource

tags:

- Time Synchronization Exposure Configurations

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

description: String identifying the individual synchronization Exposure Subscription resource in the NEF

in: path

required: true

schema:

type: string

requestBody:

description: new configuration creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'201':

description: Created (Successful creation)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

timeSyncConfigNotification:

'{$request.body#/configNotifUri}':

post:

requestBody:

description: Notification for Time Synchronization Service status.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfigNotif'

responses:

'204':

description: Expected response to a successful callback processing without a body

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{afId}/subscriptions/{subscriptionId}/configurations/{instanceId}:

get:

summary: read an active subscription for the AF and the subscription Id

tags:

- Individual Time Synchronization Exposure Subscription

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing configuration resource

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing configuration

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

responses:

'200':

description: OK (Successful deletion of the existing configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/TimeSyncExposureConfig'

'204':

description: Successful case. The resource has been successfully updated and no additional content is to be sent in the response message.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing configuration

tags:

- Individual Time Synchronization Exposure Configuration

parameters:

- name: afId

in: path

description: Identifier of the AF

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

- name: instanceId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing configuration)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

TimeSyncExposureSubsc:

description: Contains requested parameters for the subscription to the notification of time synchronization capability.

type: object

properties:

exterGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: Contains a list of UE for which the time synchronization capabilities is requested.

anyUeInd:

type: boolean

description: Any UE indication. This IE shall be present if the event subscription is applicable to any UE. Default value "false" is used, if not present.

afServiceId:

type: string

description: Identifies a service on behalf of which the AF is issuing the request.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

subsNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

subscribedEvents:

type: array

items:

$ref: '#/components/schemas/SubscribedEvent'

minItems: 1

description: Subscribed events

notifMethod:

$ref: 'TS29508\_Nsmf\_EventExposure.yaml#/components/schemas/NotificationMethod'

maxReportNbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3 of 3GPP TS 29.122. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- subsNotifUri

- subsNotifId

TimeSyncCapability:

description: Contains time synchronization capability.

type: object

properties:

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

description: Contains a list of UE for which the time synchronization capabilities is applicable.

gpsis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

minItems: 1

description: Contains a list of UE for which the time synchronization capabilities is applicable.

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

disMethods:

$ref: '#/components/schemas/DistributionMethod'

gmCapable:

$ref: '#/components/schemas/GmCapable'

ptpProfiles:

type: string

description: Identifies the PTP profiles supported by 5GS for the reported UE.

DistributionMethod:

description: Contains the time synchronization distribution methods.

type: object

properties:

1588mes:

$ref: '#/components/schemas/1588Method'

1asMe:

type: boolean

description: Indicates that the IEEE Std 802.1AS-2020 method is supported if it is included and set to true.

5gClockMe:

type: boolean

description: Indicates that Access Stratum-based 5G clock sync is supported if it is included and set to true.

1588Method:

description: Contains time synchronization distribution methods defined in IEEE Std 1588-2019.

type: object

properties:

op:

$ref: '#/components/schemas/Operation'

pro:

$ref: '#/components/schemas/Protocol'

required:

- op

- pro

TimeSyncExposureConfig:

description: Contains the Time Synchronization Configuration parameters.

type: object

properties:

upNodeId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

reqPtpIn:

$ref: '#/components/schemas/PtpInstance'

gmEnable:

type: boolean

description: Indicates that the AF requests 5GS to act as a grandmaster for PTP or gPTP if it is included and set to true.

gmPrio:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

timeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

configNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

tempValidity:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

required:

- upNodeId

- reqPtpIn

- timeDom

- configNotifId

- configNotifUri

TimeSyncExposureSubsNotif:

description: Contains the notification of time synchronization capability.

type: object

properties:

subsNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

eventNotifs:

type: array

items:

$ref: '#/components/schemas/SubsEventNotification'

minItems: 1

required:

- subsNotifId

- eventNotifs

SubsEventNotification:

description: Notifications about subscribed Individual Events.

type: object

properties:

event:

$ref: '#/components/schemas/SubscribedEvent'

timeSyncCapas:

type: array

items:

$ref: '#/components/schemas/TimeSyncCapability'

minItems: 1

required:

- event

TimeSyncExposureConfigNotif:

description: Contains the notification of time synchronization service state.

type: object

properties:

configNotifId:

type: string

description: Notification Correlation ID assigned by the NF service consumer.

stateOfConfig:

type: string

required:

- configNotifId

- stateOfConfig

Operation:

anyOf:

- type: string

enum:

- BOUNDARY\_CLOCK

- P2P\_TRANS\_CLOCK

- E2E\_TRANS\_CLOCK

- type: string

description: >

This string identifies supported operation.

description: >

Possible values are

- BOUNDARY\_CLOCK: Boundary Clock is supported.

- P2P\_TRANS\_CLOCK: Peer-to-peer Transparent Clock is supported.

- E2E\_TRANS\_CLOCK: End-to-end Transparent Clock is supported.

Protocol:

anyOf:

- type: string

enum:

- ETH

- UDP\_IPV4

- UDP\_IPV6

- type: string

description: >

This string identifies supported protocol.

description: >

Possible values are

- ETH: Ethernet is supported.

- UDP\_IPV4: UDP over IPv4 is supported.

- UDP\_IPV6: UDP over IPv6 is supported.

GmCapable:

anyOf:

- type: string

enum:

- GPTP

- PTP

- type: string

description: >

This string identifies supported grandmaste.

description: >

Possible values are

- GPTP: gPTP grandmaster is supported.

- PTP: PTP grandmaste is supported.

SubscribedEvent:

anyOf:

- type: string

enum:

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE

- type: string

description: >

This string identifies supported event.

description: >

Possible values are

- AVAILABILITY\_FOR\_TIME\_SYNC\_SERVICE: The UE is availability for time synchronization service.

\*\*\* End of Changes \*\*\*