**3GPP TSG-CT3 Meeting #118e C3-215277\_r2**

**E-Meeting, 11th – 15th October 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.519** | **CR** | **0283** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Updates to the 5G ProSe service parameters |
|  |  |
| ***Source to WG:*** | Huawei, CATT |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | 5G\_ProSe |  | ***Date:*** | 2021-09-30 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Based on the progress of CT1 on 5G ProSe, the following aspects have been clarified/updated:* CT1 has defined the encoding of the UE policies and configuration parameters for 5G ProSe UE-to-network relay in TS 29.555 and divided them into two separate parts:
	+ UE policies / Service parameters for 5G ProSe UE-to-network relay UE.
	+ UE policies / Service parameters for 5G ProSe remote UE.
* In addition, CR C3-214312 agreed during last meeting omitted to remove the service parameters for 5G ProSe usage reporting configuration and rules and the service parameters for 5G ProSe service path selection from the OpenAPI file of the Nudr\_DataRepository API for Application Data.
 |
|  |  |
| ***Summary of change:*** | This CR proposes to:* In order to align with CT1, CR C3-215xxx defines separate attributes and data types for the two components of the UE policies / Service parameters for 5G ProSe UE-to-network relay, i.e. UE policies / Service parameters for 5G ProSe UE-to-network relay UE and UE policies / Service parameters for 5G ProSe remote UE. This CR proposes to align with it.
* Remove the attributes and data types related to the service parameters for 5G ProSe usage reporting configuration and rules and the service parameters for 5G ProSe service path selection from the OpenAPI file of the Nudr\_DataRepository API for Application Data.
 |
|  |  |
| ***Consequences if not approved:*** | * Misalignment with the Stage 3 work in CT1.
 |
|  |  |
| ***Clauses affected:*** | 6.4.1, 6.4.2.15, A.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backwards compatible new features and corrections to the OpenAPI specification file of the Nudr\_DataRepository API for Application Data. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* Start of changes \* \* \* \*

### 6.4.1 General

This subclause specifies the application data model supported by the API.

Table 6.4.1-1 specifies the data types defined for the Nudr\_DataRepository Service API for Application Data service based interface protocol.

Table 6.4.1-1: Nudr\_DataRepository specific Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AmInfluData | 6.4.2.16 | Contains AM influence data. |  |
| AmInfluDataPatch | 6.4.2.17 | Contains AM influence data that can be updated. |  |
| ApplicationDataSubs | 6.4.2.10 | Contains application data subscription data. |  |
| ApplicationDataChangeNotif | 6.4.2.11 | Contains the new or updated application data or removed indication. |  |
| BdtPolicyData | 6.4.2.7 | Contains applied BDT policy data. | EnhancedBackgroundDataTransfer |
| BdtPolicyDataPatch | 6.4.2.8 | Contains modification instructions to be performed on the applied BDT policy data. | EnhancedBackgroundDataTransfer |
| DataInd | 6.4.3.3 | Indicates the type of data. |  |
| DataFilter | 6.4.2.12 | Indicates a data filter. |  |
| IptvConfigData | 6.4.2.9 | Represents IPTV configuration data information. |  |
| PfdDataForAppExt | 6.4.2.6 | The PFDs and related data for the application |  |
| ServiceParameterData | 6.4.2.15 | Contains the service parameter data. |  |
| TrafficInfluData | 6.4.2.2 | Contains traffic influence data. |  |
| TrafficInfluDataPatch | 6.4.2.3 | Contains modification instructions to be performed on the traffic influence data. |  |
| TrafficInfluDataNotif | 6.4.2.14 | Contains traffic influence data for notification. | EnhancedInfluDataNotification |
| TrafficInfluSub | 6.4.2.4 | Contains traffic influence subscription data. |  |

Table 6.4.1-2 specifies data types re-used by the Nudr\_DataRepository Service API for Application Data service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nudr\_DataRepository Service API for Application Data service based interface.

Table 6.4.1-2: Nudr\_DataRepository re-used Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AmInfluEvent | 3GPP TS 29.522 [19] | Identifies the type of AM related events of which the AF requests to be notified. |  |
| ApplicationId | 3GPP TS 29.571 [7] | Indicates an application identifier. |  |
| BdtReferenceId | 3GPP TS 29.122 [9] | Identifies a selected policy of background data transfer. | EnhancedBackgroundDataTransfer |
| DateTime | 3GPP TS 29.571 [7] | Indicates a date and time. |  |
| DnaiChangeType | 3GPP TS 29.571 [7] | Describes the types of DNAI change. |  |
| Dnn | 3GPP TS 29.571 [7] | Identifies a Data Network Name. |  |
| EthFlowDescription | 3GPP TS 29.514 [16] | Contains the Ethernet data flow information.(NOTE) |  |
| FlowInfo | 3GPP TS 29.122 [9] | Contains the flow information. |  |
| IptvConfigDataPatch | 3GPP TS 29.522 [19] | Contains the IPTV configuration data used for PATCH. |  |
| Ipv4Addr | 3GPP TS 29.571 [7] | Identifies an IPv4 address. |  |
| Ipv6Addr | 3GPP TS 29.571 [7] | Identifies an IPv6 address. |  |
| MacAddr48 | 3GPP TS 29.571 [7] | MAC Address. |  |
| MulticastAccessControl | 3GPP TS 29.522 [19] | Represents the multicast access control information. |  |
| NetworkAreaInfo | 3GPP TS 29.554 [13] | Describes a network area information. |  |
| ParameterOverPc5 | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over PC5. |  |
| ParameterOverUu | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over Uu. |  |
| ParamForProSeDd | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| ParamForProSeDc | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| ParamForProSeU2NRelUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| ParamForProSeRemUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| PfdChangeNotification | 3GPP TS 29.551 [8] | Describes the PFD change. |  |
| PfdDataForApp | 3GPP TS 29.551 [8] | Identifies the PFDs for one application identifier. |  |
| RouteToLocation | 3GPP TS 29.571 [7] | Identifies the N6 traffic routing requirement. |  |
| ServiceParamterDataPatch | 3GPP TS 29.522 [19] | Contains the service parameter data. |  |
| Snssai | 3GPP TS 29.571 [7] | Identifies a Single Network Slice Selection Assistance Information. |  |
| SubscribedEvent | 3GPP TS 29.522 [19] | Identified the type of UP path management events of which the AF requests to be notified. |  |
| Supi | 3GPP TS 29.571 [7] | Identifies a SUPI that shall contain either an IMSI or an NAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [7] | Used to negotiate the applicability of the optional features. |  |
| TemporalValidity | 3GPP TS 29.514 [16] | Indicates the time interval during which the AF request is to be applied. | MultiTemporalCondition |
| Uri | 3GPP TS 29.571 [7] | Identifies a URI. |  |
| UrspRuleRequest | 3GPP TS 29.522 [19] | Contains service parameter data used to influence the URSP. | EnEDGE |
| UserPlaneLatencyRequirements | 3GPP TS 29.512 [12] | User Plane Latency Requirements. | EnEDGE |
| NOTE: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange as specified in clause 6.1.8 of TS 29.504 [6] shall be supported. |

\* \* \* Next changes \* \* \* \*

#### 6.4.2.15 Type ServiceParameterData

Table 6.4.2.15-1: Definition of type ServiceParameterData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnn | Dnn | O | 0..1 | Identifies a DNN. (NOTE 2) |  |
| snssai | Snssai | O | 0..1 | Identifies an S-NSSAI. (NOTE 2) |  |
| appId | string | O | 0..1 | Identifies an application identifier. (NOTE 2) |  |
| supi | Supi | O | 0..1 | Identifies a user. (NOTE1) |  |
| ueIpv4 | Ipv4Addr | O | 0..1 | The IPv4 address of the served UE. (NOTE1) |  |
| ueIpv6 | Ipv6Addr | O | 0..1 | The IPv6 address of the served UE. (NOTE1) |  |
| ueMac | MacAddr48 | O | 0..1 | The MAC address of the served UE. (NOTE1) |  |
| interGroupId | GroupId | O | 0..1 | Identifies a group of users. (NOTE1) |  |
| anyUeInd | boolean | O | 0..1 | Identifies whether the service parameters applies to any UE. This attribute shall set to "true" if applicable for any UE, otherwise, set to "false". (NOTE1) |  |
| paramOverPc5 | ParameterOverPc5 | O | 0..1 | Contains the V2X service parameters used over PC5 |  |
| paramOverUu | ParameterOverUu | O | 0..1 | Contains the V2X service parameters used over Uu |  |
| urspInfluence | array(UrspRuleRequest) | O | 1..N | Contains the service parameter used to influence the URSP. | EnEDGE |
| paramForProSeDd | ParamForProSeDd | O | 0..1 | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| paramForProSeDc | ParamForProSeDc | O | 0..1 | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| paramForProSeU2NRelUe | ParamForProSeU2NRelUe | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| paramForProSeRemUe | ParamForProSeRemUe | O | 0..1 | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of Supported features used as described in subclause 5.8.This parameter shall be supplied in the PUT request that requested the creation of an individual Service parameter resource, and in the PUT response. |  |
| resUri | Uri | C | 0..1 | Represents the URI of Individual Service Parameter Data.It shall only be included in the HTTP GET response. |  |
| NOTE 1: Only one of the "supi", "anyUeInd", "interGroupId", "ueIpv4", "ueIpv6" or "ueMac" attribute shall be provided.NOTE 2: Only the combination of "dnn" and "snssai" or "appId" attribute shall be provided. |

Editor's Note: It is FFS to consider if "urspInfluence" should be encoded exactly in the same way that URSP rules are encoded in NAS messages (see TS 24.526).

Editor's Note: It is FFS to consider if a separate UDR feature should be used for "urspInfluence" instead of the EnEDGE feature.

\* \* \* Next changes \* \* \* \*

# A.3 Nudr\_DataRepository API for Application Data

For the purpose of referencing entities in the Open API file defined in this Annex, it shall be assumed that this Open API file is contained in a physical file named "TS29519\_Application\_Data.yaml".

openapi: 3.0.0

info:

 version: '-'

 title: Unified Data Repository Service API file for Application Data

 description: |

 The API version is defined in 3GPP TS 29.504

 © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.519 V17.4.0; 5G System; Usage of the Unified Data Repository Service for Policy Data, Application Data and Structured Data for Exposure.

 url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.519/'

paths:

 /application-data/pfds:

 get:

 summary: Retrieve PFDs for application identifier(s)

 operationId: ReadPFDData

 tags:

 - PFD Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: appId

 in: query

 description: Contains the information of the application identifier(s) for the querying PFD Data resource. If none appId is included in the URI, it applies to all application identifier(s) for the querying PFD Data resource.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 responses:

 '200':

 description: A representation of PFDs for request applications is returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/PfdDataForAppExt'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/pfds/{appId}:

 get:

 summary: Retrieve the corresponding PFDs of the specified application identifier

 operationId: ReadIndividualPFDData

 tags:

 - Individual PFD Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: appId

 in: path

 description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of PFDs for the request application identified by the application identifier is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PfdDataForAppExt'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete the corresponding PFDs of the specified application identifier

 operationId: DeleteIndividualPFDData

 tags:

 - Individual PFD Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: appId

 in: path

 description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: Successful case. The Individual PFD Data resource related to the application identifier was deleted.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Create or update the corresponding PFDs for the specified application identifier

 operationId: CreateOrReplaceIndividualPFDData

 tags:

 - Individual PFD Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PfdDataForAppExt'

 parameters:

 - name: appId

 in: path

 description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual PFD Data resource related to the application-identifier is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PfdDataForAppExt'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/pfds/{appId}'

 required: true

 schema:

 type: string

 '200':

 description: Successful case. The upgrade of an Individual PFD Data resource related to the application identifier is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PfdDataForAppExt'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/influenceData:

 get:

 summary: Retrieve Traffic Influence Data

 operationId: ReadInfluenceData

 tags:

 - Influence Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: influence-Ids

 in: query

 description: Each element identifies a service.

 required: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: dnns

 in: query

 description: Each element identifies a DNN.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 - name: snssais

 in: query

 description: Each element identifies a slice.

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 - name: internal-Group-Ids

 in: query

 description: Each element identifies a group of users.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 - name: supis

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 - name: supp-feat

 in: query

 required: false

 description: Supported Features

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: The Traffic Influence Data stored in the UDR are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/TrafficInfluData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/influenceData/{influenceId}:

 put:

 summary: Create or update an individual Influence Data resource

 operationId: CreateOrReplaceIndividualInfluenceData

 tags:

 - Individual Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluData'

 parameters:

 - name: influenceId

 in: path

 description: The Identifier of an Individual Influence Data to be created or updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual Traffic Influence Data resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/influenceData/{influenceId}'

 required: true

 schema:

 type: string

 '200':

 description: The update of an Individual Traffic Influence Data resource is confirmed and a response body containing Traffic Influence Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modify part of the properties of an individual Influence Data resource

 operationId: UpdateIndividualInfluenceData

 tags:

 - Individual Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/TrafficInfluDataPatch'

 parameters:

 - name: influenceId

 in: path

 description: The Identifier of an Individual Influence Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The update of an Individual Traffic Influence Data resource is confirmed and a response body containing Traffic Influence Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual Influence Data resource

 operationId: DeleteIndividualInfluenceData

 tags:

 - Individual Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: influenceId

 in: path

 description: The Identifier of an Individual Influence Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual Influence Data was deleted successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/influenceData/subs-to-notify:

 post:

 summary: Create a new Individual Influence Data Subscription resource

 operationId: CreateIndividualInfluenceDataSubscription

 tags:

 - Influence Data Subscriptions (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluSub'

 responses:

 '201':

 description: The subscription was created successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluSub'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 trafficInfluenceDataChangeNotification:

 '{$request.body#/notificationUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 oneOf:

 - $ref: '#/components/schemas/TrafficInfluData'

 - $ref: '#/components/schemas/TrafficInfluDataNotif'

 minItems: 1

 responses:

 '204':

 description: No Content, Notification was successful

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 get:

 summary: Read Influence Data Subscriptions

 operationId: ReadInfluenceDataSubscriptions

 tags:

 - Influence Data Subscriptions (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: dnn

 in: query

 description: Identifies a DNN.

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 - name: snssai

 in: query

 description: Identifies a slice.

 required: false

 content:

 application/json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 - name: internal-Group-Id

 in: query

 description: Identifies a group of users.

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 - name: supi

 in: query

 description: Identifies a user.

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 responses:

 '200':

 description: The subscription information as request in the request URI query parameter(s) are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/TrafficInfluSub'

 minItems: 0

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/influenceData/subs-to-notify/{subscriptionId}:

 get:

 summary: Get an existing individual Influence Data Subscription resource

 operationId: ReadIndividualInfluenceDataSubscription

 tags:

 - Individual Influence Data Subscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Individual Influence Data Subscription

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The subscription information is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluSub'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 summary: Modify an existing individual Influence Data Subscription resource

 operationId: ReplaceIndividualInfluenceDataSubscription

 tags:

 - Individual Influence Data Subscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluSub'

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Individual Influence Data Subscription

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The subscription was updated successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TrafficInfluSub'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual Influence Data Subscription resource

 operationId: DeleteIndividualInfluenceDataSubscription

 tags:

 - Individual Influence Data Subscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: subscriptionId

 in: path

 description: String identifying a subscription to the Individual Influence Data Subscription

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The subscription was terminated successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/bdtPolicyData:

 get:

 summary: Retrieve applied BDT Policy Data

 operationId: ReadBdtPolicyData

 tags:

 - BdtPolicy Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: bdt-policy-ids

 in: query

 description: Each element identifies a service.

 required: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: internal-group-ids

 in: query

 description: Each element identifies a group of users.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 - name: supis

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 responses:

 '200':

 description: The applied BDT policy Data stored in the UDR are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/BdtPolicyData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/bdtPolicyData/{bdtPolicyId}:

 put:

 summary: Create an individual applied BDT Policy Data resource

 operationId: CreateIndividualAppliedBdtPolicyData

 tags:

 - Individual Applied BDT Policy Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicyData'

 parameters:

 - name: bdtPolicyId

 in: path

 description: The Identifier of an Individual Applied BDT Policy Data to be created or updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual Applied BDT Policy Data resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicyData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/bdtPolicyData/{bdtPolicyId}'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modify part of the properties of an individual Applied BDT Policy Data resource

 operationId: UpdateIndividualAppliedBdtPolicyData

 tags:

 - Individual Applied BDT Policy Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/BdtPolicyDataPatch'

 parameters:

 - name: bdtPolicyId

 in: path

 description: The Identifier of an Individual Applied BDT Policy Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The update of an Individual Applied BDT Policy Data resource is confirmed and a response body containing Applied BDT Policy Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/BdtPolicyData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual Applied BDT Policy Data resource

 operationId: DeleteIndividualAppliedBdtPolicyData

 tags:

 - Individual Applied BDT Policy Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: bdtPolicyId

 in: path

 description: The Identifier of an Individual Applied BDT Policy Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual Applied BDT Policy Data was deleted successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/iptvConfigData:

 get:

 summary: Retrieve IPTV configuration Data

 operationId: ReadIPTVCongifurationData

 tags:

 - IPTV Configuration Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: config-ids

 in: query

 description: Each element identifies a configuration.

 required: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: dnns

 in: query

 description: Each element identifies a DNN.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 - name: snssais

 in: query

 description: Each element identifies a slice.

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 - name: supis

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 - name: inter-group-ids

 in: query

 description: Each element identifies a group of users.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 responses:

 '200':

 description: The IPTV configuration data stored in the UDR are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/IptvConfigData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/iptvConfigData/{configurationId}:

 put:

 summary: Create or update an individual IPTV configuration resource

 operationId: CreateOrReplaceIndividualIPTVConfigurationData

 tags:

 - Individual IPTV Configuration Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 parameters:

 - name: configurationId

 in: path

 description: The Identifier of an Individual IPTV Configuration Data to be created or updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual IPTV Configuration Data resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '200':

 description: The update of an Individual IPTV configuration resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Partial update an individual IPTV configuration resource

 operationId: PartialReplaceIndividualIPTVConfigurationData

 tags:

 - Individual IPTV Configuration Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/IptvConfigDataPatch'

 parameters:

 - name: configurationId

 in: path

 description: The Identifier of an Individual IPTV Configuration Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The update of an Individual IPTV configuration resource.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/IptvConfigData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual IPTV configuration resource

 operationId: DeleteIndividualIPTVConfigurationData

 tags:

 - Individual IPTV Configuration Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: configurationId

 in: path

 description: The Identifier of an Individual IPTV Configuration to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The resource was deleted successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/serviceParamData:

 get:

 summary: Retrieve Service Parameter Data

 operationId: ReadServiceParameterData

 tags:

 - Service Parameter Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: service-param-ids

 in: query

 description: Each element identifies a service.

 required: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: dnns

 in: query

 description: Each element identifies a DNN.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 - name: snssais

 in: query

 description: Each element identifies a slice.

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 - name: internal-group-ids

 in: query

 description: Each element identifies a group of users.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 - name: supis

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 - name: ue-ipv4s

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 - name: ue-ipv6s

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 - name: ue-macs

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 minItems: 1

 - name: supp-feat

 in: query

 description: Supported Features

 required: false

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: The Service Parameter Data stored in the UDR are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/ServiceParameterData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/serviceParamData/{serviceParamId}:

 put:

 summary: Create or update an individual Service Parameter Data resource

 operationId: CreateOrReplaceServiceParameterData

 tags:

 - Individual Service Parameter Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceParameterData'

 parameters:

 - name: serviceParamId

 in: path

 description: The Identifier of an Individual Service Parameter Data to be created or updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual Service Parameter Data resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceParameterData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/serviceParamData/{serviceParamId}'

 required: true

 schema:

 type: string

 '200':

 description: The update of an Individual Service Parameter Data resource is confirmed and a response body containing Service Parameter Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceParameterData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modify part of the properties of an individual Service Parameter Data resource

 operationId: UpdateIndividualServiceParameterData

 tags:

 - Individual Service Parameter Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ServiceParameterDataPatch'

 parameters:

 - name: serviceParamId

 in: path

 description: The Identifier of an Individual Service Parameter Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The update of an Individual Service Parameter Data resource is confirmed and a response body containing Service Parameter Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ServiceParameterData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual Service Parameter Data resource

 operationId: DeleteIndividualServiceParameterData

 tags:

 - Individual Service Parameter Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: serviceParamId

 in: path

 description: The Identifier of an Individual Service Parameter Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual Service Parameter Data was deleted successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/am-influence-data:

 get:

 summary: Retrieve AM Influence Data

 operationId: ReadAmInfluenceData

 tags:

 - AM Influence Data (Store)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: am-Influence-Ids

 in: query

 description: Each element identifies a service.

 required: false

 schema:

 type: array

 items:

 type: string

 minItems: 1

 - name: dnns

 in: query

 description: Each element identifies a DNN.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 - name: snssais

 in: query

 description: Each element identifies a slice.

 required: false

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 - name: internal-Group-Ids

 in: query

 description: Each element identifies a group of users.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 - name: supis

 in: query

 description: Each element identifies the user.

 required: false

 schema:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 - name: supp-feat

 in: query

 required: false

 description: Supported Features

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 responses:

 '200':

 description: The AM Influence Data stored in the UDR are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/AmInfluData'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/am-influence-data/{amInfluenceId}:

 put:

 summary: Create or update an individual AM Influence Data resource

 operationId: CreateOrReplaceIndividualAmInfluenceData

 tags:

 - Individual AM Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AmInfluData'

 parameters:

 - name: amInfluenceId

 in: path

 description: The Identifier of an Individual AM Influence Data to be created or updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '201':

 description: The creation of an Individual AM Influence Data resource is confirmed and a representation of that resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AmInfluData'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/am-influence-data/{amInfluenceId}'

 required: true

 schema:

 type: string

 '200':

 description: The update of an Individual AM Influence Data resource is confirmed and a response body containing AM Influence Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AmInfluData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Modify part of the properties of an individual AM Influence Data resource

 operationId: UpdateIndividualAmInfluenceData

 tags:

 - Individual AM Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/AmInfluDataPatch'

 parameters:

 - name: amInfluenceId

 in: path

 description: The Identifier of an Individual AM Influence Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The update of an Individual AM Influence Data resource is confirmed and a response body containing AM Influence Data shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AmInfluData'

 '204':

 description: No content

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete an individual AM Influence Data resource

 operationId: DeleteIndividualAmInfluenceData

 tags:

 - Individual AM Influence Data (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: amInfluenceId

 in: path

 description: The Identifier of an Individual AM Influence Data to be updated. It shall apply the format of Data type string.

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The Individual AM Influence Data was deleted successfully.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/subs-to-notify:

 post:

 summary: Create a subscription to receive notification of application data changes

 operationId: CreateIndividualApplicationDataSubscription

 tags:

 - ApplicationDataSubscriptions (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ApplicationDataSubs'

 responses:

 '201':

 description: Upon success, a response body containing a representation of each Individual subscription resource shall be returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ApplicationDataSubs'

 headers:

 Location:

 description: 'Contains the URI of the newly created resource'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 applicationDataChangeNotif:

 '{$request.body#/notificationUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/ApplicationDataChangeNotif'

 minItems: 1

 responses:

 '204':

 description: No Content, Notification was successful

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 get:

 summary: Read Application Data change Subscriptions

 operationId: ReadApplicationDataChangeSubscriptions

 tags:

 - ApplicationDataSubscriptions (Collection)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: data-filter

 in: query

 description: The data filter for the query.

 required: false

 schema:

 $ref: '#/components/schemas/DataFilter'

 responses:

 '200':

 description: The subscription information as request in the request URI query parameter(s) are returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/ApplicationDataSubs'

 minItems: 0

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /application-data/subs-to-notify/{subsId}:

 parameters:

 - name: subsId

 in: path

 required: true

 schema:

 type: string

 put:

 summary: Modify a subscription to receive notification of application data changes

 operationId: ReplaceIndividualApplicationDataSubscription

 tags:

 - IndividualApplicationDataSubscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ApplicationDataSubs'

 responses:

 '200':

 description: The individual subscription resource was updated successfully.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ApplicationDataSubs'

 '204':

 description: The individual subscription resource was updated successfully and no additional content is to be sent in the response message.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Delete the individual Application Data subscription

 operationId: DeleteIndividualApplicationDataSubscription

 tags:

 - IndividualApplicationDataSubscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 responses:

 '204':

 description: Upon success, an empty response body shall be returned.

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 get:

 summary: Get an existing individual Application Data Subscription resource

 operationId: ReadIndividualApplicationDataSubscription

 tags:

 - IndividualApplicationDataSubscription (Document)

 security:

 - {}

 - oAuth2ClientCredentials:

 - nudr-dr

 - oAuth2ClientCredentials:

 - nudr-dr

 - nudr-dr:application-data

 parameters:

 - name: subsId

 in: path

 description: String identifying a subscription to the Individual Application Data Subscription

 required: true

 schema:

 type: string

 responses:

 '200':

 description: The subscription information is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ApplicationDataSubs'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '414':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/414'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 schemas:

 TrafficInfluData:

 description: Represents the Traffic Influence Data.

 type: object

 properties:

 upPathChgNotifCorreId:

 type: string

 description: Contains the Notification Correlation Id allocated by the NEF for the UP path change notification.

 appReloInd:

 type: boolean

 description: Identifies whether an application can be relocated once a location of the application has been selected.

 afAppId:

 type: string

 description: Identifies an application.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ethTrafficFilters:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 trafficFilters:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 trafficRoutes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 description: Identifies the N6 traffic routing requirement.

 traffCorreInd:

 type: boolean

 validStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 validEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tempValidities:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

 minItems: 1

 description: Identifies the temporal validities for the N6 traffic routing requirement.

 nwAreaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 upPathChgNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 headers:

 type: array

 items:

 type: string

 minItems: 1

 subscribedEvents:

 type: array

 items:

 $ref: 'TS29522\_TrafficInfluence.yaml#/components/schemas/SubscribedEvent'

 minItems: 1

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 afAckInd:

 type: boolean

 addrPreserInd:

 type: boolean

 upLatReq:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UserPlaneLatencyRequirements'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 allOf:

 - oneOf:

 - required: [afAppId]

 - required: [trafficFilters]

 - required: [ethTrafficFilters]

 - oneOf:

 - required: [supi]

 - required: [interGroupId]

 TrafficInfluDataPatch:

 description: Represents the Traffic Influence Data to be updated in the UDR.

 type: object

 properties:

 upPathChgNotifCorreId:

 type: string

 description: Contains the Notification Correlation Id allocated by the NEF for the UP path change notification.

 appReloInd:

 type: boolean

 description: Identifies whether an application can be relocated once a location of the application has been selected.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ethTrafficFilters:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 internalGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 trafficFilters:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 trafficRoutes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 description: Identifies the N6 traffic routing requirement.

 traffCorreInd:

 type: boolean

 validStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 validEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 tempValidities:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

 minItems: 1

 nullable: true

 description: Identifies the temporal validities for the N6 traffic routing requirement.

 nwAreaInfo:

 $ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

 upPathChgNotifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 headers:

 type: array

 items:

 type: string

 minItems: 1

 afAckInd:

 type: boolean

 addrPreserInd:

 type: boolean

 upLatReq:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UserPlaneLatencyRequirements'

 TrafficInfluSub:

 description: Represents traffic influence subscription data.

 type: object

 properties:

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 description: Each element identifies a DNN.

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 description: Each element identifies a slice.

 internalGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 description: Each element identifies a group of users.

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 description: Each element identifies the user.

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - notificationUri

 oneOf:

 - required: [dnns]

 - required: [snssais]

 - required: [internalGroupIds]

 - required: [supis]

 TrafficInfluDataNotif:

 description: Represents traffic influence data for notification.

 type: object

 properties:

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 trafficInfluData:

 $ref: '#/components/schemas/TrafficInfluData'

 required:

 - resUri

 PfdDataForAppExt:

 description: Represents the PFDs and related data for the application.

 allOf:

 - $ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdDataForApp'

 - type: object

 properties:

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 BdtPolicyData:

 description: Represents applied BDT policy data.

 type: object

 properties:

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - bdtRefId

 BdtPolicyDataPatch:

 description: Represents modification instructions to be performed on the applied BDT policy data.

 type: object

 properties:

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 required:

 - bdtRefId

 IptvConfigData:

 description: Represents IPTV configuration data information.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 interGroupId:

 description: Identifies a group of users.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 afAppId:

 type: string

 multiAccCtrls:

 type: object

 additionalProperties:

 $ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/MulticastAccessControl'

 minProperties: 1

 description: Identifies a list of multicast address access control information. Any string value can be used as a key of the map.

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - afAppId

 - multiAccCtrls

 oneOf:

 - required: [interGroupId]

 - required: [supi]

 ServiceParameterData:

 description: Represents the service parameter data.

 type: object

 properties:

 appId:

 type: string

 description: Identifies an application.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 ueIpv4:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 anyUeInd:

 type: boolean

 paramOverPc5:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverPc5'

 paramOverUu:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverUu'

 paramForProSeDd:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDd'

 paramForProSeDc:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDc'

 paramForProSeU2NRelUe:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2NRelUe'

 paramForProSeRemUe:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeRemUe'

 urspInfluence:

 type: array

 items:

 $ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/UrspRuleRequest'

 minItems: 1

 description: Contains the service parameter used to influence the URSP.

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 AmInfluData:

 description: Represents the AM Influence Data.

 type: object

 properties:

 appId:

 type: string

 description: Identifies an application.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ethTrafficFilters:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 anyUeInd:

 type: boolean

 description: Indicates whether the data is applicable for any UE.

 trafficFilters:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 evSubs:

 type: array

 items:

 type: object

 # The actual type definition will be included in TS 29.522

 # $ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

 minItems: 1

 thruReq:

 type: boolean

 description: Indicates whether high throughput is desired for the indicated UE traffic.

 covReq:

 type: string

 description: Indicates the service area coverage requirement.

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 allOf:

 - anyOf:

 - required: [thruReq]

 - required: [covReq]

 - oneOf:

 - required: [supi]

 - required: [interGroupId]

 - required: [anyUeInd]

 AmInfluDataPatch:

 description: Represents the AM Influence Data that can be updated.

 type: object

 properties:

 appId:

 type: string

 description: Identifies an application.

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ethTrafficFilters:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 interGroupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 anyUeInd:

 type: boolean

 description: Indicates whether the data is applicable for any UE.

 trafficFilters:

 type: array

 items:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

 minItems: 1

 description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 evSubs:

 type: array

 items:

 type: object

 # The actual type definition will be included in TS 29.522

 # $ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

 minItems: 1

 thruReq:

 type: boolean

 description: Indicates whether high throughput is desired for the indicated UE traffic.

 covReq:

 type: string

 description: Indicates the service area coverage requirement.

 oneOf:

 - required: [supi]

 - required: [interGroupId]

 - required: [anyUeInd]

 ApplicationDataSubs:

 description: Identifies a subscription to application data change notification.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 dataFilters:

 type: array

 items:

 $ref: '#/components/schemas/DataFilter'

 minItems: 1

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - notificationUri

 ApplicationDataChangeNotif:

 description: Contains changed application data for which notification was requested.

 type: object

 properties:

 iptvConfigData:

 $ref: '#/components/schemas/IptvConfigData'

 pfdData:

 $ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdChangeNotification'

 bdtPolicyData:

 $ref: '#/components/schemas/BdtPolicyData'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 serParamData:

 $ref: '#/components/schemas/ServiceParameterData'

 amInfluData:

 $ref: '#/components/schemas/AmInfluData'

 required:

 - resUri

 DataFilter:

 description: Identifies a data filter.

 type: object

 properties:

 dataInd:

 $ref: '#/components/schemas/DataInd'

 dnns:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 minItems: 1

 snssais:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 1

 internalGroupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 supis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 minItems: 1

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 ueIpv4s:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 ueIpv6s:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 ueMacs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 minItems: 1

 required:

 - dataInd

 DataInd:

 anyOf:

 - type: string

 enum:

 - PFD

 - IPTV

 - BDT

 - SVC\_PARAM

 - AM

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PFD

 - IPTV

 - BDT

 - SVC\_PARAM

 - AM

\* \* \* End of changes \* \* \* \*