**3GPP TSG-CT3 Meeting #118e C3-215277\_r2**

**E-Meeting, 11th – 15th October 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.519** | **CR** | **0283** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Updates to the 5G ProSe service parameters | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, CATT | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_ProSe | | | | |  | ***Date:*** | | | 2021-09-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Based on the progress of CT1 on 5G ProSe, the following aspects have been clarified/updated:   * CT1 has defined the encoding of the UE policies and configuration parameters for 5G ProSe UE-to-network relay in TS 29.555 and divided them into two separate parts:   + UE policies / Service parameters for 5G ProSe UE-to-network relay UE.   + UE policies / Service parameters for 5G ProSe remote UE. * In addition, CR C3-214312 agreed during last meeting omitted to remove the service parameters for 5G ProSe usage reporting configuration and rules and the service parameters for 5G ProSe service path selection from the OpenAPI file of the Nudr\_DataRepository API for Application Data. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This CR proposes to:   * In order to align with CT1, CR C3-215xxx defines separate attributes and data types for the two components of the UE policies / Service parameters for 5G ProSe UE-to-network relay, i.e. UE policies / Service parameters for 5G ProSe UE-to-network relay UE and UE policies / Service parameters for 5G ProSe remote UE. This CR proposes to align with it. * Remove the attributes and data types related to the service parameters for 5G ProSe usage reporting configuration and rules and the service parameters for 5G ProSe service path selection from the OpenAPI file of the Nudr\_DataRepository API for Application Data. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | * Misalignment with the Stage 3 work in CT1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.4.1, 6.4.2.15, A.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR introduces backwards compatible new features and corrections to the OpenAPI specification file of the Nudr\_DataRepository API for Application Data. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* Start of changes \* \* \* \*

### 6.4.1 General

This subclause specifies the application data model supported by the API.

Table 6.4.1-1 specifies the data types defined for the Nudr\_DataRepository Service API for Application Data service based interface protocol.

Table 6.4.1-1: Nudr\_DataRepository specific Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| AmInfluData | 6.4.2.16 | Contains AM influence data. |  |
| AmInfluDataPatch | 6.4.2.17 | Contains AM influence data that can be updated. |  |
| ApplicationDataSubs | 6.4.2.10 | Contains application data subscription data. |  |
| ApplicationDataChangeNotif | 6.4.2.11 | Contains the new or updated application data or removed indication. |  |
| BdtPolicyData | 6.4.2.7 | Contains applied BDT policy data. | EnhancedBackgroundDataTransfer |
| BdtPolicyDataPatch | 6.4.2.8 | Contains modification instructions to be performed on the applied BDT policy data. | EnhancedBackgroundDataTransfer |
| DataInd | 6.4.3.3 | Indicates the type of data. |  |
| DataFilter | 6.4.2.12 | Indicates a data filter. |  |
| IptvConfigData | 6.4.2.9 | Represents IPTV configuration data information. |  |
| PfdDataForAppExt | 6.4.2.6 | The PFDs and related data for the application |  |
| ServiceParameterData | 6.4.2.15 | Contains the service parameter data. |  |
| TrafficInfluData | 6.4.2.2 | Contains traffic influence data. |  |
| TrafficInfluDataPatch | 6.4.2.3 | Contains modification instructions to be performed on the traffic influence data. |  |
| TrafficInfluDataNotif | 6.4.2.14 | Contains traffic influence data for notification. | EnhancedInfluDataNotification |
| TrafficInfluSub | 6.4.2.4 | Contains traffic influence subscription data. |  |

Table 6.4.1-2 specifies data types re-used by the Nudr\_DataRepository Service API for Application Data service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nudr\_DataRepository Service API for Application Data service based interface.

Table 6.4.1-2: Nudr\_DataRepository re-used Data Types for Application Data

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AmInfluEvent | 3GPP TS 29.522 [19] | Identifies the type of AM related events of which the AF requests to be notified. |  |
| ApplicationId | 3GPP TS 29.571 [7] | Indicates an application identifier. |  |
| BdtReferenceId | 3GPP TS 29.122 [9] | Identifies a selected policy of background data transfer. | EnhancedBackgroundDataTransfer |
| DateTime | 3GPP TS 29.571 [7] | Indicates a date and time. |  |
| DnaiChangeType | 3GPP TS 29.571 [7] | Describes the types of DNAI change. |  |
| Dnn | 3GPP TS 29.571 [7] | Identifies a Data Network Name. |  |
| EthFlowDescription | 3GPP TS 29.514 [16] | Contains the Ethernet data flow information.(NOTE) |  |
| FlowInfo | 3GPP TS 29.122 [9] | Contains the flow information. |  |
| IptvConfigDataPatch | 3GPP TS 29.522 [19] | Contains the IPTV configuration data used for PATCH. |  |
| Ipv4Addr | 3GPP TS 29.571 [7] | Identifies an IPv4 address. |  |
| Ipv6Addr | 3GPP TS 29.571 [7] | Identifies an IPv6 address. |  |
| MacAddr48 | 3GPP TS 29.571 [7] | MAC Address. |  |
| MulticastAccessControl | 3GPP TS 29.522 [19] | Represents the multicast access control information. |  |
| NetworkAreaInfo | 3GPP TS 29.554 [13] | Describes a network area information. |  |
| ParameterOverPc5 | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over PC5. |  |
| ParameterOverUu | 3GPP TS 29.522 [19] | Contains the V2X service parameters data provisioned over Uu. |  |
| ParamForProSeDd | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| ParamForProSeDc | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| ParamForProSeU2NRelUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| ParamForProSeRemUe | 3GPP TS 29.522 [19] | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| PfdChangeNotification | 3GPP TS 29.551 [8] | Describes the PFD change. |  |
| PfdDataForApp | 3GPP TS 29.551 [8] | Identifies the PFDs for one application identifier. |  |
| RouteToLocation | 3GPP TS 29.571 [7] | Identifies the N6 traffic routing requirement. |  |
| ServiceParamterDataPatch | 3GPP TS 29.522 [19] | Contains the service parameter data. |  |
| Snssai | 3GPP TS 29.571 [7] | Identifies a Single Network Slice Selection Assistance Information. |  |
| SubscribedEvent | 3GPP TS 29.522 [19] | Identified the type of UP path management events of which the AF requests to be notified. |  |
| Supi | 3GPP TS 29.571 [7] | Identifies a SUPI that shall contain either an IMSI or an NAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [7] | Used to negotiate the applicability of the optional features. |  |
| TemporalValidity | 3GPP TS 29.514 [16] | Indicates the time interval during which the AF request is to be applied. | MultiTemporalCondition |
| Uri | 3GPP TS 29.571 [7] | Identifies a URI. |  |
| UrspRuleRequest | 3GPP TS 29.522 [19] | Contains service parameter data used to influence the URSP. | EnEDGE |
| UserPlaneLatencyRequirements | 3GPP TS 29.512 [12] | User Plane Latency Requirements. | EnEDGE |
| NOTE: In order to support a set of MAC addresses with a specific range in the traffic filter, feature MacAddressRange as specified in clause 6.1.8 of TS 29.504 [6] shall be supported. | | | |

\* \* \* Next changes \* \* \* \*

#### 6.4.2.15 Type ServiceParameterData

Table 6.4.2.15-1: Definition of type ServiceParameterData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| dnn | Dnn | O | 0..1 | Identifies a DNN. (NOTE 2) |  |
| snssai | Snssai | O | 0..1 | Identifies an S-NSSAI. (NOTE 2) |  |
| appId | string | O | 0..1 | Identifies an application identifier. (NOTE 2) |  |
| supi | Supi | O | 0..1 | Identifies a user. (NOTE1) |  |
| ueIpv4 | Ipv4Addr | O | 0..1 | The IPv4 address of the served UE. (NOTE1) |  |
| ueIpv6 | Ipv6Addr | O | 0..1 | The IPv6 address of the served UE. (NOTE1) |  |
| ueMac | MacAddr48 | O | 0..1 | The MAC address of the served UE. (NOTE1) |  |
| interGroupId | GroupId | O | 0..1 | Identifies a group of users. (NOTE1) |  |
| anyUeInd | boolean | O | 0..1 | Identifies whether the service parameters applies to any UE. This attribute shall set to "true" if applicable for any UE, otherwise, set to "false". (NOTE1) |  |
| paramOverPc5 | ParameterOverPc5 | O | 0..1 | Contains the V2X service parameters used over PC5 |  |
| paramOverUu | ParameterOverUu | O | 0..1 | Contains the V2X service parameters used over Uu |  |
| urspInfluence | array(UrspRuleRequest) | O | 1..N | Contains the service parameter used to influence the URSP. | EnEDGE |
| paramForProSeDd | ParamForProSeDd | O | 0..1 | Contains the service parameters for 5G ProSe direct discovery. | ProSe |
| paramForProSeDc | ParamForProSeDc | O | 0..1 | Contains the service parameters for 5G ProSe direct communications. | ProSe |
| paramForProSeU2NRelUe | ParamForProSeU2NRelUe | O | 0..1 | Contains the service parameters for 5G ProSe UE-to-network relay UE. | ProSe |
| paramForProSeRemUe | ParamForProSeRemUe | O | 0..1 | Contains the service parameters for 5G ProSe remote UE. | ProSe |
| suppFeat | SupportedFeatures | C | 0..1 | Indicates the list of Supported features used as described in subclause 5.8.  This parameter shall be supplied in the PUT request that requested the creation of an individual Service parameter resource, and in the PUT response. |  |
| resUri | Uri | C | 0..1 | Represents the URI of Individual Service Parameter Data. It shall only be included in the HTTP GET response. |  |
| NOTE 1: Only one of the "supi", "anyUeInd", "interGroupId", "ueIpv4", "ueIpv6" or "ueMac" attribute shall be provided.  NOTE 2: Only the combination of "dnn" and "snssai" or "appId" attribute shall be provided. | | | | | |

Editor's Note: It is FFS to consider if "urspInfluence" should be encoded exactly in the same way that URSP rules are encoded in NAS messages (see TS 24.526).

Editor's Note: It is FFS to consider if a separate UDR feature should be used for "urspInfluence" instead of the EnEDGE feature.

\* \* \* Next changes \* \* \* \*

# A.3 Nudr\_DataRepository API for Application Data

For the purpose of referencing entities in the Open API file defined in this Annex, it shall be assumed that this Open API file is contained in a physical file named "TS29519\_Application\_Data.yaml".

openapi: 3.0.0

info:

version: '-'

title: Unified Data Repository Service API file for Application Data

description: |

The API version is defined in 3GPP TS 29.504

© 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.519 V17.4.0; 5G System; Usage of the Unified Data Repository Service for Policy Data, Application Data and Structured Data for Exposure.

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.519/'

paths:

/application-data/pfds:

get:

summary: Retrieve PFDs for application identifier(s)

operationId: ReadPFDData

tags:

- PFD Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: appId

in: query

description: Contains the information of the application identifier(s) for the querying PFD Data resource. If none appId is included in the URI, it applies to all application identifier(s) for the querying PFD Data resource.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minItems: 1

responses:

'200':

description: A representation of PFDs for request applications is returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdDataForAppExt'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/pfds/{appId}:

get:

summary: Retrieve the corresponding PFDs of the specified application identifier

operationId: ReadIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: appId

in: path

description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

required: true

schema:

type: string

responses:

'200':

description: A representation of PFDs for the request application identified by the application identifier is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete the corresponding PFDs of the specified application identifier

operationId: DeleteIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: appId

in: path

description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

required: true

schema:

type: string

responses:

'204':

description: Successful case. The Individual PFD Data resource related to the application identifier was deleted.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Create or update the corresponding PFDs for the specified application identifier

operationId: CreateOrReplaceIndividualPFDData

tags:

- Individual PFD Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

parameters:

- name: appId

in: path

description: Indicate the application identifier for the request pfd(s). It shall apply the format of Data type ApplicationId.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual PFD Data resource related to the application-identifier is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/pfds/{appId}'

required: true

schema:

type: string

'200':

description: Successful case. The upgrade of an Individual PFD Data resource related to the application identifier is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdDataForAppExt'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData:

get:

summary: Retrieve Traffic Influence Data

operationId: ReadInfluenceData

tags:

- Influence Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: influence-Ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: internal-Group-Ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: supp-feat

in: query

required: false

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The Traffic Influence Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TrafficInfluData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/{influenceId}:

put:

summary: Create or update an individual Influence Data resource

operationId: CreateOrReplaceIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

parameters:

- name: influenceId

in: path

description: The Identifier of an Individual Influence Data to be created or updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual Traffic Influence Data resource is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/influenceData/{influenceId}'

required: true

schema:

type: string

'200':

description: The update of an Individual Traffic Influence Data resource is confirmed and a response body containing Traffic Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Influence Data resource

operationId: UpdateIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/TrafficInfluDataPatch'

parameters:

- name: influenceId

in: path

description: The Identifier of an Individual Influence Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual Traffic Influence Data resource is confirmed and a response body containing Traffic Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Influence Data resource

operationId: DeleteIndividualInfluenceData

tags:

- Individual Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: influenceId

in: path

description: The Identifier of an Individual Influence Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Influence Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/subs-to-notify:

post:

summary: Create a new Individual Influence Data Subscription resource

operationId: CreateIndividualInfluenceDataSubscription

tags:

- Influence Data Subscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

responses:

'201':

description: The subscription was created successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

trafficInfluenceDataChangeNotification:

'{$request.body#/notificationUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

oneOf:

- $ref: '#/components/schemas/TrafficInfluData'

- $ref: '#/components/schemas/TrafficInfluDataNotif'

minItems: 1

responses:

'204':

description: No Content, Notification was successful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Read Influence Data Subscriptions

operationId: ReadInfluenceDataSubscriptions

tags:

- Influence Data Subscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: dnn

in: query

description: Identifies a DNN.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

- name: snssai

in: query

description: Identifies a slice.

required: false

content:

application/json:

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

- name: internal-Group-Id

in: query

description: Identifies a group of users.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

- name: supi

in: query

description: Identifies a user.

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

responses:

'200':

description: The subscription information as request in the request URI query parameter(s) are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/TrafficInfluSub'

minItems: 0

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/influenceData/subs-to-notify/{subscriptionId}:

get:

summary: Get an existing individual Influence Data Subscription resource

operationId: ReadIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Individual Influence Data Subscription

required: true

schema:

type: string

responses:

'200':

description: The subscription information is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

put:

summary: Modify an existing individual Influence Data Subscription resource

operationId: ReplaceIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Individual Influence Data Subscription

required: true

schema:

type: string

responses:

'200':

description: The subscription was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/TrafficInfluSub'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Influence Data Subscription resource

operationId: DeleteIndividualInfluenceDataSubscription

tags:

- Individual Influence Data Subscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: subscriptionId

in: path

description: String identifying a subscription to the Individual Influence Data Subscription

required: true

schema:

type: string

responses:

'204':

description: The subscription was terminated successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/bdtPolicyData:

get:

summary: Retrieve applied BDT Policy Data

operationId: ReadBdtPolicyData

tags:

- BdtPolicy Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: bdt-policy-ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: internal-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

responses:

'200':

description: The applied BDT policy Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/BdtPolicyData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/bdtPolicyData/{bdtPolicyId}:

put:

summary: Create an individual applied BDT Policy Data resource

operationId: CreateIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

parameters:

- name: bdtPolicyId

in: path

description: The Identifier of an Individual Applied BDT Policy Data to be created or updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual Applied BDT Policy Data resource is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/bdtPolicyData/{bdtPolicyId}'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Applied BDT Policy Data resource

operationId: UpdateIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/BdtPolicyDataPatch'

parameters:

- name: bdtPolicyId

in: path

description: The Identifier of an Individual Applied BDT Policy Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual Applied BDT Policy Data resource is confirmed and a response body containing Applied BDT Policy Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/BdtPolicyData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Applied BDT Policy Data resource

operationId: DeleteIndividualAppliedBdtPolicyData

tags:

- Individual Applied BDT Policy Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: bdtPolicyId

in: path

description: The Identifier of an Individual Applied BDT Policy Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Applied BDT Policy Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/iptvConfigData:

get:

summary: Retrieve IPTV configuration Data

operationId: ReadIPTVCongifurationData

tags:

- IPTV Configuration Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: config-ids

in: query

description: Each element identifies a configuration.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: inter-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

responses:

'200':

description: The IPTV configuration data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/IptvConfigData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/iptvConfigData/{configurationId}:

put:

summary: Create or update an individual IPTV configuration resource

operationId: CreateOrReplaceIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

parameters:

- name: configurationId

in: path

description: The Identifier of an Individual IPTV Configuration Data to be created or updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual IPTV Configuration Data resource is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: The update of an Individual IPTV configuration resource.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Partial update an individual IPTV configuration resource

operationId: PartialReplaceIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/IptvConfigDataPatch'

parameters:

- name: configurationId

in: path

description: The Identifier of an Individual IPTV Configuration Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual IPTV configuration resource.

content:

application/json:

schema:

$ref: '#/components/schemas/IptvConfigData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual IPTV configuration resource

operationId: DeleteIndividualIPTVConfigurationData

tags:

- Individual IPTV Configuration Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: configurationId

in: path

description: The Identifier of an Individual IPTV Configuration to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The resource was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/serviceParamData:

get:

summary: Retrieve Service Parameter Data

operationId: ReadServiceParameterData

tags:

- Service Parameter Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: service-param-ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: internal-group-ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: ue-ipv4s

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

- name: ue-ipv6s

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

- name: ue-macs

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

- name: supp-feat

in: query

description: Supported Features

required: false

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The Service Parameter Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ServiceParameterData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/serviceParamData/{serviceParamId}:

put:

summary: Create or update an individual Service Parameter Data resource

operationId: CreateOrReplaceServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

parameters:

- name: serviceParamId

in: path

description: The Identifier of an Individual Service Parameter Data to be created or updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual Service Parameter Data resource is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/serviceParamData/{serviceParamId}'

required: true

schema:

type: string

'200':

description: The update of an Individual Service Parameter Data resource is confirmed and a response body containing Service Parameter Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual Service Parameter Data resource

operationId: UpdateIndividualServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ServiceParameterDataPatch'

parameters:

- name: serviceParamId

in: path

description: The Identifier of an Individual Service Parameter Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual Service Parameter Data resource is confirmed and a response body containing Service Parameter Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ServiceParameterData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual Service Parameter Data resource

operationId: DeleteIndividualServiceParameterData

tags:

- Individual Service Parameter Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: serviceParamId

in: path

description: The Identifier of an Individual Service Parameter Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual Service Parameter Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/am-influence-data:

get:

summary: Retrieve AM Influence Data

operationId: ReadAmInfluenceData

tags:

- AM Influence Data (Store)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: am-Influence-Ids

in: query

description: Each element identifies a service.

required: false

schema:

type: array

items:

type: string

minItems: 1

- name: dnns

in: query

description: Each element identifies a DNN.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

- name: snssais

in: query

description: Each element identifies a slice.

required: false

content:

application/json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

- name: internal-Group-Ids

in: query

description: Each element identifies a group of users.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

- name: supis

in: query

description: Each element identifies the user.

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

- name: supp-feat

in: query

required: false

description: Supported Features

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

responses:

'200':

description: The AM Influence Data stored in the UDR are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AmInfluData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/am-influence-data/{amInfluenceId}:

put:

summary: Create or update an individual AM Influence Data resource

operationId: CreateOrReplaceIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

parameters:

- name: amInfluenceId

in: path

description: The Identifier of an Individual AM Influence Data to be created or updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'201':

description: The creation of an Individual AM Influence Data resource is confirmed and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

headers:

Location:

description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nudr-dr/<apiVersion>/application-data/am-influence-data/{amInfluenceId}'

required: true

schema:

type: string

'200':

description: The update of an Individual AM Influence Data resource is confirmed and a response body containing AM Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify part of the properties of an individual AM Influence Data resource

operationId: UpdateIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AmInfluDataPatch'

parameters:

- name: amInfluenceId

in: path

description: The Identifier of an Individual AM Influence Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'200':

description: The update of an Individual AM Influence Data resource is confirmed and a response body containing AM Influence Data shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/AmInfluData'

'204':

description: No content

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an individual AM Influence Data resource

operationId: DeleteIndividualAmInfluenceData

tags:

- Individual AM Influence Data (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: amInfluenceId

in: path

description: The Identifier of an Individual AM Influence Data to be updated. It shall apply the format of Data type string.

required: true

schema:

type: string

responses:

'204':

description: The Individual AM Influence Data was deleted successfully.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/subs-to-notify:

post:

summary: Create a subscription to receive notification of application data changes

operationId: CreateIndividualApplicationDataSubscription

tags:

- ApplicationDataSubscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

responses:

'201':

description: Upon success, a response body containing a representation of each Individual subscription resource shall be returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

applicationDataChangeNotif:

'{$request.body#/notificationUri}':

post:

requestBody:

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ApplicationDataChangeNotif'

minItems: 1

responses:

'204':

description: No Content, Notification was successful

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Read Application Data change Subscriptions

operationId: ReadApplicationDataChangeSubscriptions

tags:

- ApplicationDataSubscriptions (Collection)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: data-filter

in: query

description: The data filter for the query.

required: false

schema:

$ref: '#/components/schemas/DataFilter'

responses:

'200':

description: The subscription information as request in the request URI query parameter(s) are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ApplicationDataSubs'

minItems: 0

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/application-data/subs-to-notify/{subsId}:

parameters:

- name: subsId

in: path

required: true

schema:

type: string

put:

summary: Modify a subscription to receive notification of application data changes

operationId: ReplaceIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

responses:

'200':

description: The individual subscription resource was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

'204':

description: The individual subscription resource was updated successfully and no additional content is to be sent in the response message.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete the individual Application Data subscription

operationId: DeleteIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

responses:

'204':

description: Upon success, an empty response body shall be returned.

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

get:

summary: Get an existing individual Application Data Subscription resource

operationId: ReadIndividualApplicationDataSubscription

tags:

- IndividualApplicationDataSubscription (Document)

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

- oAuth2ClientCredentials:

- nudr-dr

- nudr-dr:application-data

parameters:

- name: subsId

in: path

description: String identifying a subscription to the Individual Application Data Subscription

required: true

schema:

type: string

responses:

'200':

description: The subscription information is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/ApplicationDataSubs'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'414':

$ref: 'TS29571\_CommonData.yaml#/components/responses/414'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

schemas:

TrafficInfluData:

description: Represents the Traffic Influence Data.

type: object

properties:

upPathChgNotifCorreId:

type: string

description: Contains the Notification Correlation Id allocated by the NEF for the UP path change notification.

appReloInd:

type: boolean

description: Identifies whether an application can be relocated once a location of the application has been selected.

afAppId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

trafficRoutes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: Identifies the N6 traffic routing requirement.

traffCorreInd:

type: boolean

validStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

validEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

tempValidities:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

minItems: 1

description: Identifies the temporal validities for the N6 traffic routing requirement.

nwAreaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

upPathChgNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

type: array

items:

type: string

minItems: 1

subscribedEvents:

type: array

items:

$ref: 'TS29522\_TrafficInfluence.yaml#/components/schemas/SubscribedEvent'

minItems: 1

dnaiChgType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

afAckInd:

type: boolean

addrPreserInd:

type: boolean

upLatReq:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UserPlaneLatencyRequirements'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

allOf:

- oneOf:

- required: [afAppId]

- required: [trafficFilters]

- required: [ethTrafficFilters]

- oneOf:

- required: [supi]

- required: [interGroupId]

TrafficInfluDataPatch:

description: Represents the Traffic Influence Data to be updated in the UDR.

type: object

properties:

upPathChgNotifCorreId:

type: string

description: Contains the Notification Correlation Id allocated by the NEF for the UP path change notification.

appReloInd:

type: boolean

description: Identifies whether an application can be relocated once a location of the application has been selected.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

internalGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

trafficRoutes:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

minItems: 1

description: Identifies the N6 traffic routing requirement.

traffCorreInd:

type: boolean

validStartTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

validEndTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

tempValidities:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TemporalValidity'

minItems: 1

nullable: true

description: Identifies the temporal validities for the N6 traffic routing requirement.

nwAreaInfo:

$ref: 'TS29554\_Npcf\_BDTPolicyControl.yaml#/components/schemas/NetworkAreaInfo'

upPathChgNotifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

headers:

type: array

items:

type: string

minItems: 1

afAckInd:

type: boolean

addrPreserInd:

type: boolean

upLatReq:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UserPlaneLatencyRequirements'

TrafficInfluSub:

description: Represents traffic influence subscription data.

type: object

properties:

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

description: Each element identifies a DNN.

snssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

description: Each element identifies a slice.

internalGroupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

description: Each element identifies a group of users.

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

description: Each element identifies the user.

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- notificationUri

oneOf:

- required: [dnns]

- required: [snssais]

- required: [internalGroupIds]

- required: [supis]

TrafficInfluDataNotif:

description: Represents traffic influence data for notification.

type: object

properties:

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

trafficInfluData:

$ref: '#/components/schemas/TrafficInfluData'

required:

- resUri

PfdDataForAppExt:

description: Represents the PFDs and related data for the application.

allOf:

- $ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdDataForApp'

- type: object

properties:

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

BdtPolicyData:

description: Represents applied BDT policy data.

type: object

properties:

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

required:

- bdtRefId

BdtPolicyDataPatch:

description: Represents modification instructions to be performed on the applied BDT policy data.

type: object

properties:

bdtRefId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

required:

- bdtRefId

IptvConfigData:

description: Represents IPTV configuration data information.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

interGroupId:

description: Identifies a group of users.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

afAppId:

type: string

multiAccCtrls:

type: object

additionalProperties:

$ref: 'TS29522\_IPTVConfiguration.yaml#/components/schemas/MulticastAccessControl'

minProperties: 1

description: Identifies a list of multicast address access control information. Any string value can be used as a key of the map.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

required:

- afAppId

- multiAccCtrls

oneOf:

- required: [interGroupId]

- required: [supi]

ServiceParameterData:

description: Represents the service parameter data.

type: object

properties:

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

ueIpv4:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ueIpv6:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

ueMac:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

anyUeInd:

type: boolean

paramOverPc5:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverPc5'

paramOverUu:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParameterOverUu'

paramForProSeDd:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDd'

paramForProSeDc:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeDc'

paramForProSeU2NRelUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeU2NRelUe'

paramForProSeRemUe:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/ParamForProSeRemUe'

urspInfluence:

type: array

items:

$ref: 'TS29522\_ServiceParameter.yaml#/components/schemas/UrspRuleRequest'

minItems: 1

description: Contains the service parameter used to influence the URSP.

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

AmInfluData:

description: Represents the AM Influence Data.

type: object

properties:

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

anyUeInd:

type: boolean

description: Indicates whether the data is applicable for any UE.

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

evSubs:

type: array

items:

type: object

# The actual type definition will be included in TS 29.522

# $ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

minItems: 1

thruReq:

type: boolean

description: Indicates whether high throughput is desired for the indicated UE traffic.

covReq:

type: string

description: Indicates the service area coverage requirement.

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

allOf:

- anyOf:

- required: [thruReq]

- required: [covReq]

- oneOf:

- required: [supi]

- required: [interGroupId]

- required: [anyUeInd]

AmInfluDataPatch:

description: Represents the AM Influence Data that can be updated.

type: object

properties:

appId:

type: string

description: Identifies an application.

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

ethTrafficFilters:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

interGroupId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

anyUeInd:

type: boolean

description: Indicates whether the data is applicable for any UE.

trafficFilters:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Identifies IP packet filters. Either "trafficFilters" or "ethTrafficFilters" shall be included if applicable.

startTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

endTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

evSubs:

type: array

items:

type: object

# The actual type definition will be included in TS 29.522

# $ref: 'TS29522\_AMInfluence.yaml#/components/schemas/AmInfluEvent'

minItems: 1

thruReq:

type: boolean

description: Indicates whether high throughput is desired for the indicated UE traffic.

covReq:

type: string

description: Indicates the service area coverage requirement.

oneOf:

- required: [supi]

- required: [interGroupId]

- required: [anyUeInd]

ApplicationDataSubs:

description: Identifies a subscription to application data change notification.

type: object

properties:

notificationUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

dataFilters:

type: array

items:

$ref: '#/components/schemas/DataFilter'

minItems: 1

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- notificationUri

ApplicationDataChangeNotif:

description: Contains changed application data for which notification was requested.

type: object

properties:

iptvConfigData:

$ref: '#/components/schemas/IptvConfigData'

pfdData:

$ref: 'TS29551\_Nnef\_PFDmanagement.yaml#/components/schemas/PfdChangeNotification'

bdtPolicyData:

$ref: '#/components/schemas/BdtPolicyData'

resUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

serParamData:

$ref: '#/components/schemas/ServiceParameterData'

amInfluData:

$ref: '#/components/schemas/AmInfluData'

required:

- resUri

DataFilter:

description: Identifies a data filter.

type: object

properties:

dataInd:

$ref: '#/components/schemas/DataInd'

dnns:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

minItems: 1

snssais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

minItems: 1

internalGroupIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

minItems: 1

supis:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

minItems: 1

appIds:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

minItems: 1

ueIpv4s:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

minItems: 1

ueIpv6s:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

ueMacs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

required:

- dataInd

DataInd:

anyOf:

- type: string

enum:

- PFD

- IPTV

- BDT

- SVC\_PARAM

- AM

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- PFD

- IPTV

- BDT

- SVC\_PARAM

- AM

\* \* \* End of changes \* \* \* \*