**3GPP TSG-CT3 Meeting #120e C3-221660**

**E-Meeting, 17th – 25th February 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **29.122** | **CR** | **0573** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update of info and externalDocs fields | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | CT3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | TEI17 | | | | |  | ***Date:*** | | | 2022-02-24 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | During this plenary cycle (2022-Q1), there have been some backwards compatible changes / corrections / addition of new features to the following T8 APIs defined in TS 29.122.  The following agreed CRs update the OpenAPI file of the **CommonData API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file for **MonitoringEvent API** for the present release:   * TS 29.122 CR#0554 introduces a backwards compatible feature * TS 29.122 CR#0555 introduces a backwards compatible feature * TS 29.122 CR#0557 introduces backwards compatible corrections * TS 29.122 CR#0560 introduces backwards compatible corrections * TS 29.122 CR#0561 introduces a backwards compatible feature * TS 29.122 CR#0568 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**4** to 1.2.0-alpha.**5**  The following agreed CRs update theOpenAPI file for **ResourceManagementOfBdt API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**2**  The following agreed CRs update theOpenAPI file of the **ChargeableParty API** for the present release:   * TS 29.122 CR#0557 introduces backwards compatible corrections * TS 29.122 CR#0560 introduces backwards compatible corrections   The API version need to be updated from 1.2.0-alpha.**5** to 1.2.0-alpha.**6**  The following agreed CRs update theOpenAPI file of the **NIDD API** for the present release:   * TS 29.122 CR#0547 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**4** to 1.2.0-alpha.**5**  The following agreed CRs update theOpenAPI file of the **DeviceTriggering API** for the present release:   * TS 29.122 CR#0548 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file for **GMDviaMBMSbyMB2 API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**3**  The following agreed CRs update theOpenAPI file of the **GMDviaMBMSbyxMB API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**3**  The following agreed CRs update theOpenAPI file of the **ReportingNetworkStatus API** for the present release:   * TS 29.122 CR#0572 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file of the **CpProvisioning API** for the present release:   * TS 29.122 CR#0569 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file of the **PfdManagement API** for the present release:   * TS 29.122 CR#0558 introduces a backwards compatible feature * TS 29.122 CR#0571 introduces a backwards compatible feature * TS 29.551 CR#0102 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update the OpenAPI file of the **ECRControl API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**1**  The following agreed CRs update theOpenAPI file of the **NpConfiguration API** for the present release:   * TS 29.122 CR#0570 introduces a backwards compatible feature   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file of the **AsSessionWithQoS API** for the present release:   * TS 29.122 CR#0557 introduces backwards compatible corrections * TS 29.122 CR#0559 introduces a backwards compatible feature * TS 29.122 CR#0560 introduces backwards compatible corrections   The API version need to be updated from 1.2.0-alpha.**3** to 1.2.0-alpha.**4**  The following agreed CRs update theOpenAPI file of the **MsisdnLessMoSms API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.2.0-alpha.**2**  The following agreed CRs update theOpenAPI file of the **RacsParameterProvisioning API** for the present release:   * None.   The API version hence does not need to be updated and remains 1.1.0-alpha.**4**  As these APIs are under pre-release development, the pre-release version number (“alpha.n”) of the APIs need to be incremented as per the provisions of clause 4.3.1.2 of 3GPP TS 29.501. The "externalDocs" object description field should also be updated to "v17.**5**.0" for these APIs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The CR proposes the following changes:   * Increment the pre-release version number from "…-alpha.**n**" to "…-alpha.**n+1**" for the above listed APIs. * Update the TS version number in "externalDocs" object description field to “v17.**5**.0” | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | OpenAPI version and the "externalDocs" object description field are not updated in the OpenAPI files impacted by the agreed CRs during Q1-2022 plenary cycle in CT3. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | A.3, A.5, A.6, A.7, A.9, A.10, A.11, A.13, A.14 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\* \* \* Start of changes \* \* \* \*

## A.3 MonitoringEvent API

openapi: 3.0.0

info:

title: 3gpp-monitoring-event

version: 1.2.0-alpha.5

description: |

API for Monitoring Event.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-monitoring-event/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: Read all of the active subscriptions for the SCS/AS.

operationId: FetchAllMonitoringEventSubscriptions

tags:

- Monitoring Event Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: The IPv4 address domain identifier. The attribute may only be provided if IPv4 address is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK (Successful get all of the active subscriptions for the SCS/AS)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventSubscription'

minItems: 0

description: Monitoring event subscriptions

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource for monitoring event notification.

operationId: CreateMonitoringEventSubscription

tags:

- Monitoring Event Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Subscription for notification about monitoring event

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'200':

description: The operation is successful and immediate report is included.

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/MonitoringEventReport'

- $ref: '#/components/schemas/MonitoringEventReports'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: Read an active subscriptions for the SCS/AS and the subscription Id.

operationId: FetchIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource.

operationId: UpdateIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/MonitoringEventSubscription'

'204':

description: No Content (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Modifies an existing subscription of monitoring event.

operationId: ModifyIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource.

required: true

schema:

type: string

requestBody:

description: This is used for PATCH request for partial cancellation of certain UE(s) within an active group.

required: true

content:

application/json-patch+json:

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchItem'

minItems: 1

responses:

'204':

description: The resource was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing monitoring event subscription.

operationId: DeleteIndMonitoringEventSubscription

tags:

- Individual Monitoring Event Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: The subscription was terminated successfully, the monitoring event report(s) shall be included if received.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

MonitoringEventSubscription:

description: Represents a subscription to event(s) monitoring.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

excludedExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Indicates cancellation of the external Identifier(s) within the active group.

excludedMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Indicates cancellation of the MSISDN(s) within the active group.

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

addExtGroupId:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

minItems: 2

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

maximumNumberOfReports:

type: integer

minimum: 1

description: Identifies the maximum number of event reports to be generated by the HSS, MME/SGSN as specified in subclause 5.6.0 of 3GPP TS 23.682.

monitorExpireTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

repPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

groupReportGuardTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: If "monitoringType" is "UE\_REACHABILITY", this parameter may be included to identify the number of packets that the serving gateway shall buffer in case that the UE is not reachable.

idleStatusIndication:

type: boolean

description: If "monitoringType" is set to "UE\_REACHABILITY" or "AVAILABILITY\_AFTER\_DDN\_FAILURE", this parameter may be included to indicate the notification of when a UE, for which PSM is enabled, transitions into idle mode. "true" indicates enabling of notification; "false" indicate no need to notify. Default value is "false".

locationType:

$ref: '#/components/schemas/LocationType'

accuracy:

$ref: '#/components/schemas/Accuracy'

minimumReportInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maxRptExpireIntvl:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

samplingInterval:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

reportingLocEstInd:

type: boolean

description: Indicates whether to request the location estimate for event reporting.

linearDistance:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LinearDistance'

locQoS:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LocationQoS'

svcId:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/ServiceIdentity'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

velocityRequested:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityRequested'

maxAgeOfLocEst:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AgeOfLocationEstimate'

locTimeWindow:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

supportedGADShapes:

type: array

items:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/SupportedGADShapes'

codeWord:

$ref: 'TS29515\_Ngmlc\_Location.yaml#/components/schemas/CodeWord'

associationType:

$ref: '#/components/schemas/AssociationType'

plmnIndication:

type: boolean

description: If "monitoringType" is "ROAMING\_STATUS", this parameter may be included to indicate the notification of UE's Serving PLMN ID. Value "true" indicates enabling of notification; "false" indicates disabling of notification. Default value is "false".

locationArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

locationArea5G:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

dddTraDescriptors:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

minItems: 1

dddStati:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

minItems: 1

apiNames:

type: array

items:

type: string

minItems: 1

monitoringEventReport:

$ref: '#/components/schemas/MonitoringEventReport'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

tgtNsThreshold:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SACInfo'

immediateRep:

type: boolean

uavPolicy:

$ref: '#/components/schemas/UavPolicy'

sesEstInd:

type: boolean

description: Set to true by the SCS/AS so that only UAV’s with “PDU session established for DNN(s) subject to aerial service” are to be listed in the Event report. Set to false or omitted otherwise.

subType:

$ref: '#/components/schemas/SubType'

addnMonTypes:

type: array

items:

$ref: '#/components/schemas/MonitoringType'

addnMonEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

required:

- notificationDestination

- monitoringType

anyOf:

- required: [maximumNumberOfReports]

- required: [monitorExpireTime]

MonitoringNotification:

description: Represents an event monitoring notification.

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

configResults:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

minItems: 1

description: Each element identifies a notification of grouping configuration result.

monitoringEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

description: Monitoring event reports.

cancelInd:

type: boolean

description: Indicates whether to request to cancel the corresponding monitoring subscription. Set to false or omitted otherwise.

cancelExternalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Identifies the cancelled external Identifier(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data.

cancelMsisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Identifies the cancelled MSISDN(s) within the active group via the "externalGroupId" attribute within the MonitoringEventSubscription data.

appliedParam:

$ref: '#/components/schemas/AppliedParameterConfiguration'

required:

- subscription

MonitoringEventReport:

description: Represents an event monitoring report.

type: object

properties:

imeiChange:

$ref: '#/components/schemas/AssociationType'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

idleStatusInfo:

$ref: '#/components/schemas/IdleStatusInfo'

locationInfo:

$ref: '#/components/schemas/LocationInfo'

locFailureCause:

$ref: '#/components/schemas/LocationFailureCause'

lossOfConnectReason:

type: integer

description: If "monitoringType" is "LOSS\_OF\_CONNECTIVITY", this parameter shall be included if available to identify the reason why loss of connectivity is reported. Refer to 3GPP TS 29.336 subclause 8.4.58.

maxUEAvailabilityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

monitoringType:

$ref: '#/components/schemas/MonitoringType'

uePerLocationReport:

$ref: '#/components/schemas/UePerLocationReport'

plmnId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/PlmnId'

reachabilityType:

$ref: '#/components/schemas/ReachabilityType'

roamingStatus:

type: boolean

description: If "monitoringType" is "ROAMING\_STATUS", this parameter shall be set to "true" if the UE is on roaming status. Set to false or omitted otherwise.

failureCause:

$ref: '#/components/schemas/FailureCause'

eventTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

pdnConnInfoList:

type: array

items:

$ref: '#/components/schemas/PdnConnectionInformation'

minItems: 1

dddStatus:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

dddTrafDescriptor:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

maxWaitTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

apiCaps:

type: array

items:

$ref: '#/components/schemas/ApiCapabilityInfo'

minItems: 0

nSStatusInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SACEventStatus'

servLevelDevId:

type: string

description: If "monitoringType" is "AREA\_OF\_INTEREST", this parameter may be included to identify the UAV.

uavPresInd:

type: boolean

description: If "monitoringType" is "AREA\_OF\_INTEREST", this parameter shall be set to true if the specified UAV is in the monitoring area. Set to false or omitted otherwise.

required:

- monitoringType

MonitoringEventReports:

description: Represents a set of event monitoring reports.

type: object

properties:

monitoringEventReports:

type: array

items:

$ref: '#/components/schemas/MonitoringEventReport'

minItems: 1

required:

- monitoringEventReports

IdleStatusInfo:

description: Represents the information relevant to when the UE transitions into idle mode.

type: object

properties:

activeTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

edrxCycleLength:

format: float

type: number

minimum: 0

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: Identifies the number of packets shall be buffered in the serving gateway. It shall be present if the idle status indication is requested by the SCS/AS with "idleStatusIndication" in the "monitoringEventSubscription" sets to "true".

idleStatusTimestamp:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

periodicAUTimer:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

UePerLocationReport:

description: Represents the number of UEs found at the indicated location.

type: object

properties:

ueCount:

type: integer

minimum: 0

description: Identifies the number of UEs.

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

servLevelDevIds:

type: array

items:

type: string

minItems: 1

description: Each element uniquely identifies a UAV.

required:

- ueCount

LocationInfo:

description: Represents the user location information.

type: object

properties:

ageOfLocationInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationMin'

cellId:

type: string

description: Indicates the Cell Global Identification of the user which identifies the cell the UE is registered.

enodeBId:

type: string

description: Indicates the eNodeB in which the UE is currently located.

routingAreaId:

type: string

description: Identifies the Routing Area Identity of the user where the UE is located.

trackingAreaId:

type: string

description: Identifies the Tracking Area Identity of the user where the UE is located.

plmnId:

type: string

description: Identifies the PLMN Identity of the user where the UE is located.

twanId:

type: string

description: Identifies the TWAN Identity of the user where the UE is located.

geographicArea:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/GeographicArea'

civicAddress:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/CivicAddress'

positionMethod:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/PositioningMethod'

qosFulfilInd:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/AccuracyFulfilmentIndicator'

ueVelocity:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/VelocityEstimate'

ldrType:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/LdrType'

achievedQos:

$ref: 'TS29572\_Nlmf\_Location.yaml#/components/schemas/MinorLocationQoS'

FailureCause:

description: Represents the reason of communication failure.

type: object

properties:

bssgpCause:

type: integer

description: Identifies a non-transparent copy of the BSSGP cause code. Refer to 3GPP TS 29.128.

causeType:

type: integer

description: Identify the type of the S1AP-Cause. Refer to 3GPP TS 29.128.

gmmCause:

type: integer

description: Identifies a non-transparent copy of the GMM cause code. Refer to 3GPP TS 29.128.

ranapCause:

type: integer

description: Identifies a non-transparent copy of the RANAP cause code. Refer to 3GPP TS 29.128.

ranNasCause:

type: string

description: Indicates RAN and/or NAS release cause code information, TWAN release cause code information or untrusted WLAN release cause code information. Refer to 3GPP TS 29.214.

s1ApCause:

type: integer

description: Identifies a non-transparent copy of the S1AP cause code. Refer to 3GPP TS 29.128.

smCause:

type: integer

description: Identifies a non-transparent copy of the SM cause code. Refer to 3GPP TS 29.128.

PdnConnectionInformation:

description: Represents the PDN connection information of the UE.

type: object

properties:

status:

$ref: '#/components/schemas/PdnConnectionStatus'

apn:

type: string

description: Identify the APN, it is depending on the SCEF local configuration whether or not this attribute is sent to the SCS/AS.

pdnType:

$ref: '#/components/schemas/PdnType'

interfaceInd:

$ref: '#/components/schemas/InterfaceIndication'

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipv6Addrs:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

minItems: 1

macAddrs:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

required:

- status

- pdnType

AppliedParameterConfiguration:

description: Represents the parameter configuration applied in the network.

type: object

properties:

externalIds:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

minItems: 1

description: Each element uniquely identifies a user.

msisdns:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

minItems: 1

description: Each element identifies the MS internal PSTN/ISDN number allocated for a UE.

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumDetectionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

ApiCapabilityInfo:

description: Represents the availability information of supported API.

type: object

properties:

apiName:

type: string

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- apiName

- suppFeat

UavPolicy:

description: Represents the policy information included in the UAV presence monitoring request.

type: object

properties:

uavMoveInd:

type: boolean

revokeInd:

type: boolean

required:

- uavMoveInd

- revokeInd

#

# ENUMS

#

MonitoringType:

anyOf:

- type: string

enum:

- LOSS\_OF\_CONNECTIVITY

- UE\_REACHABILITY

- LOCATION\_REPORTING

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION

- ROAMING\_STATUS

- COMMUNICATION\_FAILURE

- AVAILABILITY\_AFTER\_DDN\_FAILURE

- NUMBER\_OF\_UES\_IN\_AN\_AREA

- PDN\_CONNECTIVITY\_STATUS

- DOWNLINK\_DATA\_DELIVERY\_STATUS

- API\_SUPPORT\_CAPABILITY

- NUM\_OF\_REGD\_UES

- NUM\_OF\_ESTD\_PDU\_SESSIONS

- AREA\_OF\_INTEREST

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- LOSS\_OF\_CONNECTIVITY: The SCS/AS requests to be notified when the 3GPP network detects that the UE is no longer reachable for signalling or user plane communication

- UE\_REACHABILITY: The SCS/AS requests to be notified when the UE becomes reachable for sending either SMS or downlink data to the UE

- LOCATION\_REPORTING: The SCS/AS requests to be notified of the current location or the last known location of the UE

- CHANGE\_OF\_IMSI\_IMEI\_ASSOCIATION: The SCS/AS requests to be notified when the association of an ME (IMEI(SV)) that uses a specific subscription (IMSI) is changed

- ROAMING\_STATUS: The SCS/AS queries the UE's current roaming status and requests to get notified when the status changes

- COMMUNICATION\_FAILURE: The SCS/AS requests to be notified of communication failure events

- AVAILABILITY\_AFTER\_DDN\_FAILURE: The SCS/AS requests to be notified when the UE has become available after a DDN failure

- NUMBER\_OF\_UES\_IN\_AN\_AREA: The SCS/AS requests to be notified the number of UEs in a given geographic area

- PDN\_CONNECTIVITY\_STATUS: The SCS/AS requests to be notified when the 3GPP network detects that the UE’s PDN connection is set up or torn down

- DOWNLINK\_DATA\_DELIVERY\_STATUS: The AF requests to be notified when the 3GPP network detects that the downlink data delivery status is changed.

- API\_SUPPORT\_CAPABILITY: The SCS/AS requests to be notified of the availability of support of service APIs.

- NUM\_OF\_REGD\_UES: The AF requests to be notified of the current number of registered UEs for a network slice.

- NUM\_OF\_ESTD\_PDU\_SESSIONS: The AF requests to be notified of the current number of established PDU Sessions for a network slice.

- AREA\_OF\_INTEREST: The SCS/AS requests to be notified when the UAV moves in or out of the geographic area.

ReachabilityType:

anyOf:

- type: string

enum:

- SMS

- DATA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SMS : The SCS/AS requests to be notified when the UE becomes reachable for sending SMS to the UE

- DATA: The SCS/AS requests to be notified when the UE becomes reachable for sending downlink data to the UE

LocationType:

anyOf:

- type: string

enum:

- CURRENT\_LOCATION

- LAST\_KNOWN\_LOCATION

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION

- INITIAL\_LOCATION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CURRENT\_LOCATION: The SCS/AS requests to be notified for current location

- LAST\_KNOWN\_LOCATION: The SCS/AS requests to be notified for last known location

- CURRENT\_OR\_LAST\_KNOWN\_LOCATION: The AF requests the current or last known location

- INITIAL\_LOCATION: The AF requests the initial location

AssociationType:

anyOf:

- type: string

enum:

- IMEI

- IMEISV

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- IMEI: The value shall be used when the change of IMSI-IMEI association shall be detected

- IMEISV: The value shall be used when the change of IMSI-IMEISV association shall be detected

Accuracy:

anyOf:

- type: string

enum:

- CGI\_ECGI

- ENODEB

- TA\_RA

- PLMN

- TWAN\_ID

- GEO\_AREA

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CGI\_ECGI: The SCS/AS requests to be notified at cell level location accuracy.

- ENODEB: The SCS/AS requests to be notified at eNodeB level location accuracy.

- TA\_RA: The SCS/AS requests to be notified at TA/RA level location accuracy.

- PLMN: The SCS/AS requests to be notified at PLMN level location accuracy.

- TWAN\_ID: The SCS/AS requests to be notified at TWAN identifier level location accuracy.

- GEO\_AREA: The SCS/AS requests to be notified of the geographical area accuracy.

PdnConnectionStatus:

anyOf:

- type: string

enum:

- CREATED

- RELEASED

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CREATED: The PDN connection is created.

- RELEASED: The PDN connection is released.

PdnType:

anyOf:

- type: string

enum:

- IPV4

- IPV6

- IPV4V6

- NON\_IP

- ETHERNET

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- IPV4: PDN connection of IPv4 type.

- IPV6: PDN connection of IPv6 type.

- IPV4V6: PDN connection of IPv4v6 type.

- NON\_IP: PDN connection of non-IP type.

- ETHERNET: PDN connection of Ethernet type.

InterfaceIndication:

anyOf:

- type: string

enum:

- EXPOSURE\_FUNCTION

- PDN\_GATEWAY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- EXPOSURE\_FUNCTION: SCEF is used for the PDN connection towards the SCS/AS.

- PDN\_GATEWAY: PDN gateway is used for the PDN connection towards the SCS/AS.

LocationFailureCause:

anyOf:

- type: string

enum:

- POSITIONING\_DENIED

- UNSUPPORTED\_BY\_UE

- NOT\_REGISTED\_UE

- UNSPECIFIED

- type: string

description: >

This string Indicates the location positioning failure cause.

Possible values are

- POSITIONING\_DENIED: Positioning is denied.

- UNSUPPORTED\_BY\_UE: Positioning is not supported by UE.

- NOT\_REGISTED\_UE: UE is not registered.

- UNSPECIFIED: Unspecified.

SubType:

anyOf:

- type: string

enum:

- AERIAL\_UE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- AERIAL\_UE: The UE has Aerial subscription.

\* \* \* Next changes \* \* \* \*

## A.5 ChargeableParty API

openapi: 3.0.0

info:

title: 3gpp-chargeable-party

version: 1.2.0-alpha.6

description: |

API for Chargeable Party management.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-chargeable-party/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/transactions:

get:

summary: Read all chargeable party transaction resources for a given SCS/AS.

operationId: FetchAllChargeablePartyTransactions

tags:

- Chargeable Party Transaction Operation

parameters:

- name: scsAsId

in: path

description: Identifier of SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: The IPv4 address domain identifier. The attribute may only be provided if IPv4 address is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK (successful query of Chargeable Party resource)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ChargeableParty'

minItems: 0

description: individual BDT policy subscription.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create a new chargeable party transaction resource.

operationId: CreateChargeablePartyTransaction

tags:

- Chargeable Party Transaction Operation

parameters:

- name: scsAsId

in: path

description: Identifier of SCS/AS

required: true

schema:

type: string

requestBody:

description: representation of the Chargeable Party resource to be Created in the SCEF

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ChargeableParty'

callbacks:

eventNotification:

'{$request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/NotificationData'

responses:

'204':

description: No Content (The successful acknowledgement of the notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: successful creation of a chargeable party resource

content:

application/json:

schema:

$ref: '#/components/schemas/ChargeableParty'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/transactions/{transactionId}:

get:

summary: Read a chargeable party resource for a given SCS/AS and a transaction Id.

operationId: FetchIndChargeablePartyTransaction

tags:

- Individual chargeable party resource Operation

parameters:

- name: scsAsId

in: path

description: Identifier of SCS/AS

required: true

schema:

type: string

- name: transactionId

in: path

description: Identifier of transaction

required: true

schema:

type: string

responses:

'200':

description: OK (successful query of a chargeable party resource)

content:

application/json:

schema:

$ref: '#/components/schemas/ChargeableParty'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates a existing chargeable party resource for a given SCS/AS and transaction Id.

operationId: UpdateChargeablePartyTransaction

tags:

- Individual chargeable party resource Operation

parameters:

- name: scsAsId

in: path

description: Identifier of SCS/AS

required: true

schema:

type: string

- name: transactionId

in: path

description: Identifier of transaction

required: true

schema:

type: string

requestBody:

description: representation of the chargeable party resource to be udpated in the SCEF

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/ChargeablePartyPatch'

responses:

'200':

description: successful update of a chargeable party resource

content:

application/json:

schema:

$ref: '#/components/schemas/ChargeableParty'

'204':

description: No Content

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes a chargeable party resource for a given SCS/AS and a transcation Id.

operationId: DeleteChargeablePartyTransaction

tags:

- Individual chargeable party resource Operation

parameters:

- name: scsAsId

in: path

description: Identifier of SCS/AS

required: true

schema:

type: string

- name: transactionId

in: path

description: Identifier of transaction

required: true

schema:

type: string

responses:

'204':

description: successful deletion of an resouce of chargeable party

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/NotificationData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

ChargeableParty:

description: Represents the configuration of a chargeable party.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

exterAppId:

type: string

description: Identifies the external Application Identifier.

ipv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ipv6Addr :

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

macAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describes the application flows.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

sponsorInformation:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/SponsorInformation'

sponsoringEnabled:

type: boolean

description: Indicates sponsoring status.

referenceId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

servAuthInfo:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/ServAuthInfo'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

events:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Event'

minItems: 1

description: Represents the list of event(s) to which the SCS/AS requests to subscribe to.

required:

- notificationDestination

- sponsorInformation

- sponsoringEnabled

ChargeablePartyPatch:

description: Represents a modification request of a chargeable party resource.

type: object

properties:

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describes the IP flows.

exterAppId:

type: string

description: Identifies the external Application Identifier.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

sponsoringEnabled:

type: boolean

description: Indicates sponsoring status.

referenceId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

events:

description: Represents the list of event(s) to which the SCS/AS requests to subscribe to.

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Event'

minItems: 1

\* \* \* Next changes \* \* \* \*

## A.6 NIDD API

openapi: 3.0.0

info:

title: 3gpp**-**nidd

version: 1.2.0-alpha.5

description: |

API for non IP data delivery.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp**-**nidd/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/configurations:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

get:

summary: Read all NIDD configuration resources for a given SCS/AS.

operationId: FetchAllNIDDConfigurations

tags:

- NIDD configurations

responses:

'200':

description: all NIDD configurations.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/NiddConfiguration'

minItems: 0

description: individual NIDD configuration.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create a new NIDD configuration resource.

operationId: CreateNIDDConfiguration

tags:

- NIDD configurations

requestBody:

description: Contains the data to create a NIDD configuration.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NiddConfiguration'

responses:

'201':

description: NIDD configuration is successfully created.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddConfiguration'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

niddNotifications:

'{$request.body#/notificationDestination}':

post:

requestBody:

description: Notification for NIDD configuration status, MO NIDD, MT NIDD delivery report.

required: true

content:

application/json:

schema:

oneOf:

- $ref: '#/components/schemas/NiddConfigurationStatusNotification'

- $ref: '#/components/schemas/NiddUplinkDataNotification'

- $ref: '#/components/schemas/NiddDownlinkDataDeliveryStatusNotification'

- $ref: '#/components/schemas/GmdNiddDownlinkDataDeliveryNotification'

- $ref: '#/components/schemas/ManagePortNotification'

responses:

'204':

description: Expected response to a successful callback processing without a body

'200':

description: Expected response to a successful callback processing with a body

content:

application/json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Acknowledgement'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

- name: configurationId

description: String identifying the individual NIDD configuration resource in the SCEF.

in: path

required: true

schema:

type: string

get:

summary: Read an NIDD configuration resource.

operationId: FetchIndNIDDConfiguration

tags:

- Individual NIDD configuration

responses:

'200':

description: The individual NIDD configuration is successfully retrieved.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddConfiguration'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Modify an existing NIDD configuration resource.

operationId: ModifyNIDDConfiguration

tags:

- Individual NIDD configuration

requestBody:

description: Contains information to be applied to the individual NIDD configuration.

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/NiddConfigurationPatch'

responses:

'200':

description: The Individual NIDD configuration is modified successfully and a representation of that resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddConfiguration'

'204':

description: The Individual NIDD configuration is modified successfully and no content is to be sent in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing NIDD configuration resource.

operationId: DeleteNIDDConfiguration

tags:

- Individual NIDD configuration

responses:

'204':

description: The Individual NIDD configuration is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}/downlink-data-deliveries:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

- name: configurationId

description: String identifying the individual NIDD configuration resource in the SCEF.

in: path

required: true

schema:

type: string

get:

summary: Read all pending NIDD downlink data delivery resources related to a particular NIDD configuration resource.

operationId: FetchAllDownlinkDataDeliveries

tags:

- NIDD downlink data deliveries

responses:

'200':

description: all NIDD downlink data deliveries.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

minItems: 0

description: individual NIDD downlink data delivery.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create an NIDD downlink data delivery resource related to a particular NIDD configuration resource.

operationId: CreateDownlinkDataDelivery

tags:

- NIDD downlink data deliveries

requestBody:

description: Contains the data to create a NIDD downlink data delivery.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

responses:

'200':

description: NIDD downlink data delivery is successful.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

'201':

description: NIDD downlink data delivery is pending.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The NIDD downlink data delivery request was not successful.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataDeliveryFailure'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}/downlink-data-deliveries/{downlinkDataDeliveryId}:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

- name: configurationId

description: String identifying the individual NIDD configuration resource in the SCEF.

in: path

required: true

schema:

type: string

- name: downlinkDataDeliveryId

description: String identifying the individual NIDD downlink data delivery in the SCEF.

in: path

required: true

schema:

type: string

get:

summary: Read pending NIDD downlink data delivery resource.

operationId: FetchIndDownlinkDataDelivery

tags:

- Individual NIDD downlink data delivery

responses:

'200':

description: The individual NIDD downlink data delivery is successfully retrieved.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Replace an NIDD downlink data delivery resource.

operationId: UpdateIndDownlinkDataDelivery

tags:

- Individual NIDD downlink data delivery

requestBody:

description: Contains information to be applied to the individual NIDD downlink data delivery.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

responses:

'200':

description: The pending NIDD downlink data is replaced sucessfully but delivery is pending.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

'204':

description: The NIDD downlink data delivery has been replaced successfully and no content is to be sent in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

$ref: 'TS29122\_CommonData.yaml#/components/responses/409'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The NIDD downlink data replacement request was not successful.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataDeliveryFailure'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an NIDD downlink data delivery resource.

operationId: DeleteIndDownlinkDataDelivery

tags:

- Individual NIDD downlink data delivery

responses:

'204':

description: The pending NIDD downlink data is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

$ref: 'TS29122\_CommonData.yaml#/components/responses/409'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The NIDD downlink data cancellation request was not successful.

content:

application/json:

schema:

$ref: '#/components/schemas/NiddDownlinkDataDeliveryFailure'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}/rds-ports:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

- name: configurationId

description: String identifying the individual NIDD configuration resource in the SCEF.

in: path

required: true

schema:

type: string

get:

summary: Read all RDS ManagePort Configurations.

operationId: FetchAllManagePortConfigurations

tags:

- ManagePort Configurations

responses:

'200':

description: all ManagePort configurations.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/ManagePort'

minItems: 0

description: individual ManagePort configuration.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}/rds-ports/{portId}:

parameters:

- name: scsAsId

description: String identifying the SCS/AS.

in: path

required: true

schema:

type: string

- name: configurationId

description: String identifying the individual NIDD configuration resource in the SCEF.

in: path

required: true

schema:

type: string

- name: portId

description: The UE port number.

in: path

required: true

schema:

type: string

pattern: '^(ue([0-9]|(1[0-5]))-ef([0-9]|(1[0-5])))$'

get:

summary: Read an Individual ManagePort Configuration resource to query port numbers.

operationId: FetchIndManagePortConfiguration

tags:

- Individual ManagePort Configuration

responses:

'200':

description: The individual ManagePort configuration is successfully retrieved.

content:

application/json:

schema:

$ref: '#/components/schemas/ManagePort'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Create a new Individual ManagePort Configuration resource to reserve port numbers.

operationId: UpdateIndManagePortConfiguration

tags:

- Individual ManagePort Configuration

requestBody:

description: Contains information to be applied to the individual ManagePort configuration.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ManagePort'

responses:

'201':

description: The individual ManagePort configuration is created.

content:

application/json:

schema:

$ref: '#/components/schemas/ManagePort'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'202':

description: The request is accepted and under processing.

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

$ref: 'TS29122\_CommonData.yaml#/components/responses/409'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The request was not successful.

content:

application/problem+json:

schema:

$ref: '#/components/schemas/RdsDownlinkDataDeliveryFailure'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an Individual ManagePort Configuration resource to release port numbers.

operationId: DeleteIndManagePortConfiguration

tags:

- Individual ManagePort Configuration

responses:

'202':

description: The request is accepted and under processing.

'204':

description: The individual ManagePort configuration is deleted.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

$ref: 'TS29122\_CommonData.yaml#/components/responses/409'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The request was not successful.

content:

application/problem+json:

schema:

$ref: '#/components/schemas/RdsDownlinkDataDeliveryFailure'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

NiddConfiguration:

description: Represents the configuration for NIDD.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

duration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

reliableDataService:

type: boolean

description: The reliable data service (as defined in subclause 4.5.15.3 of 3GPP TS 23.682) to indicate if a reliable data service acknowledgment is enabled or not.

rdsPorts:

type: array

items:

$ref: '#/components/schemas/RdsPort'

minItems: 1

description: Indicates the static port configuration that is used for reliable data transfer between specific applications using RDS (as defined in subclause 5.2.4 and 5.2.5 of 3GPP TS 24.250).

pdnEstablishmentOption:

$ref: '#/components/schemas/PdnEstablishmentOptions'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

maximumPacketSize:

type: integer

minimum: 1

description: The Maximum Packet Size is the maximum NIDD packet size that was transferred to the UE by the SCEF in the PCO, see subclause 4.5.14.1 of 3GPP TS 23.682. If no maximum packet size was provided to the UE by the SCEF, the SCEF sends a default configured max packet size to SCS/AS. Unit bit.

readOnly: true

niddDownlinkDataTransfers:

type: array

items:

$ref: '#/components/schemas/NiddDownlinkDataTransfer'

minItems: 1

description: The downlink data deliveries that needed to be executed by the SCEF. The cardinality of the property shall be 0..1 in the request and 0..N in the response (i.e. response may contain multiple buffered MT NIDD).

status:

$ref: '#/components/schemas/NiddStatus'

required:

- notificationDestination

oneOf:

- required: [externalId]

- required: [msisdn]

- required: [externalGroupId]

NiddDownlinkDataTransfer:

description: Represents the received NIDD downlink data from the SCS/AS.

type: object

properties:

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

data:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Bytes'

reliableDataService:

type: boolean

description: The reliable data service (as defined in subclause 4.5.15.3 of 3GPP TS 23.682) to indicate if a reliable data service acknowledgment is enabled or not.

rdsPort:

$ref: '#/components/schemas/RdsPort'

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

priority:

type: integer

description: It is used to indicate the priority of the non-IP data packet relative to other non-IP data packets.

pdnEstablishmentOption:

$ref: '#/components/schemas/PdnEstablishmentOptions'

deliveryStatus:

$ref: '#/components/schemas/DeliveryStatus'

requestedRetransmissionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- data

oneOf:

- required: [externalId]

- required: [msisdn]

- required: [externalGroupId]

NiddUplinkDataNotification:

description: Represents NIDD uplink data to be notified to the SCS/AS.

type: object

properties:

niddConfiguration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

data:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Bytes'

reliableDataService:

type: boolean

description: Indicates whether the reliable data service is enabled.

rdsPort:

$ref: '#/components/schemas/RdsPort'

required:

- niddConfiguration

- data

oneOf:

- required: [externalId]

- required: [msisdn]

NiddDownlinkDataDeliveryStatusNotification:

description: Represents the delivery status of a specific NIDD downlink data delivery.

type: object

properties:

niddDownlinkDataTransfer:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

deliveryStatus:

$ref: '#/components/schemas/DeliveryStatus'

requestedRetransmissionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- niddDownlinkDataTransfer

- deliveryStatus

NiddConfigurationStatusNotification:

description: Represents an NIDD configuration status notification.

type: object

properties:

niddConfiguration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

status:

$ref: '#/components/schemas/NiddStatus'

rdsCapIndication:

type: boolean

description: It indicates whether the network capability for the reliable data service is enabled or not.

rdsPort:

$ref: '#/components/schemas/RdsPort'

required:

- niddConfiguration

- status

oneOf:

- required: [externalId]

- required: [msisdn]

GmdNiddDownlinkDataDeliveryNotification:

description: Represents the delivery status of a specific group NIDD downlink data delivery.

type: object

properties:

niddDownlinkDataTransfer:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

gmdResults:

type: array

items:

$ref: '#/components/schemas/GmdResult'

minItems: 1

description: Indicates the group message delivery result.

required:

- niddDownlinkDataTransfer

- gmdResults

RdsPort:

description: Represents the port configuration for Reliable Data Transfer.

type: object

properties:

portUE:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

portSCEF:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

required:

- portUE

- portSCEF

GmdResult:

description: Represents the group message delivery result.

type: object

properties:

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

deliveryStatus:

$ref: '#/components/schemas/DeliveryStatus'

requestedRetransmissionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- deliveryStatus

oneOf:

- required: [externalId]

- required: [msisdn]

NiddDownlinkDataDeliveryFailure:

description: Represents information related to a failure delivery result.

type: object

properties:

problemDetail:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

requestedRetransmissionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

required:

- problemDetail

ManagePort:

description: Represents the configuration of a RDS dynamic port management.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

appId:

type: string

description: Identifies the application.

manageEntity:

$ref: '#/components/schemas/ManageEntity'

skipUeInquiry:

type: boolean

description: Indicate whether to skip UE inquiry.

supportedFormats:

type: array

items:

$ref: '#/components/schemas/SerializationFormat'

minItems: 1

description: Indicates the serialization format(s) that are supported by the SCS/AS on the associated RDS port.

configuredFormat:

$ref: '#/components/schemas/SerializationFormat'

required:

- appId

ManagePortNotification:

description: Represents a ManagePort notification of port numbers that are reserved.

type: object

properties:

niddConfiguration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

managedPorts:

type: array

items:

$ref: '#/components/schemas/ManagePort'

minItems: 1

description: Indicates the reserved RDS port configuration information.

required:

- niddConfiguration

oneOf:

- required: [externalId]

- required: [msisdn]

RdsDownlinkDataDeliveryFailure:

description: Represents the failure delivery result for RDS.

allOf:

- $ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

- type: object

properties:

requestedRetransmissionTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

supportedUeFormats:

type: array

items:

$ref: '#/components/schemas/SerializationFormat'

minItems: 1

description: Indicates the serialization format(s) that are supported by the UE on the associated RDS port.

PdnEstablishmentOptions:

anyOf:

- type: string

enum:

- WAIT\_FOR\_UE

- INDICATE\_ERROR

- SEND\_TRIGGER

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- WAIT\_FOR\_UE: wait for the UE to establish the PDN connection

- INDICATE\_ERROR: respond with an error cause

- SEND\_TRIGGER: send a device trigger

PdnEstablishmentOptionsRm:

description: Represents the same information as the PdnEstablishmentOptions data type with the difference that it allows also the null value.

anyOf:

- $ref: '#/components/schemas/PdnEstablishmentOptions'

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

DeliveryStatus:

anyOf:

- type: string

enum:

- SUCCESS

- SUCCESS\_NEXT\_HOP\_ACKNOWLEDGED

- SUCCESS\_NEXT\_HOP\_UNACKNOWLEDGED

- SUCCESS\_ACKNOWLEDGED

- SUCCESS\_UNACKNOWLEDGED

- TRIGGERED

- BUFFERING

- BUFFERING\_TEMPORARILY\_NOT\_REACHABLE

- SENDING

- FAILURE

- FAILURE\_RDS\_DISABLED

- FAILURE\_NEXT\_HOP

- FAILURE\_TIMEOUT

- FAILURE\_TEMPORARILY\_NOT\_REACHABLE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SUCCESS: Success but details not provided

- SUCCESS\_NEXT\_HOP\_ACKNOWLEDGED: Successful delivery to the next hop with acknowledgment.

- SUCCESS\_NEXT\_HOP\_UNACKNOWLEDGED: Successful delivery to the next hop without acknowledgment

- SUCCESS\_ACKNOWLEDGED: Reliable delivery was acknowledged by the UE

- SUCCESS\_UNACKNOWLEDGED: Reliable delivery was not acknowledged by the UE

- TRIGGERED: The SCEF triggered the device and is buffering the data.

- BUFFERING: The SCEF is buffering the data due to no PDN connection established.

- BUFFERING\_TEMPORARILY\_NOT\_REACHABLE: The SCEF has been informed that the UE is temporarily not reachable but is buffering the data

- SENDING: The SCEF has forwarded the data, but they may be stored elsewhere

- FAILURE: Delivery failure but details not provided

- FAILURE\_RDS\_DISABLED: RDS was disabled

- FAILURE\_NEXT\_HOP: Unsuccessful delivery to the next hop.

- FAILURE\_TIMEOUT: Unsuccessful delivery due to timeout.

- FAILURE\_TEMPORARILY\_NOT\_REACHABLE: The SCEF has been informed that the UE is temporarily not reachable without buffering the data.

readOnly: true

NiddStatus:

anyOf:

- type: string

enum:

- ACTIVE

- TERMINATED\_UE\_NOT\_AUTHORIZED

- TERMINATED

- RDS\_PORT\_UNKNOWN

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- ACTIVE: The NIDD configuration is active.

- TERMINATED\_UE\_NOT\_AUTHORIZED: The NIDD configuration was terminated because the UE´s authorisation was revoked.

- TERMINATED: The NIDD configuration was terminated.

- RDS\_PORT\_UNKNOWN: The RDS port is unknown.

readOnly: true

ManageEntity:

anyOf:

- type: string

enum:

- UE

- AS

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- UE: Representing the UE.

- AS: Representing the Application Server.

readOnly: true

SerializationFormat:

anyOf:

- type: string

enum:

- CBOR

- JSON

- XML

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- CBOR: The CBOR Serialzition format

- JSON: The JSON Serialzition format

- XML: The XML Serialzition format

NiddConfigurationPatch:

description: Represents the parameters to update a NIDD configuration.

type: object

properties:

duration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTimeRm'

reliableDataService:

type: boolean

description: The reliable data service (as defined in subclause 4.5.15.3 of 3GPP TS 23.682) to indicate if a reliable data service acknowledgment is enabled or not.

nullable: true

rdsPorts:

type: array

items:

$ref: '#/components/schemas/RdsPort'

minItems: 1

description: Indicates the static port configuration that is used for reliable data transfer between specific applications using RDS (as defined in subclause 5.2.4 and 5.2.5 of 3GPP TS 24.250).

pdnEstablishmentOption:

$ref: '#/components/schemas/PdnEstablishmentOptionsRm'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

\* \* \* Next changes \* \* \* \*

## A.7 DeviceTriggering API

openapi: 3.0.0

info:

title: 3gpp-device-triggering

version: 1.2.0-alpha.4

description: |

API for device trigger.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-device-triggering/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/transactions:

get:

summary: read all active device triggering transactions for a given SCS/AS.

operationId: FetchAllDeviceTriggeringTransactions

tags:

- Device Triggering Transactions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

responses:

'200':

description: OK (Successful get all of the active device triggering transactions for the SCS/AS)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/DeviceTriggering'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create a long-term transaction for a device triggering.

operationId: CreateDeviceTriggeringTransaction

tags:

- Device Triggering API Transactions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

requestBody:

description: Parameters to request a device triggering delivery.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggeringDeliveryReportNotification'

responses:

'200':

description: OK (successful notification)

content:

application/json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Acknowledgement'

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/transactions/{transactionId}:

get:

summary: Read a device triggering transaction resource.

operationId: FetchIndDeviceTriggeringTransaction

tags:

- Individual Device Triggering Transaction

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

- name: transactionId

in: path

description: Identifier of the transaction resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Replace an existing device triggering transaction resource and the corresponding device trigger request.

operationId: UpdateIndDeviceTriggeringTransaction

tags:

- Individual Device Triggering Transaction

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

- name: transactionId

in: path

description: Identifier of the transaction resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing device triggering

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

responses:

'200':

description: OK (Successful update of the device triggering)

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

'204':

description: No Content (Successful update of the device triggering)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing device triggering transaction.

operationId: DeleteIndDeviceTriggeringTransaction

tags:

- Individual Device Triggering Transaction

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

- name: transactionId

in: path

description: Identifier of the transaction resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/DeviceTriggering'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

DeviceTriggering:

description: Represents device triggering related information.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

validityPeriod:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

priority:

$ref: '#/components/schemas/Priority'

applicationPortId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

appSrcPortId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Port'

triggerPayload:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Bytes'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

deliveryResult:

$ref: '#/components/schemas/DeliveryResult'

required:

- validityPeriod

- priority

- applicationPortId

- triggerPayload

- notificationDestination

oneOf:

- required: [externalId]

- required: [msisdn]

DeviceTriggeringDeliveryReportNotification:

description: Represents a device triggering delivery report notification.

type: object

properties:

transaction:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

result:

$ref: '#/components/schemas/DeliveryResult'

required:

- transaction

- result

DeliveryResult:

anyOf:

- type: string

enum:

- SUCCESS

- UNKNOWN

- FAILURE

- TRIGGERED

- EXPIRED

- UNCONFIRMED

- REPLACED

- TERMINATE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SUCCESS: This value indicates that the device action request was successfully completed.

- UNKNOWN: This value indicates any unspecified errors.

- FAILURE: This value indicates that this trigger encountered a delivery error and is deemed permanently undeliverable.

- TRIGGERED: This value indicates that device triggering request is accepted by the SCEF.

- EXPIRED: This value indicates that the validity period expired before the trigger could be delivered.

- UNCONFIRMED: This value indicates that the delivery of the device action request is not confirmed.

- REPLACED: This value indicates that the device triggering replacement request is accepted by the SCEF.

- TERMINATE: This value indicates that the delivery of the device action request is terminated by the SCS/AS.

readOnly: true

Priority:

anyOf:

- type: string

enum:

- NO\_PRIORITY

- PRIORITY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- NO\_PRIORITY: This value indicates that the device trigger has no priority.

- PRIORITY: This value indicates that the device trigger has priority.

\* \* \* Next changes \* \* \* \*

## A.9 ReportingNetworkStatus API

openapi: 3.0.0

info:

title: 3gpp-network-status-reporting

version: 1.2.0-alpha.4

description: |

API for reporting network status.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-net-stat-report/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

get:

summary: Read all network status reporting subscription resources for a given SCS/AS.

operationId: FetchAllNwStatusReportSubscriptions

tags:

- Network Status Reporting Subscriptions

responses:

'200':

description: The requested information was returned successfully.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create a new network status reporting subscription resource.

operationId: CreateNwStatusReportSubscription

tags:

- Network Status Reporting Subscriptions

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: The subscription was created successfully. The URI of the created resource shall be returned in the "Location" HTTP header.

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ScsAsId'

- name: subscriptionId

in: path

description: Identifier of the subscription resource of type string

required: true

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ResourceId'

get:

summary: Read an active network status reporting subscription resource.

operationId: FetchIndNwStatusReportSubscription

tags:

- Individual Network Status Reporting subscription

responses:

'200':

description: The requested information was returned successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Modify an existing subscription resource to update a subscription.

operationId: UpdateIndNwStatusReportSubscription

tags:

- Individual Network Status Reporting subscription

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

responses:

'200':

description: The subscription was updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/NetworkStatusReportingSubscription'

'204':

description: No Content. The subscription was updated successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete an existing continuous network status reporting subscription resource.

operationId: DeleteIndNwStatusReportSubscription

tags:

- Individual Network Status Reporting subscription

responses:

'204':

description: The subscription was updated successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

NetworkStatusReportingSubscription:

description: Represents a subscription to network status information reporting.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

locationArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

timeDuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

thresholdValues:

type: array

items:

$ref: '#/components/schemas/CongestionValue'

minItems: 1

description: Identifies a list of congestion level(s) with exact value that the SCS/AS requests to be informed of when reached.

thresholdTypes:

type: array

items:

$ref: '#/components/schemas/CongestionType'

minItems: 1

description: Identifies a list of congestion level(s) with abstracted value that the SCS/AS requests to be informed of when reached.

required:

- notificationDestination

- locationArea

not:

required: [thresholdValues, thresholdTypes]

NetworkStatusReportingNotification:

description: Represents a network status reporting notification.

type: object

properties:

subscription:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

nsiValue:

$ref: '#/components/schemas/CongestionValue'

nsiType:

$ref: '#/components/schemas/CongestionType'

required:

- subscription

not:

required: [nsiValue, nsiType]

CongestionValue:

type: integer

minimum: 0

maximum: 31

description: Unsigned integer with valid values between 0 and 31. The value 0 indicates that there is no congestion. The value 1 is the lowest congestion level and value 31 is the highest congestion level.

CongestionType:

anyOf:

- type: string

enum:

- HIGH

- MEDIUM

- LOW

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- HIGH: The congestion status is high.

- MEDIUM: The congestion status is medium.

- LOW: The congestion status is low.

\* \* \* Next changes \* \* \* \*

## A.10 CpProvisioning API

openapi: 3.0.0

info:

title: 3gpp-cp-parameter-provisioning

version: 1.2.0-alpha.4

description: |

API for provisioning communication pattern parameters.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-cp-parameter-provisioning/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

summary: Read all active CP parameter provisioning subscription resources for a given SCS/AS.

operationId: FetchAllCPProvisioningSubscriptions

tags:

- CP provisioning Subscriptions

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpInfo'

minItems: 0

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

summary: Create a new subscription resource of provisioning CP parameter set(s).

operationId: CreateCPProvisioningSubscription

tags:

- CP provisioning Subscriptions

requestBody:

description: create new subscriptions for a given SCS/AS and the provisioning CP parameter sets.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

responses:

'201':

description: Created. The subscription was created successfully. The SCEF shall return the created subscription in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The CP parameters for all sets were not created successfully. CpReport may be included with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

summary: Read a CP parameter provisioning subscription resource.

operationId: FetchIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Modify a CP parameter provisioning subscription resource.

operationId: UpdateIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

requestBody:

description: Modify a CP parameter provisioning subscription resource.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

responses:

'200':

description: OK. The subscription was modified successfully. The SCEF shall return an updated subscription in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/CpInfo'

'204':

description: No Content. The subscription was modified successfully and no content is to be sent in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The CP parameters for all sets were not updated successfully. CpReport may be included with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/CpReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

summary: Delete a CP parameter provisioning subscription resource.

operationId: DeleteIndCPProvisioningSubscription

tags:

- Individual CP Provisioning Subscription

responses:

'204':

description: No Content. The subscription was deleted successfully. The payload body shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}/cpSets/{setId}:

get:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

summary: Read CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: FetchIndCPSetProvisioning

tags:

- Individual CP set Provisioning

responses:

'200':

description: OK. The subscription information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: UpdateIndCPSetProvisioning

tags:

- Individual CP set Provisioning

requestBody:

description: Change information for a CP parameter set.

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

responses:

'200':

description: OK. The CP parameter set resource was modified successfully. The SCEF shall return an updated CP parameter set resource in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/CpParameterSet'

'204':

description: No Content. The CP parameter set resource was modified successfully and no content is to be sent in the response message body.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

description: The CP parameters for the CP set were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/CpReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The CP parameters for the CP set were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/CpReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Subscription ID

required: true

schema:

type: string

- name: setId

in: path

description: Identifier of the CP parameter set

required: true

schema:

type: string

summary: Delete CP at individual CP set(s) level associated with a CP parameter set Id.

operationId: DeleteIndCPSetProvisioning

tags:

- Individual CP set Provisioning

responses:

'204':

description: No Content. The subscription was deleted successfully. The payload body shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

CpInfo:

description: Represents the resources for communication pattern parameter provisioning.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

cpParameterSets:

type: object

additionalProperties:

$ref: '#/components/schemas/CpParameterSet'

minProperties: 1

description: Identifies a set of CP parameter information that may be part of this CpInfo structure. Any string value can be used as a key of the map.

cpReports:

type: object

additionalProperties:

$ref: '#/components/schemas/CpReport'

minProperties: 1

description: Supplied by the SCEF and contains the CP set identifiers for which CP parameter(s) are not added or modified successfully. The failure reason is also included. Each element provides the related information for one or more CP set identifier(s) and is identified in the map via the failure identifier as key.

readOnly: true

required:

- cpParameterSets

oneOf:

- required: [externalId]

- required: [msisdn]

- required: [externalGroupId]

CpParameterSet:

description: Represents an offered communication pattern parameter set.

type: object

properties:

setId:

type: string

description: SCS/AS-chosen correlator provided by the SCS/AS in the request to create a resource fo CP parameter set(s).

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

validityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

periodicCommunicationIndicator:

$ref: '#/components/schemas/CommunicationIndicator'

communicationDurationTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

periodicTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

scheduledCommunicationTime:

$ref: '#/components/schemas/ScheduledCommunicationTime'

scheduledCommunicationType:

$ref: '#/components/schemas/ScheduledCommunicationType'

stationaryIndication:

$ref: '#/components/schemas/StationaryIndication'

batteryInds:

type: array

items:

$ref: '#/components/schemas/BatteryIndication'

minItems: 1

trafficProfile:

$ref: '#/components/schemas/TrafficProfile'

expectedUmts:

type: array

items:

$ref: '#/components/schemas/UmtLocationArea5G'

minItems: 1

description: Identifies the UE's expected geographical movement. The attribute is only applicable in 5G.

expectedUmtDays:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DayOfWeek'

required:

- setId

ScheduledCommunicationTime:

description: Represents an offered scheduled communication time.

type: object

properties:

daysOfWeek:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DayOfWeek'

minItems: 1

maxItems: 6

description: Identifies the day(s) of the week. If absent, it indicates every day of the week.

timeOfDayStart:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

timeOfDayEnd:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

CpReport:

description: Represents a CP report indicating the CP set identifier(s) which CP parameter(s) are not added or modified successfully and the corresponding failure cause(s).

type: object

properties:

setIds:

type: array

items:

type: string

minItems: 1

description: Identifies the CP set identifier(s) which CP parameter(s) are not added or modified successfully

failureCode:

$ref: '#/components/schemas/CpFailureCode'

required:

- failureCode

UmtLocationArea5G:

description: Represents the user location area describing the UE moving trajectory.

allOf:

- $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

- type: object

properties:

umtTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeOfDay'

umtDuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

CommunicationIndicator:

anyOf:

- type: string

enum:

- PERIODICALLY

- ON\_DEMAND

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- PERIODICALLY: Identifies the UE communicates periodically

- ON\_DEMAND: Identifies the UE communicates on demand

StationaryIndication:

anyOf:

- type: string

enum:

- STATIONARY

- MOBILE

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- STATIONARY: Identifies the UE is stationary

- MOBILE: Identifies the UE is mobile

CpFailureCode:

anyOf:

- type: string

enum:

- MALFUNCTION

- SET\_ID\_DUPLICATED

- OTHER\_REASON

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- MALFUNCTION: This value indicates that something functions wrongly in CP parameter provisioning or the CP parameter provisioning does not function at all.

- SET\_ID\_DUPLICATED: The received CP set identifier(s) are already provisioned.

- OTHER\_REASON: Other reason unspecified.

BatteryIndication:

anyOf:

- type: string

enum:

- BATTERY\_RECHARGE

- BATTERY\_REPLACE

- BATTERY\_NO\_RECHARGE

- BATTERY\_NO\_REPLACE

- NO\_BATTERY

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- BATTERY\_RECHARGE: UE powered with rechargeable battery.

- BATTERY\_REPLACE: UE powered with replaceable battery.

- BATTERY\_NO\_RECHARGE: UE powered with no rechargeable battery.

- BATTERY\_NO\_REPLACE: UE powered with no replaceable battery.

- NO\_BATTERY: UE not battery powered.

TrafficProfile:

anyOf:

- type: string

enum:

- SINGLE\_TRANS\_UL

- SINGLE\_TRANS\_DL

- DUAL\_TRANS\_UL\_FIRST

- DUAL\_TRANS\_DL\_FIRST

- MULTI\_TRANS

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SINGLE\_TRANS\_UL: Uplink single packet transmission.

- SINGLE\_TRANS\_DL: Downlink single packet transmission.

- DUAL\_TRANS\_UL\_FIRST: Dual packet transmission, firstly uplink packet transmission with subsequent downlink packet transmission.

- DUAL\_TRANS\_DL\_FIRST: Dual packet transmission, firstly downlink packet transmission with subsequent uplink packet transmission.

- MULTI\_TRANS: Multiple packet transmission.

ScheduledCommunicationType:

anyOf:

- type: string

enum:

- DOWNLINK

- UPLINK

- BIDIRECTIONAL

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- DOWNLINK: Downlink only.

- UPLINK: Uplink only.

- BIDIRECTIONAL: Bi-directional.

\* \* \* Next changes \* \* \* \*

## A.11 PfdManagement API

openapi: 3.0.0

info:

title: 3gpp-pfd-management

version: 1.2.0-alpha.4

description: |

API for PFD management.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-pfd-management/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/transactions:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

get:

summary: Read all PFDs for a given SCS/AS.

operationId: FetchAllPFDManagementTransactions

tags:

- PFD Management Transactions

responses:

'200':

description: OK. All transactions related to the request URI are returned.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdManagement'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Create PFDs for a given SCS/AS and one or more external Application Identifier(s).

operationId: CreatePFDManagementTransaction

tags:

- PFD Management Transactions

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PfdManagement'

description: Create a new transaction for PFD management.

responses:

'201':

description: Created. The transaction was created successfully. The SCEF shall return the created transaction in the response payload body. PfdReport may be included to provide detailed failure information for some applications.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdManagement'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The PFDs for all applications were not created successfully. PfdReport is included with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdReport'

minItems: 1

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/transactions/{transactionId}:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: transactionId

in: path

description: Transaction ID

required: true

schema:

type: string

get:

summary: Read all PFDs for a given SCS/AS and a transaction for one or more external Application Identifier(s).

operationId: FetchIndPFDManagementTransaction

tags:

- Individual PFD Management Transaction

responses:

'200':

description: OK. The transaction information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdManagement'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update PFDs for a given SCS/AS and a transaction for one or more external Application Identifier(s).

operationId: UpdateIndPFDManagementTransaction

tags:

- Individual PFD Management Transaction

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PfdManagement'

description: Change information in PFD management transaction.

responses:

'200':

description: OK. The transaction was modified successfully. The SCEF shall return an updated transaction in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdManagement'

'204':

description: No Content.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The PFDs for all applications were not updated successfully. PfdReport is included with detailed information.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/PfdReport'

minItems: 1

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete PFDs for a given SCS/AS and a transaction for one or more external Application Identifier(s).

operationId: DeleteIndPFDManagementTransaction

tags:

- Individual PFD Management Transaction

responses:

'204':

description: No Content. The transaction was deleted successfully. The payload body shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/transactions/{transactionId}/applications/{appId}:

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS as defined in subclause subclause 5.2.4 of 3GPP TS 29.122.

required: true

schema:

type: string

- name: transactionId

in: path

description: Transaction ID

required: true

schema:

type: string

- name: appId

in: path

description: Identifier of the application

required: true

schema:

type: string

get:

summary: Read PFDs at individual application level.

operationId: FetchIndApplicationPFDManagement

tags:

- Individual Application PFD Management

responses:

'200':

description: OK. The application information related to the request URI is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Update PFDs at individual application level.

operationId: UpdateIndApplicationPFDManagement

tags:

- Individual Application PFD Management

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/PfdData'

description: Change information in application.

responses:

'200':

description: OK. The application resource was modified successfully. The SCEF shall return an updated application resource in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdData'

'204':

description: No Content.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Update PFDs at individual application level.

operationId: ModifyIndApplicationPFDManagement

tags:

- Individual Application PFD Management

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/PfdData'

description: Change information in PFD management transaction.

responses:

'200':

description: OK. The transaction was modified successfully. The SCEF shall return an updated transaction in the response payload body.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdData'

'204':

description: No Content

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'409':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

description: The PFDs for the application were not updated successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/PfdReport'

application/problem+json:

schema:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ProblemDetails'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Delete PFDs at individual application level.

operationId: DeleteIndApplicationPFDManagement

tags:

- Individual Application PFD Management

responses:

'204':

description: No Content. The application was deleted successfully. The payload body shall be empty.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

PfdManagement:

description: Represents a PFD management resource for a PFD management request.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

pfdDatas:

type: object

additionalProperties:

$ref: '#/components/schemas/PfdData'

minProperties: 1

description: Each element uniquely identifies the PFDs for an external application identifier. Each element is identified in the map via an external application identifier as key. The response shall include successfully provisioned PFD data of application(s).

pfdReports:

type: object

additionalProperties:

$ref: '#/components/schemas/PfdReport'

minProperties: 1

description: Supplied by the SCEF and contains the external application identifiers for which PFD(s) are not added or modified successfully. The failure reason is also included. Each element provides the related information for one or more external application identifier(s) and is identified in the map via the failure identifier as key.

readOnly: true

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

required:

- pfdDatas

PfdData:

description: Represents a PFD request to add, update or remove PFD(s) for one external application identifier.

type: object

properties:

externalAppId:

type: string

description: Each element uniquely external application identifier

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

pfds:

type: object

additionalProperties:

$ref: '#/components/schemas/Pfd'

description: Contains the PFDs of the external application identifier. Each PFD is identified in the map via a key containing the PFD identifier.

allowedDelay:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

cachingTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRo'

required:

- externalAppId

- pfds

Pfd:

description: Represents a PFD for an external Application Identifier.

type: object

properties:

pfdId:

type: string

description: Identifies a PDF of an application identifier.

flowDescriptions:

type: array

items:

type: string

minItems: 1

description: Represents a 3-tuple with protocol, server ip and server port for UL/DL application traffic. The content of the string has the same encoding as the IPFilterRule AVP value as defined in IETF RFC 6733.

urls:

type: array

items:

type: string

minItems: 1

description: Indicates a URL or a regular expression which is used to match the significant parts of the URL.

domainNames:

type: array

items:

type: string

minItems: 1

description: Indicates an FQDN or a regular expression as a domain name matching criteria.

dnProtocol:

$ref: '#/components/schemas/DomainNameProtocol'

required:

- pfdId

PfdReport:

description: Represents a PFD report indicating the external application identifier(s) which PFD(s) are not added or modified successfully and the corresponding failure cause(s).

type: object

properties:

externalAppIds:

type: array

items:

type: string

minItems: 1

description: Identifies the external application identifier(s) which PFD(s) are not added or modified successfully

failureCode:

$ref: '#/components/schemas/FailureCode'

cachingTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

locationArea:

$ref: '#/components/schemas/UserPlaneLocationArea'

required:

- externalAppIds

- failureCode

UserPlaneLocationArea:

description: Represents location area(s) of the user plane functions which are unable to enforce the provisioned PFD(s) successfully.

type: object

properties:

locationArea:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea'

locationArea5G:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

dnais:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

minItems: 0

description: Identifies a list of DNAI which the user plane functions support.

FailureCode:

anyOf:

- type: string

enum:

- MALFUNCTION

- RESOURCE\_LIMITATION

- SHORT\_DELAY

- APP\_ID\_DUPLICATED

- PARTIAL\_FAILURE

- OTHER\_REASON

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- MALFUNCTION: This value indicates that something functions wrongly in PFD provisioning or the PFD provisioning does not function at all.

- RESOURCE\_LIMITATION: This value indicates there is resource limitation for PFD storage.

- SHORT\_DELAY: This value indicates that the allowed delay is too short and PFD(s) are not stored.

- APP\_ID\_DUPLICATED: The received external application identifier(s) are already provisioned.

- PARTIAL\_FAILURE: The PFD(s) are not provisioned to all PCEFs/TDFs/SMFs.

- OTHER\_REASON: Other reason unspecified.

DomainNameProtocol:

anyOf:

- type: string

enum:

- DNS\_QNAME

- TLS\_SNI

- TLS\_SAN

- TSL\_SCN

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- DNS\_QNAME: Identifies the DNS protocol and the question name in DNS query.

- TLS\_SNI: Identifies the Server Name Indication in TLS ClientHello message.

- TLS\_SAN: Identifies the Subject Alternative Name in TLS ServerCertificate message.

- TLS\_SCN: Identifies the Subject Common Name in TLS ServerCertificate message.

\* \* \* Next changes \* \* \* \*

## A.13 NpConfiguration API

openapi: 3.0.0

info:

title: 3gpp-network-parameter-configuration

version: 1.2.0-alpha.4

description: |

API for network parameter configuration.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-network-parameter-configuration/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause of 3GPP TS 29.122.

paths:

/{scsAsId}/configurations:

get:

summary: Read all of the active configurations for the SCS/AS.

operationId: FetchAllNPConfigurations

tags:

- Np Configurations

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get all of the active NpConfigurations for the SCS/AS)

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/NpConfiguration'

minItems: 0

description: Network Parameter configurations

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new configuration resource for network parameter configuration.

operationId: CreateNPConfiguration

tags:

- Np Configurations

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: new configuration creation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/ConfigurationNotification'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/configurations/{configurationId}:

get:

summary: Read an active configuration for the SCS/AS and the configuration Id.

operationId: FetchIndNPConfiguration

tags:

- Individual Np Configuration

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: configurationId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing configuration resource.

operationId: UpdateIndNPConfiguration

tags:

- Individual Np Configuration

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: configurationId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing configuration

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

responses:

'200':

description: OK (Successful update of the existing configuration)

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

'204':

description: No Content (Successful update of the configuration)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates/replaces an existing configuration resource.

operationId: ModifyIndNPConfiguration

tags:

- Individual Np Configuration

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: configurationId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/NpConfigurationPatch'

responses:

'200':

description: OK. The configuration was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/NpConfiguration'

'204':

description: No Content. The configuration was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing configuration.

operationId: DeleteIndNPConfiguration

tags:

- Individual Np Configuration

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: configurationId

in: path

description: Identifier of the configuration resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing configuration)

'200':

description: OK. (Successful deletion of the existing configuration)

content:

application/json:

schema:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

minItems: 1

description: The configuration was terminated successfully, the configuration failure information for group members shall be included if received.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

NpConfiguration:

description: Represents a network parameters configuration.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

mtcProviderId:

type: string

description: Identifies the MTC Service Provider and/or MTC Application.

externalId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalId'

msisdn:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Msisdn'

externalGroupId:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ExternalGroupId'

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: This parameter may be included to identify the number of packets that the serving gateway shall buffer in case that the UE is not reachable.

groupReportingGuardTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSec'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

validityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTime'

oneOf:

- required: [externalId]

- required: [msisdn]

- required: [externalGroupId]

NpConfigurationPatch:

description: Represents parameters used to request the modification of a network parameters configuration resource.

type: object

properties:

maximumLatency:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

maximumResponseTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

suggestedNumberOfDlPackets:

type: integer

minimum: 0

description: This parameter may be included to identify the number of packets that the serving gateway shall buffer in case that the UE is not reachable.

nullable: true

groupReportGuardTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DurationSecRm'

validityTime:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/DateTimeRm'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

ConfigurationNotification:

description: Represents a configuration result notification.

type: object

properties:

configuration:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

configResults:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/ConfigResult'

minItems: 1

description: The grouping configuration result notification provided by the SCEF.

appliedParam:

$ref: 'TS29122\_MonitoringEvent.yaml#/components/schemas/AppliedParameterConfiguration'

required:

- configuration

\* \* \* Next changes \* \* \* \*

## A.14 AsSessionWithQoS API

openapi: 3.0.0

info:

title: 3gpp-as-session-with-qos

version: 1.2.0-alpha.4

description: |

API for setting us an AS session with required QoS.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.122 V17.5.0 T8 reference point for Northbound APIs.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.122/'

security:

- {}

- oAuth2ClientCredentials: []

servers:

- url: '{apiRoot}/3gpp-as-session-with-qos/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 5.2.4 of 3GPP TS 29.122.

paths:

/{scsAsId}/subscriptions:

get:

summary: Read all of the active subscriptions for the SCS/AS.

operationId: FetchAllASSessionWithQoSSubscriptions

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: ip-addrs

in: query

description: The IP address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

minItems: 1

- name: ip-domain

in: query

description: The IPv4 address domain identifier. The attribute may only be provided if IPv4 address is included in the ip-addrs query parameter.

required: false

schema:

type: string

- name: mac-addrs

in: query

description: The MAC address(es) of the requested UE(s).

required: false

schema:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

minItems: 1

responses:

'200':

description: OK.

content:

application/json:

schema:

type: array

items:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

post:

summary: Creates a new subscription resource.

operationId: CreateASSessionWithQoSSubscription

tags:

- AS Session with Required QoS Subscriptions

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

requestBody:

description: Request to create a new subscription resource

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

callbacks:

notificationDestination:

'{request.body#/notificationDestination}':

post:

requestBody: # contents of the callback message

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

responses:

'204':

description: No Content (successful notification)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

responses:

'201':

description: Created (Successful creation of subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

headers:

Location:

description: 'Contains the URI of the newly created resource'

required: true

schema:

type: string

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

/{scsAsId}/subscriptions/{subscriptionId}:

get:

summary: Read an active subscriptions for the SCS/AS and the subscription Id.

operationId: FetchIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'200':

description: OK (Successful get the active subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29122\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

put:

summary: Updates/replaces an existing subscription resource.

operationId: UpdateIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

description: Parameters to update/replace the existing subscription

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

responses:

'200':

description: OK (Successful update of the subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content (Successful update of the subscription)

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

patch:

summary: Updates/replaces an existing subscription resource.

operationId: ModifyIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscriptionPatch'

responses:

'200':

description: OK. The subscription was modified successfully.

content:

application/json:

schema:

$ref: '#/components/schemas/AsSessionWithQoSSubscription'

'204':

description: No Content. The subscription was modified successfully.

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29122\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29122\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29122\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an already existing subscription.

operationId: DeleteIndASSessionWithQoSSubscription

tags:

- Individual AS Session with Required QoS Subscription

parameters:

- name: scsAsId

in: path

description: Identifier of the SCS/AS

required: true

schema:

type: string

- name: subscriptionId

in: path

description: Identifier of the subscription resource

required: true

schema:

type: string

responses:

'204':

description: No Content (Successful deletion of the existing subscription)

'200':

description: OK (Successful deletion of the existing subscription)

content:

application/json:

schema:

$ref: '#/components/schemas/UserPlaneNotificationData'

'307':

$ref: 'TS29122\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29122\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29122\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29122\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29122\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29122\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29122\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29122\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29122\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{tokenUrl}'

scopes: {}

schemas:

AsSessionWithQoSSubscription:

description: Represents an individual AS session with required QoS subscription resource.

type: object

properties:

self:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

exterAppId:

type: string

description: Identifies the external Application Identifier.

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

qosReference:

type: string

description: Identifies a pre-defined QoS information

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority.

disUeNotif:

type: boolean

ueIpv4Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipDomain:

type: string

ueIpv6Addr:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Ipv6Addr'

macAddr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

sponsorInfo:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/SponsorInformation'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformation'

directNotifInd:

type: boolean

tscQosReq:

$ref: '#/components/schemas/TscQosRequirement'

requestTestNotification:

type: boolean

description: Set to true by the SCS/AS to request the SCEF to send a test notification as defined in subclause 5.2.5.3. Set to false or omitted otherwise.

websockNotifConfig:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/WebsockNotifConfig'

events:

description: Represents the list of user plane event(s) to which the SCS/AS requests to subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

required:

- notificationDestination

AsSessionWithQoSSubscriptionPatch:

description: Represents parameters to modify an AS session with specific QoS subscription.

type: object

properties:

exterAppId:

type: string

description: Identifies the external Application Identifier.

flowInfo:

type: array

items:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/FlowInfo'

minItems: 1

description: Describe the data flow which requires QoS.

ethFlowInfo:

type: array

items:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

minItems: 1

description: Identifies Ethernet packet flows.

qosReference:

type: string

description: Pre-defined QoS reference

altQoSReferences:

type: array

items:

type: string

minItems: 1

description: Identifies an ordered list of pre-defined QoS information. The lower the index of the array for a given entry, the higher the priority.

disUeNotif:

type: boolean

usageThreshold:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

qosMonInfo:

$ref: '#/components/schemas/QosMonitoringInformationRm'

directNotifInd:

type: boolean

notificationDestination:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

tscQosReq:

$ref: '#/components/schemas/TscQosRequirementRm'

events:

description: Represents the updated list of user plane event(s) to which the SCS/AS requests to subscribe to.

type: array

items:

$ref: '#/components/schemas/UserPlaneEvent'

minItems: 1

QosMonitoringInformation:

description: Represents QoS monitoring information.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

required:

- reqQosMonParams

- repFreqs

QosMonitoringInformationRm:

description: Represents the same as the QosMonitoringInformation data type but with the nullable:true property.

type: object

properties:

reqQosMonParams:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

minItems: 1

repFreqs:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/ReportingFrequency'

minItems: 1

repThreshDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

repThreshRp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

waitTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

repPeriod:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

QosMonitoringReport:

description: Represents a QoS monitoring report.

type: object

properties:

ulDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

dlDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

rtDelays:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

minItems: 1

UserPlaneNotificationData:

description: Represents the parameters to be conveyed in a user plane event(s) notification.

type: object

properties:

transaction:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/Link'

eventReports:

type: array

items:

$ref: '#/components/schemas/UserPlaneEventReport'

minItems: 1

description: Contains the reported event and applicable information

required:

- transaction

- eventReports

UserPlaneEventReport:

description: Represents an event report for user plane.

type: object

properties:

event:

$ref: '#/components/schemas/UserPlaneEvent'

accumulatedUsage:

$ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

flowIds:

type: array

items:

type: integer

minItems: 1

description: Identifies the IP flows that were sent during event subscription

appliedQosRef:

type: string

description: The currently applied QoS reference. Applicable for event QOS\_NOT\_GUARANTEED or SUCCESSFUL\_RESOURCES\_ALLOCATION.

qosMonReports:

type: array

items:

$ref: '#/components/schemas/QosMonitoringReport'

minItems: 1

description: Contains the QoS Monitoring Reporting information

required:

- event

TscQosRequirement:

description: Represents QoS requirements for time sensitive communication.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevel'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

TscQosRequirementRm:

description: Represents the same as the TscQosRequirement data type but with the nullable:true property.

type: object

properties:

reqGbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqGbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

reqMbrUl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

maxTscBurstSize:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

req5Gsdelay:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

priority:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscPriorityLevelRm'

tscaiTimeDom:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UintegerRm'

tscaiInputDl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

tscaiInputUl:

$ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/TscaiInputContainer'

UserPlaneEvent:

anyOf:

- type: string

enum:

- SESSION\_TERMINATION

- LOSS\_OF\_BEARER

- RECOVERY\_OF\_BEARER

- RELEASE\_OF\_BEARER

- USAGE\_REPORT

- FAILED\_RESOURCES\_ALLOCATION

- QOS\_GUARANTEED

- QOS\_NOT\_GUARANTEED

- QOS\_MONITORING

- SUCCESSFUL\_RESOURCES\_ALLOCATION

- type: string

description: >

This string provides forward-compatibility with future

extensions to the enumeration but is not used to encode

content defined in the present version of this API.

description: >

Possible values are

- SESSION\_TERMINATION: Indicates that Rx session is terminated.

- LOSS\_OF\_BEARER : Indicates a loss of a bearer.

- RECOVERY\_OF\_BEARER: Indicates a recovery of a bearer.

- RELEASE\_OF\_BEARER: Indicates a release of a bearer.

- USAGE\_REPORT: Indicates the usage report event.

- FAILED\_RESOURCES\_ALLOCATION: Indicates the resource allocation is failed.

- QOS\_GUARANTEED: The QoS targets of one or more SDFs are guaranteed again.

- QOS\_NOT\_GUARANTEED: The QoS targets of one or more SDFs are not being guaranteed.

- QOS\_MONITORING: Indicates a QoS monitoring event.

- SUCCESSFUL\_RESOURCES\_ALLOCATION: Indicates the resource allocation is successful.

\* \* \* End of changes \* \* \*