**3GPP TSG-CT3 Meeting #120e C3-221666**

**E-Meeting, 17th – 25th February 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | C3 |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CRs modifying the Npcf\_PolicyAuthorization API have been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CRs update the OpenAPI file for Npcf\_PolicyAuthorization for the present release:* TS 29.514 CR# 0379 impacts the OpenAPI file with a backwards compatible feature.
* TS 29.514 CR# 0380 impacts the OpenAPI file with a backwards compatible correction.
* TS 29.514 CR# 0383 impacts the OpenAPI file with a backwards compatible feature.
* TS 29.514 CR# 0389 impacts the OpenAPI file with a backwards compatible correction.
* TS 29.514 CR# 0390 impacts the OpenAPI file with a backwards compatible correction.
* TS 29.514 CR# 0391 impacts the OpenAPI file with a backwards compatible correction.
* TS 29.571 CR# 0332 impacts the OpenAPI file with a backwards compatible correction.

As the present release is not frozen, the API version needs to be upated from 1.2.0-alpha.4 to 1.2.0-alpha.5, and the TS version in the externalDocs field from 17.3.0 to 17.4.0.In addition, the description field covering TS information is updated to cover proper line breaks structure, and the URL of the External Docs field is updated to https. |
|  |  |
| ***Summary of change:*** | Update of the API version number and TS version in externalDocs field for Npcf\_PolicyAuthorization API. Update of description field of TS information and URL of the External Docs field. |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and TS version in externalDocs field. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**Additional discussion(if needed):**

**…**

**Proposed changes:**

\*\*\* 1st Change \*\*\*

# A.2 Npcf\_PolicyAuthorization API

openapi: 3.0.0

info:

 title: Npcf\_PolicyAuthorization Service API

 version: 1.2.0-alpha.5

 description: |

 PCF Policy Authorization Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.514 V17.4.0; 5G System; Policy Authorization Service; Stage 3.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.514/'

#

servers:

 - url: '{apiRoot}/npcf-policyauthorization/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-policyauthorization

paths:

 /app-sessions:

 post:

 summary: Creates a new Individual Application Session Context resource

 operationId: PostAppSessions

 tags:

 - Application Sessions (Collection)

 requestBody:

 description: Contains the information for the creation the resource

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 responses:

 '201':

 description: Successful creation of the resource

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 headers:

 Location:

 description: 'Contains the URI of the created individual application session context resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId} or the URI of the created events subscription sub-resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

 required: true

 schema:

 type: string

 '303':

 description: See Other. The result of the HTTP POST request would be equivalent to the existing Application Session Context.

 headers:

 Location:

 description: 'Contains the URI of the existing individual Application Session Context resource.'

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: '#/components/schemas/ExtendedProblemDetails'

 headers:

 Retry-After:

 description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

 schema:

 anyOf:

 - type: integer

 - type: string

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 terminationRequest:

 '{$request.body#/ascReqData/notifUri}/terminate':

 post:

 requestBody:

 description: Request of the termination of the Individual Application Session Context

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TerminationInfo'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 eventNotification:

 '{$request.body#/ascReqData/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 detected5GsBridgeForPduSession:

 '{$request.body#/ascReqData/evSubsc/notifUri}/new-bridge':

 post:

 requestBody:

 description: Notification of a new TSC user plane node detected in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PduSessionTsnBridge'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 eventNotificationPduSession:

 '{$request.body#/ascReqData/evSubsc/notifUri}/pdu-session':

 post:

 requestBody:

 description: Notification of PDU session established or terminated.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PduSessionEventNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /app-sessions/pcscf-restoration:

 post:

 summary: "Indicates P-CSCF restoration and does not create an Individual Application Session Context"

 operationId: PcscfRestoration

 tags:

 - PCSCF Restoration Indication

 requestBody:

 description: PCSCF Restoration Indication

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PcscfRestorationRequestData'

 responses:

 '204':

 description: The deletion is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

 /app-sessions/{appSessionId}:

 get:

 summary: "Reads an existing Individual Application Session Context"

 operationId: GetAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the resource

 in: path

 required: true

 schema:

 type: string

 responses:

 '200':

 description: A representation of the resource is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 patch:

 summary: "Modifies an existing Individual Application Session Context"

 operationId: ModAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: modification of the resource.

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/AppSessionContextUpdateDataPatch'

 responses:

 '200':

 description: successful modification of the resource and a representation of that resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '204':

 description: The successful modification

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: '#/components/schemas/ExtendedProblemDetails'

 headers:

 Retry-After:

 description: 'Indicates the time the AF has to wait before making a new request. It can be a non-negative integer (decimal number) indicating the number of seconds the AF has to wait before making a new request or an HTTP-date after which the AF can retry a new request.'

 schema:

 anyOf:

 - type: integer

 - type: string

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/ascReqData/evSubsc/notifUri}/notify':

 post:

 requestBody:

 description: Notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

#

 /app-sessions/{appSessionId}/delete:

 post:

 summary: "Deletes an existing Individual Application Session Context"

 operationId: DeleteAppSession

 tags:

 - Individual Application Session Context (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Individual Application Session Context resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: deletion of the Individual Application Session Context resource, req notification

 required: false

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '200':

 description: The deletion of the resource is confirmed and a resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AppSessionContext'

 '204':

 description: The deletion is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

#

 /app-sessions/{appSessionId}/events-subscription:

 put:

 summary: "creates or modifies an Events Subscription subresource"

 operationId: updateEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Events Subscription resource

 in: path

 required: true

 schema:

 type: string

 requestBody:

 description: Creation or modification of an Events Subscription resource.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscReqData'

 responses:

 '201':

 description: The creation of the Events Subscription resource is confirmed and its representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscPutData'

 headers:

 Location:

 description: 'Contains the URI of the created Events Subscription resource, according to the structure: {apiRoot}/npcf-policyauthorization/v1/app-sessions/{appSessionId}/events-subscription}'

 required: true

 schema:

 type: string

 '200':

 description: The modification of the Events Subscription resource is confirmed its representation is returned.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsSubscPutData'

 '204':

 description: The modification of the Events Subscription subresource is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 eventNotification:

 '{$request.body#/notifUri}/notify':

 post:

 requestBody:

 description: Contains the information for the notification of an event occurrence in the PCF.

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/EventsNotification'

 responses:

 '204':

 description: The receipt of the notification is acknowledged.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 summary: deletes the Events Subscription subresource

 operationId: DeleteEventsSubsc

 tags:

 - Events Subscription (Document)

 parameters:

 - name: appSessionId

 description: string identifying the Individual Application Session Context resource

 in: path

 required: true

 schema:

 type: string

 responses:

 '204':

 description: The deletion of the of the Events Subscription sub-resource is confirmed without returning additional data.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-policyauthorization: Access to the Npcf\_PolicyAuthorization API

 schemas:

 AppSessionContext:

 description: Represents an Individual Application Session Context resource.

 type: object

 properties:

 ascReqData:

 $ref: '#/components/schemas/AppSessionContextReqData'

 ascRespData:

 $ref: '#/components/schemas/AppSessionContextRespData'

 evsNotif:

 $ref: '#/components/schemas/EventsNotification'

 AppSessionContextReqData:

 description: Identifies the service requirements of an Individual Application Session Context.

 type: object

 required:

 - notifUri

 - suppFeat

 oneOf:

 - required: [ueIpv4]

 - required: [ueIpv6]

 - required: [ueMac]

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afChargId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 afReqData:

 $ref: '#/components/schemas/AfRequestedData'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirement'

 aspId:

 $ref: '#/components/schemas/AspId'

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqData'

 mcpttId:

 description: indication of MCPTT service request

 type: string

 mcVideoId:

 description: indication of MCVideo service request

 type: string

 medComponents:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponent'

 minProperties: 1

 description: Contains media component information. The key of the map is the medCompN attribute.

 ipDomain:

 type: string

 mpsAction:

 $ref: '#/components/schemas/MpsAction'

 mpsId:

 description: indication of MPS service request

 type: string

 mcsId:

 description: indication of MCS service request

 type: string

 preemptControlInfo:

 $ref: '#/components/schemas/PreemptionControlInformation'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 servInfStatus:

 $ref: '#/components/schemas/ServiceInfoStatus'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 servUrn:

 $ref: '#/components/schemas/ServiceUrn'

 sliceInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 sponId:

 $ref: '#/components/schemas/SponId'

 sponStatus:

 $ref: '#/components/schemas/SponsoringStatus'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 AppSessionContextRespData:

 description: Describes the authorization data of an Individual Application Session Context created by the PCF.

 type: object

 properties:

 servAuthInfo:

 $ref: '#/components/schemas/ServAuthInfo'

 ueIds:

 type: array

 items:

 $ref: '#/components/schemas/UeIdentityInfo'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 AppSessionContextUpdateDataPatch:

 description: Identifies the modifications to an Individual Application Session Context and/or the modifications to the sub-resource Events Subscription.

 type: object

 properties:

 ascReqData:

 $ref: '#/components/schemas/AppSessionContextUpdateData'

 AppSessionContextUpdateData:

 description: Identifies the modifications to the "ascReqData" property of an Individual Application Session Context which may include the modifications to the sub-resource Events Subscription.

 type: object

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirementRm'

 aspId:

 $ref: '#/components/schemas/AspId'

 bdtRefId:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/BdtReferenceId'

 evSubsc:

 $ref: '#/components/schemas/EventsSubscReqDataRm'

 mcpttId:

 description: indication of MCPTT service request

 type: string

 mcVideoId:

 description: indication of modification of MCVideo service

 type: string

 medComponents:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponentRm'

 minProperties: 1

 description: Contains media component information. The key of the map is the medCompN attribute.

 mpsAction:

 $ref: '#/components/schemas/MpsAction'

 mpsId:

 description: indication of MPS service request

 type: string

 mcsId:

 description: indication of MCS service request

 type: string

 preemptControlInfo:

 $ref: '#/components/schemas/PreemptionControlInformationRm'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 servInfStatus:

 $ref: '#/components/schemas/ServiceInfoStatus'

 sipForkInd:

 $ref: '#/components/schemas/SipForkingIndication'

 sponId:

 $ref: '#/components/schemas/SponId'

 sponStatus:

 $ref: '#/components/schemas/SponsoringStatus'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 EventsSubscReqData:

 description: Identifies the events the application subscribes to.

 type: object

 required:

 - events

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/AfEventSubscription'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqQosMonParams:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

 minItems: 1

 qosMon:

 $ref: '#/components/schemas/QosMonitoringInformation'

 reqAnis:

 type: array

 items:

 $ref: '#/components/schemas/RequiredAccessInfo'

 minItems: 1

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThreshold'

 notifCorreId:

 type: string

 afAppIds:

 type: array

 items:

 $ref: '#/components/schemas/AfAppId'

 minItems: 1

 directNotifInd:

 type: boolean

 EventsSubscReqDataRm:

 description: this data type is defined in the same way as the EventsSubscReqData data type, but with the OpenAPI nullable property set to true.

 type: object

 required:

 - events

 properties:

 events:

 type: array

 items:

 $ref: '#/components/schemas/AfEventSubscription'

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 reqQosMonParams:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RequestedQosMonitoringParameter'

 minItems: 1

 qosMon:

 $ref: '#/components/schemas/QosMonitoringInformationRm'

 reqAnis:

 type: array

 items:

 $ref: '#/components/schemas/RequiredAccessInfo'

 minItems: 1

 usgThres:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/UsageThresholdRm'

 notifCorreId:

 type: string

 directNotifInd:

 type: boolean

 nullable: true

 MediaComponent:

 description: Identifies a media component.

 type: object

 required:

 - medCompN

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirement'

 qosReference:

 type: string

 disUeNotif:

 type: boolean

 altSerReqs:

 type: array

 items:

 type: string

 minItems: 1

 contVer:

 $ref: '#/components/schemas/ContentVersion'

 codecs:

 type: array

 items:

 $ref: '#/components/schemas/CodecData'

 minItems: 1

 maxItems: 2

 desMaxLatency:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 desMaxLoss:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 flusId:

 type: string

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxPacketLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxSuppBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 maxSuppBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 medCompN:

 type: integer

 medSubComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaSubComponent'

 minProperties: 1

 description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

 medType:

 $ref: '#/components/schemas/MediaType'

 minDesBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 minDesBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 preemptCap:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapability'

 preemptVuln:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerability'

 prioSharingInd:

 $ref: '#/components/schemas/PrioritySharingIndicator'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 rrBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 rsBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 sharingKeyDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sharingKeyUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 tsnQos:

 $ref: '#/components/schemas/TsnQosContainer'

 tscaiInputDl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiTimeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 MediaComponentRm:

 description: This data type is defined in the same way as the MediaComponent data type, but with the OpenAPI nullable property set to true

 type: object

 required:

 - medCompN

 properties:

 afAppId:

 $ref: '#/components/schemas/AfAppId'

 afRoutReq:

 $ref: '#/components/schemas/AfRoutingRequirementRm'

 qosReference:

 type: string

 nullable: true

 altSerReqs:

 type: array

 items:

 type: string

 minItems: 1

 nullable: true

 disUeNotif:

 type: boolean

 contVer:

 $ref: '#/components/schemas/ContentVersion'

 codecs:

 type: array

 items:

 $ref: '#/components/schemas/CodecData'

 minItems: 1

 maxItems: 2

 desMaxLatency:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

 desMaxLoss:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/FloatRm'

 flusId:

 type: string

 nullable: true

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxPacketLossRateDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxPacketLossRateUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketLossRateRm'

 maxSuppBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 maxSuppBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 medCompN:

 type: integer

 medSubComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaSubComponentRm'

 minProperties: 1

 description: Contains the requested bitrate and filters for the set of service data flows identified by their common flow identifier. The key of the map is the fNum attribute.

 medType:

 $ref: '#/components/schemas/MediaType'

 minDesBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 minDesBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 mirBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 mirBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 preemptCap:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionCapabilityRm'

 preemptVuln:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PreemptionVulnerabilityRm'

 prioSharingInd:

 $ref: '#/components/schemas/PrioritySharingIndicator'

 resPrio:

 $ref: '#/components/schemas/ReservPriority'

 rrBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 rsBw:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 sharingKeyDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

 sharingKeyUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32Rm'

 tsnQos:

 $ref: '#/components/schemas/TsnQosContainerRm'

 tscaiInputDl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiInputUl:

 $ref: '#/components/schemas/TscaiInputContainer'

 tscaiTimeDom:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 nullable: true

 MediaSubComponent:

 description: Identifies a media subcomponent

 type: object

 required:

 - fNum

 properties:

 afSigProtocol:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

 ethfDescs:

 type: array

 items:

 $ref: '#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 fNum:

 type: integer

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 tosTrCl:

 $ref: '#/components/schemas/TosTrafficClass'

 flowUsage:

 $ref: '#/components/schemas/FlowUsage'

 MediaSubComponentRm:

 description: This data type is defined in the same way as the MediaSubComponent data type, but with the OpenAPI nullable property set to true. Removable attributes marBwDl and marBwUl are defined with the corresponding removable data type.

 type: object

 required:

 - fNum

 properties:

 afSigProtocol:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AfSigProtocol'

 ethfDescs:

 type: array

 items:

 $ref: '#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 nullable: true

 fNum:

 type: integer

 fDescs:

 type: array

 items:

 $ref: '#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 nullable: true

 fStatus:

 $ref: '#/components/schemas/FlowStatus'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRateRm'

 tosTrCl:

 $ref: '#/components/schemas/TosTrafficClassRm'

 flowUsage:

 $ref: '#/components/schemas/FlowUsage'

 nullable: true

 EventsNotification:

 description: describes the notification of a matched event

 type: object

 required:

 - evSubsUri

 - evNotifs

 properties:

 adReports:

 type: array

 items:

 $ref: '#/components/schemas/AppDetectionReport'

 minItems: 1

 description: includes the detected application report.

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 addAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 relAccessInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AdditionalAccessInfo'

 anChargAddr:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AccNetChargingAddress'

 anChargIds:

 type: array

 items:

 $ref: '#/components/schemas/AccessNetChargingIdentifier'

 minItems: 1

 anGwAddr:

 $ref: '#/components/schemas/AnGwAddress'

 evSubsUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 evNotifs:

 type: array

 items:

 $ref: '#/components/schemas/AfEventNotification'

 minItems: 1

 failedResourcAllocReports:

 type: array

 items:

 $ref: '#/components/schemas/ResourcesAllocationInfo'

 minItems: 1

 succResourcAllocReports:

 type: array

 items:

 $ref: '#/components/schemas/ResourcesAllocationInfo'

 minItems: 1

 noNetLocSupp:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/NetLocAccessSupport'

 outOfCredReports:

 type: array

 items:

 $ref: '#/components/schemas/OutOfCreditInformation'

 minItems: 1

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 qncReports:

 type: array

 items:

 $ref: '#/components/schemas/QosNotificationControlInfo'

 minItems: 1

 qosMonReports:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 1

 ranNasRelCauses:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

 minItems: 1

 description: Contains the RAN and/or NAS release cause.

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 satBackhaulCategory:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SatelliteBackhaulCategory'

 ueLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueLocTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 usgRep:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/AccumulatedUsage'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 AfEventSubscription:

 description: describes the event information delivered in the subscription

 type: object

 required:

 - event

 properties:

 event:

 $ref: '#/components/schemas/AfEvent'

 notifMethod:

 $ref: '#/components/schemas/AfNotifMethod'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 waitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 AfEventNotification:

 description: describes the event information delivered in the notification

 type: object

 required:

 - event

 properties:

 event:

 $ref: '#/components/schemas/AfEvent'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 TerminationInfo:

 description: indicates the cause for requesting the deletion of the Individual Application Session Context resource

 type: object

 required:

 - termCause

 - resUri

 properties:

 termCause:

 $ref: '#/components/schemas/TerminationCause'

 resUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 AfRoutingRequirement:

 description: describes the event information delivered in the subscription

 type: object

 properties:

 appReloc:

 type: boolean

 routeToLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 spVal:

 $ref: '#/components/schemas/SpatialValidity'

 tempVals:

 type: array

 items:

 $ref: '#/components/schemas/TemporalValidity'

 minItems: 1

 upPathChgSub:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

 addrPreserInd:

 type: boolean

 simConnInd:

 type: boolean

 description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

 simConnTerm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 easIpReplaceInfos:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/EasIpReplacementInfo'

 minItems: 1

 description: Contains EAS IP replacement information.

 SpatialValidity:

 description: describes explicitly the route to an Application location

 type: object

 required:

 - presenceInfoList

 properties:

 presenceInfoList:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

 SpatialValidityRm:

 description: this data type is defined in the same way as the SpatialValidity data type, but with the OpenAPI nullable property set to true

 type: object

 required:

 - presenceInfoList

 properties:

 presenceInfoList:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: Defines the presence information provisioned by the AF. The praId attribute within the PresenceInfo data type is the key of the map.

 nullable: true

 AfRoutingRequirementRm:

 description: this data type is defined in the same way as the AfRoutingRequirement data type, but with the OpenAPI nullable property set to true and the spVal and tempVals attributes defined as removable.

 type: object

 properties:

 appReloc:

 type: boolean

 routeToLocs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 minItems: 1

 nullable: true

 spVal:

 $ref: '#/components/schemas/SpatialValidityRm'

 tempVals:

 type: array

 items:

 $ref: '#/components/schemas/TemporalValidity'

 minItems: 1

 nullable: true

 upPathChgSub:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/UpPathChgEvent'

 addrPreserInd:

 type: boolean

 nullable: true

 simConnInd:

 type: boolean

 nullable: true

 description: Indicates whether simultaneous connectivity should be temporarily maintained for the source and target PSA.

 simConnTerm:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSecRm'

 easIpReplaceInfos:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/EasIpReplacementInfo'

 minItems: 1

 description: Contains EAS IP replacement information.

 nullable: true

 nullable: true

 AnGwAddress:

 description: describes the address of the access network gateway control node

 type: object

 anyOf:

 - required: [anGwIpv4Addr]

 - required: [anGwIpv6Addr]

 properties:

 anGwIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 anGwIpv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 Flows:

 description: Identifies the flows

 type: object

 required:

 - medCompN

 properties:

 contVers:

 type: array

 items:

 $ref: '#/components/schemas/ContentVersion'

 minItems: 1

 fNums:

 type: array

 items:

 type: integer

 minItems: 1

 medCompN:

 type: integer

 EthFlowDescription:

 description: Identifies an Ethernet flow

 type: object

 required:

 - ethType

 properties:

 destMacAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 ethType:

 type: string

 fDesc:

 $ref: '#/components/schemas/FlowDescription'

 fDir:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowDirection'

 sourceMacAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 vlanTags:

 type: array

 items:

 type: string

 minItems: 1

 maxItems: 2

 srcMacAddrEnd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 destMacAddrEnd:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 ResourcesAllocationInfo:

 description: describes the status of the PCC rule(s) related to certain media components.

 type: object

 properties:

 mcResourcStatus:

 $ref: '#/components/schemas/MediaComponentResourcesStatus'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 altSerReq:

 type: string

 TemporalValidity:

 description: Indicates the time interval(s) during which the AF request is to be applied

 type: object

 properties:

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

#

 QosNotificationControlInfo:

 description: Indicates whether the QoS targets for a GRB flow are not guaranteed or guaranteed again

 type: object

 required:

 - notifType

 properties:

 notifType:

 $ref: '#/components/schemas/QosNotifType'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 altSerReq:

 type: string

#

 AcceptableServiceInfo:

 description: Indicates the maximum bandwidth that shall be authorized by the PCF.

 type: object

 properties:

 accBwMedComps:

 type: object

 additionalProperties:

 $ref: '#/components/schemas/MediaComponent'

 description: Indicates the maximum bandwidth that shall be authorized by the PCF for each media component of the map. The key of the map is the media component number.

 minProperties: 1

 marBwUl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 marBwDl:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

 UeIdentityInfo:

 description: Represents 5GS-Level UE identities.

 type: object

 anyOf:

 - required: [gpsi]

 - required: [pei]

 - required: [supi]

 properties:

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

#

 AccessNetChargingIdentifier:

 description: Describes the access network charging identifier.

 type: object

 required:

 - accNetChaIdValue

 properties:

 accNetChaIdValue:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

#

 OutOfCreditInformation:

 description: Indicates the SDFs without available credit and the corresponding termination action.

 type: object

 required:

 - finUnitAct

 properties:

 finUnitAct:

 $ref: 'TS32291\_Nchf\_ConvergedCharging.yaml#/components/schemas/FinalUnitAction'

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

#

 QosMonitoringInformation:

 description: Indicates the QoS Monitoring information to report, i.e. UL and/or DL and or round trip delay.

 type: object

 properties:

 repThreshDl:

 type: integer

 repThreshUl:

 type: integer

 repThreshRp:

 type: integer

#

#

 PduSessionTsnBridge:

 description: Contains the new TSC user plane node information and may contain the DS-TT port and/or NW-TT port management information.

 type: object

 required:

 - tsnBridgeInfo

 properties:

 tsnBridgeInfo:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/TsnBridgeInfo'

 tsnBridgeManCont:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/BridgeManagementContainer'

 tsnPortManContDstt:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 tsnPortManContNwtts:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/PortManagementContainer'

 minItems: 1

 ueIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6AddrPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

#

 QosMonitoringInformationRm:

 description: this data type is defined in the same way as the QosMonitoringInformation data type, but with the OpenAPI nullable property set to true.

 type: object

 properties:

 repThreshDl:

 type: integer

 repThreshUl:

 type: integer

 repThreshRp:

 type: integer

 nullable: true

#

 PcscfRestorationRequestData:

 description: Indicates P-CSCF restoration.

 type: object

 oneOf:

 - required: [ueIpv4]

 - required: [ueIpv6]

 properties:

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 ipDomain:

 type: string

 sliceInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

#

#

 QosMonitoringReport:

 description: QoS Monitoring reporting information

 type: object

 properties:

 flows:

 type: array

 items:

 $ref: '#/components/schemas/Flows'

 minItems: 1

 ulDelays:

 type: array

 items:

 type: integer

 minItems: 1

 dlDelays:

 type: array

 items:

 type: integer

 minItems: 1

 rtDelays:

 type: array

 items:

 type: integer

 minItems: 1

#

 TsnQosContainer:

 description: Indicates TSC Traffic QoS.

 type: object

 properties:

 maxTscBurstSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVol'

 tscPackDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

 tscPrioLevel:

 $ref: '#/components/schemas/TscPriorityLevel'

#

#

 TsnQosContainerRm:

 description: Indicates removable TSC Traffic QoS.

 type: object

 properties:

 maxTscBurstSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExtMaxDataBurstVolRm'

 tscPackDelay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudgetRm'

 tscPrioLevel:

 $ref: '#/components/schemas/TscPriorityLevelRm'

 nullable: true

#

 TscaiInputContainer:

 description: Indicates TSC Traffic pattern.

 type: object

 properties:

 periodicity:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 burstArrivalTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 surTimeInNumMsg:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 surTimeInTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 nullable: true

#

#

 AppDetectionReport:

 description: Indicates the start or stop of the detected application traffic and the application identifier of the detected application traffic.

 type: object

 required:

 - adNotifType

 - afAppId

 properties:

 adNotifType:

 $ref: '#/components/schemas/AppDetectionNotifType'

 afAppId:

 $ref: '#/components/schemas/AfAppId'

#

#

 PduSessionEventNotification:

 description: Indicates PDU session information for the concerned established/terminated PDU session.

 type: object

 required:

 - evNotif

 properties:

 evNotif:

 $ref: '#/components/schemas/AfEventNotification'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 ueIpv4:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ueIpv6:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 status:

 $ref: '#/components/schemas/PduSessionStatus'

 pcfInfo:

 $ref: '#/components/schemas/PcfAddressingInfo'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

#

#

 PcfAddressingInfo:

 description: Contains PCF address information.

 type: object

 properties:

 pcfFqdn:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

 pcfIpEndPoints:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/IpEndPoint'

 minItems: 1

 description: IP end points of the PCF hosting the Npcf\_PolicyAuthorization service.

 pcfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 pcfSetId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfSetId'

 bindLevel:

 $ref: 'TS29521\_Nbsf\_Management.yaml#/components/schemas/BindingLevel'

#

 EventsSubscPutData:

 description: Identifies the events the application subscribes to within an Events Subscription sub-resource data. It may contain the notification of the already met events

 anyOf:

 - $ref: '#/components/schemas/EventsSubscReqData'

 - $ref: '#/components/schemas/EventsNotification'

#

# EXTENDED PROBLEMDETAILS

#

 ExtendedProblemDetails:

 description: Extends ProblemDetails to also include the acceptable service info.

 allOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - type: object

 properties:

 acceptableServInfo:

 $ref: '#/components/schemas/AcceptableServiceInfo'

#

# SIMPLE DATA TYPES

#

 AfAppId:

 description: Contains an AF application identifier.

 type: string

 AspId:

 description: Contains an identity of an application service provider.

 type: string

 CodecData:

 description: Contains codec related information.

 type: string

 ContentVersion:

 description: Represents the content version of some content.

 type: integer

 FlowDescription:

 description: Defines a packet filter of an IP flow.

 type: string

 SponId:

 description: Contains an identity of a sponsor.

 type: string

 ServiceUrn:

 description: Contains values of the service URN and may include subservices.

 type: string

 TosTrafficClass:

 description: 2-octet string, where each octet is encoded in hexadecimal representation. The first octet contains the IPv4 Type-of-Service or the IPv6 Traffic-Class field and the second octet contains the ToS/Traffic Class mask field.

 type: string

 TosTrafficClassRm:

 description: this data type is defined in the same way as the TosTrafficClass data type, but with the OpenAPI nullable property set to true

 type: string

 nullable: true

 TscPriorityLevel:

 description: Represents the priority level of TSC Flows.

 type: integer

 minimum: 1

 maximum: 8

 TscPriorityLevelRm:

 description: This data type is defined in the same way as the TscPriorityLevel data type, but with the OpenAPI nullable property set to true.

 type: integer

 minimum: 1

 maximum: 8

 nullable: true

#

# ENUMERATIONS DATA TYPES

#

 MediaType:

 description: Indicates the media type of a media component.

 anyOf:

 - type: string

 enum:

 - AUDIO

 - VIDEO

 - DATA

 - APPLICATION

 - CONTROL

 - TEXT

 - MESSAGE

 - OTHER

 - type: string

#

 MpsAction:

 description: Indicates whether it is an invocation, a revocation or an invocation with authorization of the MPS for DTS service.

 anyOf:

 - type: string

 enum:

 - DISABLE\_MPS\_FOR\_DTS

 - ENABLE\_MPS\_FOR\_DTS

 - AUTHORIZE\_AND\_ENABLE\_MPS\_FOR\_DTS

 - type: string

#

 ReservPriority:

 description: Indicates the reservation priority.

 anyOf:

 - type: string

 enum:

 - PRIO\_1

 - PRIO\_2

 - PRIO\_3

 - PRIO\_4

 - PRIO\_5

 - PRIO\_6

 - PRIO\_7

 - PRIO\_8

 - PRIO\_9

 - PRIO\_10

 - PRIO\_11

 - PRIO\_12

 - PRIO\_13

 - PRIO\_14

 - PRIO\_15

 - PRIO\_16

 - type: string

#

 ServAuthInfo:

 description: Indicates the result of the Policy Authorization service request from the AF.

 anyOf:

 - type: string

 enum:

 - TP\_NOT\_KNOWN

 - TP\_EXPIRED

 - TP\_NOT\_YET\_OCURRED

 - ROUT\_REQ\_NOT\_AUTHORIZED

 - type: string

#

 SponsoringStatus:

 description: Indicates whether sponsored data connectivity is enabled or disabled/not enabled.

 anyOf:

 - type: string

 enum:

 - SPONSOR\_DISABLED

 - SPONSOR\_ENABLED

 - type: string

#

 AfEvent:

 description: Represents an event to notify to the AF.

 anyOf:

 - type: string

 enum:

 - ACCESS\_TYPE\_CHANGE

 - ANI\_REPORT

 - APP\_DETECTION

 - CHARGING\_CORRELATION

 - EPS\_FALLBACK

 - FAILED\_QOS\_UPDATE

 - FAILED\_RESOURCES\_ALLOCATION

 - OUT\_OF\_CREDIT

 - PDU\_SESSION\_STATUS

 - PLMN\_CHG

 - QOS\_MONITORING

 - QOS\_NOTIF

 - RAN\_NAS\_CAUSE

 - REALLOCATION\_OF\_CREDIT

 - SAT\_CATEGORY\_CHG

 - SUCCESSFUL\_QOS\_UPDATE

 - SUCCESSFUL\_RESOURCES\_ALLOCATION

 - TSN\_BRIDGE\_INFO

 - UP\_PATH\_CHG\_FAILURE

 - USAGE\_REPORT

 - type: string

#

 AfNotifMethod:

 description: Represents the notification methods that can be subscribed for an event.

 anyOf:

 - type: string

 enum:

 - EVENT\_DETECTION

 - ONE\_TIME

 - PERIODIC

 - PDU\_SESSION\_RELEASE

 - type: string

#

 QosNotifType:

 description: Indicates the notification type for QoS Notification Control.

 anyOf:

 - type: string

 enum:

 - GUARANTEED

 - NOT\_GUARANTEED

 - type: string

#

 TerminationCause:

 description: Indicates the cause behind requesting the deletion of the Individual Application Session Context resource.

 anyOf:

 - type: string

 enum:

 - ALL\_SDF\_DEACTIVATION

 - PDU\_SESSION\_TERMINATION

 - PS\_TO\_CS\_HO

 - INSUFFICIENT\_SERVER\_RESOURCES

 - INSUFFICIENT\_QOS\_FLOW\_RESOURCES

 - SPONSORED\_DATA\_CONNECTIVITY\_DISALLOWED

 - type: string

#

 MediaComponentResourcesStatus:

 description: Indicates whether the media component is active or inactive.

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

#

#

 FlowUsage:

 description: Describes the flow usage of the flows described by a media subcomponent.

 anyOf:

 - type: string

 enum:

 - NO\_INFO

 - RTCP

 - AF\_SIGNALLING

 - type: string

 FlowStatus:

 description: Describes whether the IP flow(s) are enabled or disabled.

 anyOf:

 - type: string

 enum:

 - ENABLED-UPLINK

 - ENABLED-DOWNLINK

 - ENABLED

 - DISABLED

 - REMOVED

 - type: string

#

 RequiredAccessInfo:

 description: Indicates the access network information required for an AF session.

 anyOf:

 - type: string

 enum:

 - USER\_LOCATION

 - UE\_TIME\_ZONE

 - type: string

#

 SipForkingIndication:

 description: Indicates whether several SIP dialogues are related to an "Individual Application Session Context" resource.

 anyOf:

 - type: string

 enum:

 - SINGLE\_DIALOGUE

 - SEVERAL\_DIALOGUES

 - type: string

#

 AfRequestedData:

 description: Represents the information that the AF requested to be exposed.

 anyOf:

 - type: string

 enum:

 - UE\_IDENTITY

 - type: string

#

 ServiceInfoStatus:

 description: Represents the preliminary or final service information status.

 anyOf:

 - type: string

 enum:

 - FINAL

 - PRELIMINARY

 - type: string

#

 PreemptionControlInformation:

 description: Represents Pre-emption control information.

 anyOf:

 - type: string

 enum:

 - MOST\_RECENT

 - LEAST\_RECENT

 - HIGHEST\_BW

 - type: string

#

 PrioritySharingIndicator:

 description: Represents the Priority sharing indicator.

 anyOf:

 - type: string

 enum:

 - ENABLED

 - DISABLED

 - type: string

#

 PreemptionControlInformationRm:

 description: This data type is defined in the same way as the PreemptionControlInformation data type, but with the OpenAPI nullable property set to true.

 anyOf:

 - $ref: '#/components/schemas/PreemptionControlInformation'

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/NullValue'

#

 AppDetectionNotifType:

 description: Indicates the notification type for Application Detection Control.

 anyOf:

 - type: string

 enum:

 - APP\_START

 - APP\_STOP

 - type: string

#

 PduSessionStatus:

 description: Indicates whether the PDU session is established or terminated.

 anyOf:

 - type: string

 enum:

 - ESTABLISHED

 - TERMINATED

 - type: string

\*\*\* End of Changes \*\*\*