**3GPP TSG-CT3 Meeting #121e C3-222067**

**E-Meeting, 6th – 12th April 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.525** | **CR** | **0201** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Formatting of description fields |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | SBIProtoc17 |  | ***Date:*** | 2022-03-30 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Formatting of description fields is not consistently applied along the OpenAPI file according to CommonMark Markdown formatting (see <https://spec.commonmark.org/0.27>). |
|  |  |
| ***Summary of change:*** | Update of the description fields to follow the guidelines specified in TS 29.501 (see [C4-220197](https://www.3gpp.org/ftp/tsg_ct/WG4_protocollars_ex-CN4/TSGCT4_107e-bis_meeting/Docs/C4-220197.zip) agreed in CT4 #107-bis-e meeting). |
|  |  |
| ***Consequences if not approved:*** | The documentation of 3GPP OpenAPI descriptions, which is frequently generated automatically with tools from the YAML files, is not formatted as intended and gives an image of low quality documentation. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces backward compatible correction to the OpenAPI file of the Npcf\_UEPolicyControl API. |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Npcf\_UEPolicyControl API

openapi: 3.0.0

info:

 version: 1.2.0-alpha.7

 title: Npcf\_UEPolicyControl

 description: |

 UE Policy Control Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.525 V17.6.0; 5G System; UE Policy Control Service.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.525/'

servers:

 - url: '{apiRoot}/npcf-ue-policy-control/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - npcf-ue-policy-control

paths:

 /policies:

 post:

 operationId: CreateIndividualUEPolicyAssociation

 summary: Create individual UE policy association.

 tags:

 - UE Policy Associations (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociationRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociation'

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource, according to the structure:

 {apiRoot}/npcf-ue-policy-control/v1/policies/{polAssoId}

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 policyUpdateNotification:

 '{$request.body#/notificationUri}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyUpdate'

 responses:

 '200':

 description: >

 OK. The current applicable values corresponding to the policy control

 request trigger is reported

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/UeRequestedValueRep'

 '204':

 description: No Content, Notification was successful

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 policyAssocitionTerminationRequestNotification:

 '{$request.body#/notificationUri}/terminate':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/TerminationNotification'

 responses:

 '204':

 description: No Content, Notification was successful

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /policies/{polAssoId}:

 get:

 operationId: ReadIndividualUEPolicyAssociation

 summary: Read individual UE policy association.

 tags:

 - Individual UE Policy Association (Document)

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociation'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualUEPolicyAssociation

 summary: Delete individual UE policy association.

 tags:

 - Individual UE Policy Association (Document)

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /policies/{polAssoId}/update:

 post:

 operationId: ReportObservedEventTriggersForIndividualUEPolicyAssociation

 summary: >

 Report observed event triggers and possibly obtain updated policies for an individual UE

 policy association.

 tags:

 - Individual UE Policy Association (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyAssociationUpdateRequest'

 parameters:

 - name: polAssoId

 in: path

 description: Identifier of a policy association

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated policies are returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/PolicyUpdate'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 npcf-ue-policy-control: Access to the Npcf\_UEPolicyControl API

 schemas:

 PolicyAssociation:

 description: >

 Contains the description of a policy association that is returned by the PCF when a policy

 Association is created, updated, or read.

 type: object

 properties:

 request:

 $ref: '#/components/schemas/PolicyAssociationRequest'

 uePolicy:

 $ref: '#/components/schemas/UePolicy'

 n2Pc5Pol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 n2Pc5ProSePol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 description: >

 Request Triggers that the PCF subscribes. Only values "LOC\_CH" and "PRA\_CH" are

 permitted.

 pras:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: >

 Contains the presence reporting area(s) for which reporting was requested. The praId

 attribute within the PresenceInfo data type is the key of the map.

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - suppFeat

 PolicyAssociationRequest:

 description: >

 Represents information that the NF service consumer provides when requesting the creation of

 a policy association.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 description: Alternate or backup IPv4 Address(es) where to send Notifications.

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 description: Alternate or backup IPv6 Address(es) where to send Notifications.

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 accessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 pei:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 timeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 servingPlmn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnIdNid'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 groupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 hPcfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 uePolReq:

 $ref: '#/components/schemas/UePolicyRequest'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 serviceName:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

 servingNfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 pc5Capab:

 $ref: '#/components/schemas/Pc5Capability'

 proSeCapab:

 type: array

 items:

 $ref: '#/components/schemas/ProSeCapability'

 minItems: 1

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - notificationUri

 - suppFeat

 - supi

 PolicyAssociationUpdateRequest:

 description: >

 Represents Information that the NF service consumer provides when requesting the update of

 a policy association.

 type: object

 properties:

 notificationUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 minItems: 1

 description: Alternate or backup IPv4 Address(es) where to send Notifications.

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 description: Alternate or backup IPv6 Address(es) where to send Notifications.

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 description: Request Triggers that the NF service consumer observes.

 praStatuses:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 description: >

 Contains the UE presence status for tracking area for which changes of the UE presence

 occurred. The praId attribute within the PresenceInfo data type is the key of the map.

 minProperties: 1

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uePolDelResult:

 $ref: '#/components/schemas/UePolicyDeliveryResult'

 uePolTransFailNotif:

 $ref: '#/components/schemas/UePolicyTransferFailureNotification'

 uePolReq:

 $ref: '#/components/schemas/UePolicyRequest'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 servingNfId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 connectState:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CmState'

 groupIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 minItems: 1

 proSeCapab:

 type: array

 items:

 $ref: '#/components/schemas/ProSeCapability'

 minItems: 1

 PolicyUpdate:

 description: >

 Represents updated policies that the PCF provides in a notification or in the reply to an

 Update Request.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 uePolicy:

 $ref: '#/components/schemas/UePolicy'

 n2Pc5Pol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 n2Pc5ProSePol:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N2InfoContent'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/RequestTrigger'

 minItems: 1

 nullable: true

 description: >

 Request Triggers that the PCF subscribes. Only values "LOC\_CH" and "PRA\_CH" are

 permitted.

 pras:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 description: >

 Contains the presence reporting area(s) for which reporting was requested. The praId

 attribute within the PresenceInfo data type is the key of the map.

 minProperties: 1

 nullable: true

 required:

 - resourceUri

 TerminationNotification:

 description: >

 Represents a request to terminate a policy association that the PCF provides in a

 notification.

 type: object

 properties:

 resourceUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 cause:

 $ref: '#/components/schemas/PolicyAssociationReleaseCause'

 required:

 - resourceUri

 - cause

 UePolicyTransferFailureNotification:

 description: >

 Represents information on the failure of a UE policy transfer to the UE because the UE is

 not reachable.

 type: object

 properties:

 cause:

 $ref: 'TS29518\_Namf\_Communication.yaml#/components/schemas/N1N2MessageTransferCause'

 ptis:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 required:

 - cause

 - ptis

 UeRequestedValueRep:

 description: >

 Contains the current applicable values corresponding to the policy control request triggers.

 type: object

 properties:

 userLoc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 praStatuses:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 1

 description: >

 Contains the UE presence statuses for tracking areas. The praId attribute within the

 PresenceInfo data type is the key of the map.

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 connectState:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CmState'

 UePolicy:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 UePolicyDeliveryResult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 UePolicyRequest:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 RequestTrigger:

 anyOf:

 - type: string

 enum:

 - LOC\_CH

 - PRA\_CH

 - UE\_POLICY

 - PLMN\_CH

 - CON\_STATE\_CH

 - GROUP\_ID\_LIST\_CHG

 - UE\_CAP\_CH

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LOC\_CH: Location change (tracking area). The tracking area of the UE has changed.

 - PRA\_CH: Change of UE presence in PRA. The AMF reports the current presence status of the

 UE in a Presence Reporting Area, and notifies that the UE enters/leaves the Presence

 Reporting Area.

 - UE\_POLICY: A MANAGE UE POLICY COMPLETE message or a MANAGE UE POLICY COMMAND REJECT

 message, as defined in Annex D.5 of 3GPP TS 24.501 or a "UE POLICY PROVISIONING REQUEST"

 message, as defined in subclause 7.2.1.1 of 3GPP TS 24.587 , has been received by the AMF

 and is being forwarded.

 - PLMN\_CH: PLMN change. the serving PLMN of UE has changed.

 - CON\_STATE\_CH: Connectivity state change: the connectivity state of UE has changed.

 - GROUP\_ID\_LIST\_CHG: UE Internal Group Identifier(s) has changed. This policy control

 request trigger does not require a subscription

 - UE\_CAP\_CH: UE Capabilities change: the UE provided 5G ProSe capabilities have changed.

 This policy control request trigger does not require subscription.

 PolicyAssociationReleaseCause:

 anyOf:

 - type: string

 enum:

 - UNSPECIFIED

 - UE\_SUBSCRIPTION

 - INSUFFICIENT\_RES

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - UNSPECIFIED: This value is used for unspecified reasons.

 - UE\_SUBSCRIPTION: This value is used to indicate that the policy association needs to be

 terminated because the subscription of UE has changed (e.g. was removed).

 - INSUFFICIENT\_RES: This value is used to indicate that the server is overloaded and needs

 to abort the policy association.

 Pc5Capability:

 anyOf:

 - type: string

 enum:

 - LTE\_PC5

 - NR\_PC5

 - LTE\_NR\_PC5

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - LTE\_PC5: This value is used to indicate that UE supports PC5 LTE RAT for V2X

 communications over the PC5 reference point.

 - NR\_PC5: This value is used to indicate that UE supports PC5 NR RAT for V2X communications

 over the PC5 reference point.

 - LTE\_NR\_PC5: This value is used to indicate that UE supports both PC5 LTE and NR RAT for

 V2X communications over the PC5 reference point.

 ProSeCapability:

 anyOf:

 - type: string

 enum:

 - PROSE\_DD

 - PROSE\_DC

 - PROSE\_L2\_U2N\_RELAY

 - PROSE\_L3\_U2N\_RELAY

 - PROSE\_L2\_REMOTE\_UE

 - PROSE\_L3\_REMOTE\_UE

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 the content defined in the present version of this API.

 description: >

 Possible values are

 - PROSE\_DD: This value is used to indicate that 5G ProSe Direct Discovery is supported by

 the UE.

 - PROSE\_DC: This value is used to indicate that 5G ProSe Direct Communication is supported

 by the UE.

 - PROSE\_L2\_U2N\_RELAY: This value is used to indicate that Layer-2 5G ProSe UE-to-Network

 Relay is supported by the UE.

 - PROSE\_L3\_U2N\_RELAY: This value is used to indicate that Layer-3 5G ProSe UE-to-Network

 Relay is supported by the UE.

 - PROSE\_L2\_REMOTE\_UE: This value is used to indicate that Layer-2 5G ProSe Remote UE is

 supported by the UE.

 - PROSE\_L3\_REMOTE\_UE: This value is used to indicate that Layer-3 5G ProSe Remote UE is

 supported by the UE.

\*\*\* End of Changes \*\*\*