**3GPP TSG-CT3 Meeting #121e C3-222160**

**E-Meeting, 6th – 12th April 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.522** | **CR** | **0571** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Correction to the TSCTSF discovery of subscription to notification of Time Synchronization Capabilites |
|  |  |
| ***Source to WG:*** | Huawei, Ericsson |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | IIoT |  | ***Date:*** | 2022-04-12 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Stage 2 specified that only one TSCTSF for a given DNN, S-NSSAI would exist in a deployment, and eliminated the need to impact the UDR for TSCTSF discovery.  |
|  |  |
| ***Summary of change:*** | The NEF shall select a TSCTSF based on the local configuration or discover the TSCTSF via Nnrf\_NFDiscovery service as defined in 3GPP TS 29.510 [27] for a DNN/S-NSSAI combination, if not configured |
|  |  |
| ***Consequences if not approved:*** | Not aligned with stage 2. Misleading proceduring, which may lead to incorrect implementations |
|  |  |
| ***Clauses affected:*** | 2, 4.4.24.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR doesn’t impact any OpenAPI files. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* Start of Changes \* \* \* \*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.502: "Procedures for the 5G system".

[3] 3GPP TS 23.501: "System Architecture for the 5G".

[4] 3GPP TS 29.122: "T8 reference point for northbound Application Programming Interfaces (APIs)".

[5] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[6] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[7] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[8] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[9] 3GPP TS 29.521: "5G System; Binding Support Management Service; Stage 3".

[10] Void.

[11] 3GPP TS 23.222: "Common API Framework for 3GPP Northbound APIs; Stage 2".

[12] 3GPP TS 29.222: "Common API Framework for 3GPP Northbound APIs; Stage 3".

[13] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[14] 3GPP TS 33.122: "Security Aspects of Common API Framework for 3GPP Northbound APIs".

[15] Void.

[16] Void

[17] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[18] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[19] 3GPP TS 29.554: "5G System; Background Data Transfer Policy Control Service; Stage 3".

[20] 3GPP TS 29.504: "5G System; Unified Data Repository Services; Stage 3".

[21] 3GPP TR 21.900: "Technical Specification Group working methods".

[22] 3GPP TS 29.523: "5G System; Policy Control Event Exposure Service; Stage 3".

[23] 3GPP TS 29.519: "5G System; Usage of the Unified Data Repository service for Policy Control Data, Application Data and Structured Data for Exposure; Stage 3".

[24] 3GPP TS 29.541: "5G System; Network Exposure (NE) function services for Non-IP Data Delivery (NIDD); Stage 3".

[25] 3GPP TS 29.542: "5G System, Session management services for Non-IP Data Delivery (NIDD); Stage 3".

[26] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[27] 3GPP TS 29.520: "5G System; Network Data Analytics Services; Stage 3".

[28] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G system (5GS)".

[29] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[30] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[31] Void

[32] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[33] 3GPP TS 24.588: "Vehicle-to-Everything (V2X) services in 5G System (5GS); User Equipment (UE) policies; Stage 3".

[34] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

[35] 3GPP TS 29.515: "5G System; Gateway Mobile Location Services; Stage 3".

[36] 3GPP TS 23.273: "5G System Location Services (LCS)".

[37] 3GPP TS 33.535: "Authentication and Key Management for Applications (AKMA) based on 3GPP credentials in the 5G System (5GS)".

[38] 3GPP TS 29.535: "5G System; AKMA Anchor Services; Stage 3".

[39] 3GPP TS 33.220: "Generic Authentication Architecture (GAA); Generic Bootstrapping Architecture (GBA)".

[40] IETF RFC 7542: "The Network Access Identifier".

[41] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[42] 3GPP TS 23.548: "5G System Enhancements for Edge Computing; Stage 2".

[43] 3GPP TS 29.534: "5G System; Access and Mobility Policy Authorization Service; Stage 3".

[44] IETF RFC 3986: "Uniform Resource Identifier (URI): Generic Syntax".

[45] IEEE Std 1588-2019: "IEEE Standard for a Precision Clock Synchronization Protocol for Networked Measurement and Control".

[46] IEEE Std 802.1AS-2020: "IEEE Standard for Local and metropolitan area networks--Timing and Synchronization for Time-Sensitive Applications".

[47] 3GPP TS 29.536: "5G System; Network Slice Admission Control Services; Stage 3".

[48] 3GPP TS 24.526: "User Equipment (UE) policies for 5G System (5GS); Stage 3".

[49] 3GPP TS 24.555: "Proximity based services (ProSe) in 5G system (5GS); User Equipment (UE) policies; Stage 3".

[50] 3GPP TS 29.565: "5G System; Time Sensitive Communication and Time Synchronization Function Services; Stage 3".

[51] IEEE 802.1Q: "Virtual Bridged Local Area Networks".

[52] 3GPP TS 29.532: "5G System; 5G Multicast-Broadcast Session Management Services; Stage 3".

[53] 3GPP TS 23.247: "Architectural enhancements for 5G multicast-broadcast services; Stage 2".

[54] IETF RFC 6733: "Diameter Base Protocol".

[x] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

\* \* \* \* Next Change \* \* \* \*

#### 4.4.24.1 Subscription to notification of Time Synchronization Capabilites

The procedures are used by the AF to subscribe to notifications and to explicitly cancel a previous subscription for UE availability for the time synchronization service via the NEF.

In order to subscribe to the notification for UE availability for the time synchronization service, the AF shall send an HTTP POST rmessage to the NEF to the customized operation URI "{apiRoot}/3gpp-time-sync/v1/{afId}/subscriptions". The HTTP POST message shall include the TimeSyncExposureSubsc data structure as request body. The TimeSyncExposureSubsc data structure shall include:

- one of the indication of the UEs to which the time synchronization capabilities is requested via:

- identification of a list of individual UEs within a "gpsis" attribute;

- indication of any UE within the "anyUeInd" attribute if DNN and S-NSSAI are provisioned; or

- identification of a group of UE(s) via a "exterGroupId" attribute.

- subscription to event(s) notification as "evSubsc" attribute;

- notification URI within the "subsNotifUri" attribute;

- notification correlation Id within the "subsNotifId" attribute;

and may include:

* either the DNN within the "dnn" attribute and the "snssai" attribute or the AF Service Identifier within the "afServiceId" attribute;
* the requested event filter(s) within the "eventFilters" attribute;
* notification methods within the "notifMethods" attribute
* maximum number of reports within the "maxReportNbr" attribute;
* expiry time within the "expiry" attribute; and
* report period within the "repPeriod" attribute.

In order to delete an existing subscription, the AF shall send an HTTP DELETE message to the NEF targeting the resource "Individual Time Synchronization Exposure Subscription".

Upon the reception of an HTTP POST request, if the AF is authorized, the NEF shall interact with the UDM by using Nudm\_SubscriberDataManagement service as defined in 3GPP TS 29.503 [17] to translate the GPSI or external group identifier into the corresponding SUPI or internal group identifier. Then the NEF shall select a TSCTSF based on the local configuration or discover the TSCTSF via Nnrf\_NFDiscovery service as defined in 3GPP TS 29.510 [x] for a DNN/S-NSSAI combination, if not configured. After the NEF obtains TSCTSF, the NEF shall invokes the Ntsctsf\_TimeSynchronization\_CapsSubscribe request service operation to the selected TSCTSF. If the NEF receives an error code from the TSCTSF, the NEF shall not create or delete the resource and shall respond to the AF with a proper error status code.

NOTE: It is assumed that there is only one TSCTSF set for a given DNN/S-NSSAI in this release of the specification.

After receiving a successful response from the TSCTSF, the NEF shall,

- for an HTTP POST request, create an "Individual Time Synchronization Exposure Subscription" resource which represents the time synchronization exposure subscription request, addressed by a URI that contains the AF Identifier and a NEF-created configuration identifier, and shall respond to the AF with a 201 Created status code, including a Location header field containing the URI for the created resource. The AF shall use the URI received in the Location header in subsequent requests to the NEF to refer to this Time Synchronization Exposure Subscription.

- when the NEF receives the notification of the time synchronization capability for a list of UE(s) from the TSCSF by Ntsctsf\_TimeSynchronization\_CapsNotify service operation defined in 3GPP TS 29.565 [50], the NEF shall provide a notification to AF by sending HTTP POST message that include the TimeSyncExposureSubsNotif data structure in the request body. Upon receipt of the notification, the AF shall respond with a "204 No Content" status code to confirm the received notification.

- for an HTTP DELETE request, remove all properties of the resource and delete the corresponding active "Individual Time Synchronization Exposure Subscription" resource, then respond to the AF with a 204 No Content status code.

\* \* \* \* End of change \* \* \* \*