**3GPP TSG-CT3 Meeting #122e C3-223709**

**E-Meeting, 12th – 20th May 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **29.508** | **CR** | **0183** | **rev** | **-** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Update of info and externalDocs fields |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 2022-05-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | CR modifying Nsmf\_EventExposure API has been agreed and the version number of the corresponding OpenAPI file thus needs to be incremented following the rules in TS 29.501, subclause 4.3.1.The following agreed CR updates the Nsmf\_EventExposure API for the present release:+ TS 29.508 CR #0173 is a backward compatible correction in Rel-17+ TS 29.508 CR #0174 is a backward compatible correction in Rel-17+ TS 29.508 CR #0179 is a backward compatible feature in Rel-17+ TS 29.508 CR #0180 is a backward compatible correction in Rel-17+ TS 29.508 CR #0182 is a backward compatible feature in Rel-17As backward compatible features and corrections (but no backward incompatible changes) are added before the OpenAPI freeze of the present release, and major and minor version numbers have already been assigned for the present release, only the "pre-release version" is incremented.Since a new Rel-17 TS version will be provided with changes to the OpenAPI specification file, the TS version number included in the "description" field of the "externalDocs" object also needs to be updated. |
|  |  |
| ***Summary of change:*** | The Nsmf\_EventExposure API version value changed to "1.2.0".The TS version number included in the "description" field of the "externalDocs" object changed to "17.7.0". |
|  |  |
| ***Consequences if not approved:*** | Incorrect API version number and incorrect TS version number in the "description" field of the "externalDocs" object. |
|  |  |
| ***Clauses affected:*** | A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

# A.2 Nsmf\_EventExposure API

openapi: 3.0.0

info:

 version: 1.2.0

 title: Nsmf\_EventExposure

 description: |

 Session Management Event Exposure Service.

 © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: 3GPP TS 29.508 V17.7.0; 5G System; Session Management Event Exposure Service.

 url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.508/

servers:

 - url: '{apiRoot}/nsmf-event-exposure/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501

security:

 - {}

 - oAuth2ClientCredentials:

 - nsmf-event-exposure

paths:

 /subscriptions:

 post:

 operationId: CreateIndividualSubcription

 summary: Create an individual subscription for event notifications from the SMF

 tags:

 - Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 responses:

 '201':

 description: Created.

 headers:

 Location:

 description: 'Contains the URI of the newly created resource, according to the structure: {apiRoot}/nsmf-event-exposure/v1/subscriptions/{subId}'

 required: true

 schema:

 type: string

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 myNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposureNotification'

 responses:

 '204':

 description: No Content, Notification was successful.

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 afAcknowledgement:

 '{request.body#/ackUri}':

 post:

 requestBody: # contents of the callback message

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/AckOfNotify'

 responses:

 '204':

 description: No Content (successful acknowledgement)

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 /subscriptions/{subId}:

 get:

 operationId: GetIndividualSubcription

 summary: Read an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 put:

 operationId: ReplaceIndividualSubcription

 summary: Replace an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Resource was successfully modified and representation is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/NsmfEventExposure'

 '204':

 description: No Content. Resource was successfully modified

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 delete:

 operationId: DeleteIndividualSubcription

 summary: Delete an individual subscription for event notifications from the SMF

 tags:

 - IndividualSubscription (Document)

 parameters:

 - name: subId

 in: path

 description: Event Subscription ID

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content. Resource was successfully deleted

 '307':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nsmf-event-exposure: Access to the Nsmf\_EventExposure API

 schemas:

 NsmfEventExposure:

 description: Represents an Individual SMF Notification Subscription resource. The serviveName property corresponds to the serviceName in the main body of the specification.

 type: object

 properties:

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 anyUeInd:

 type: boolean

 description: Any UE indication. This IE shall be present if the event subscription is applicable to any UE. Default value "false" is used, if not present.

 groupId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 pduSeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 subId:

 $ref: '#/components/schemas/SubId'

 notifId:

 type: string

 description: Notification Correlation ID assigned by the NF service consumer.

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 altNotifIpv4Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 description: Alternate or backup IPv4 address(es) where to send Notifications.

 minItems: 1

 altNotifIpv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 description: Alternate or backup IPv6 address(es) where to send Notifications.

 minItems: 1

 altNotifFqdns:

 type: array

 items:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

 minItems: 1

 description: Alternate or backup FQDN(s) where to send Notifications.

 eventSubs:

 type: array

 items:

 $ref: '#/components/schemas/EventSubscription'

 minItems: 1

 description: Subscribed events

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 ImmeRep:

 type: boolean

 notifMethod:

 $ref: '#/components/schemas/NotificationMethod'

 maxReportNbr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 expiry:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 repPeriod:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 guami:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Guami'

 serviveName:

 $ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/ServiceName'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 sampRatio:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SamplingRatio'

 partitionCriteria:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PartitioningCriteria'

 minItems: 1

 description: Criteria for partitioning the UEs before applying the sampling ratio.

 grpRepTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 notifFlag:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NotificationFlag'

 required:

 - notifId

 - notifUri

 - eventSubs

 NsmfEventExposureNotification:

 description: Represents notifications on events that occurred.

 type: object

 properties:

 notifId:

 type: string

 description: Notification correlation ID

 eventNotifs:

 type: array

 items:

 $ref: '#/components/schemas/EventNotification'

 minItems: 1

 description: Notifications about Individual Events

 ackUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 required:

 - notifId

 - eventNotifs

 EventSubscription:

 description: Represents a subscription to a single event.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/SmfEvent'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 dddTraDescriptors:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 minItems: 1

 dddStati:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 minItems: 1

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 targetPeriod:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 transacDispInd:

 type: boolean

 description: Indicates the subscription for UE transaction dispersion collectionon, if it is included and set to "true". Default value is "false".

 transacMetrics:

 type: array

 items:

 $ref: '#/components/schemas/TransactionMetric'

 description: Indicates Session Management Transaction metrics.

 minItems: 1

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 required:

 - event

 EventNotification:

 description: Represents a notification related to a single event that occurred.

 type: object

 properties:

 event:

 $ref: '#/components/schemas/SmfEvent'

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 ueIpAddr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/IpAddr'

 transacInfos:

 type: array

 items:

 $ref: '#/components/schemas/TransactionInfo'

 description: Transaction Information.

 minItems: 1

 sourceDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 targetDnai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 dnaiChgType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DnaiChangeType'

 sourceUeIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 sourceUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 targetUeIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 targetUeIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 sourceTraRouting:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 targetTraRouting:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 ueMac:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/MacAddr48'

 adIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 adIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 reIpv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 reIpv6Prefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 plmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 accType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AccessType'

 pduSeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dddStatus:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DlDataDeliveryStatus'

 dddTraDescriptor:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DddTrafficDescriptor'

 maxWaitTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 commFailure:

 $ref: 'TS29518\_Namf\_EventExposure.yaml#/components/schemas/CommunicationFailure'

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Prefixes:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 minItems: 1

 ipv6Addrs:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 minItems: 1

 pduSessType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 qfi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 appId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 ethfDescs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/EthFlowDescription'

 minItems: 1

 maxItems: 2

 fDescs:

 type: array

 items:

 $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/FlowDescription'

 minItems: 1

 maxItems: 2

 dnn:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 ulDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 dlDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 rtDelays:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 minItems: 1

 timeWindow:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/TimeWindow'

 smNasFromUe:

 $ref: '#/components/schemas/SmNasFromUe'

 smNasFromSmf:

 $ref: '#/components/schemas/SmNasFromSmf'

 upRedTrans:

 type: string

 ssId:

 type: string

 bssId:

 type: string

 startWlan:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endWlan:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 pduSessInfos:

 type: array

 items:

 $ref: '#/components/schemas/PduSessionInformation'

 minItems: 1

 upfInfo:

 $ref: '#/components/schemas/UpfInformation'

 required:

 - event

 - timeStamp

 SubId:

 type: string

 format: SubId

 description: Identifies an Individual SMF Notification Subscription. To enable that the value is used as part of a URI, the string shall only contain characters allowed according to the "lower-with-hyphen" naming convention defined in 3GPP TS 29.501. In an OpenAPI schema, the format shall be designated as "SubId".

 AckOfNotify:

 description: Represents an acknowledgement information of an event notification.

 type: object

 properties:

 notifId:

 type: string

 ackResult:

 $ref: 'TS29522\_TrafficInfluence.yaml#/components/schemas/AfResultInfo'

 supi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 gpsi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 required:

 - notifId

 - ackResult

 SmNasFromUe:

 description: Represents information on the SM NAS messages that SMF receives from UE for PDU Session.

 type: object

 properties:

 smNasType:

 type: string

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - smNasType

 - timeStamp

 SmNasFromSmf:

 description: Represents information on the SM congestion control applied SM NAS messages that SMF sends to UE for PDU Session.

 type: object

 properties:

 smNasType:

 type: string

 timeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 backoffTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 appliedSmccType:

 $ref: '#/components/schemas/AppliedSmccType'

 required:

 - smNasType

 - timeStamp

 - backoffTimer

 - appliedSmccType

 TransactionInfo:

 description: Represents SMF Transaction Information.

 type: object

 properties:

 transaction:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

 snssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 appIds:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationId'

 minItems: 1

 transacMetrics:

 type: array

 items:

 $ref: '#/components/schemas/TransactionMetric'

 minItems: 1

 required:

 - transaction

 PduSessionInformation:

 description: Represents the PDU session related information.

 type: object

 properties:

 pduSessId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 sessInfo:

 $ref: '#/components/schemas/PduSessionInfo'

 PduSessionInfo:

 description: Represents session information.

 type: object

 properties:

 n4SessId:

 type: string

 sessInactiveTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 pduSessStatus:

 $ref: '#/components/schemas/PduSessionStatus'

 UpfInformation:

 description: Represents the ID/address/FQDN of the UPF.

 type: object

 properties:

 upfId:

 type: string

 upfAddr:

 $ref: 'TS29517\_Naf\_EventExposure.yaml#/components/schemas/AddrFqdn'

 SmfEvent:

 anyOf:

 - type: string

 enum:

 - AC\_TY\_CH

 - UP\_PATH\_CH

 - PDU\_SES\_REL

 - PLMN\_CH

 - UE\_IP\_CH

 - RAT\_TY\_CH

 - DDDS

 - COMM\_FAIL

 - PDU\_SES\_EST

 - QFI\_ALLOC

 - QOS\_MON

 - SMCC\_EXP

 - DISPERSION

 - RED\_TRANS\_EXP

 - WLAN\_INFO

 - UPF\_INFO

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - AC\_TY\_CH: Access Type Change

 - UP\_PATH\_CH: UP Path Change

 - PDU\_SES\_REL: PDU Session Release

 - PLMN\_CH: PLMN Change

 - UE\_IP\_CH: UE IP address change

 - RAT\_TY\_CH: RAT Type Change

 - DDDS: Downlink data delivery status

 - COMM\_FAIL: Communication Failure

 - PDU\_SES\_EST: PDU Session Establishment

 - QFI\_ALLOC: QFI allocation

 - QOS\_MON: QoS Monitoring

 - SMCC\_EXP: SM congestion control experience for PDU Session

 - DISPERSION: Session Management transaction dispersion

 - RED\_TRANS\_EXP: Redundant transmission experience for PDU Session

 - WLAN\_INFO: WLAN information on PDU session for which Access Type is NON\_3GPP\_ACCESS and RAT Type is TRUSTED\_WLAN

 - UPF\_INFO: The UPF information, including the UPF ID/address/FQDN information.

 NotificationMethod:

 anyOf:

 - type: string

 enum:

 - PERIODIC

 - ONE\_TIME

 - ON\_EVENT\_DETECTION

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - PERIODIC

 - ONE\_TIME

 - ON\_EVENT\_DETECTION

 AppliedSmccType:

 anyOf:

 - type: string

 enum:

 - DNN\_CC

 - SNSSAI\_CC

 description: >

 This string indicates the applied SM congestion control.

 - type: string

 description: >

 This string provides forward-compatibility with future

 extensions to the enumeration but is not used to encode

 content defined in the present version of this API.

 description: >

 Possible values are

 - DNN\_CC: Indicates the DNN based congestion control.

 - SNSSAI\_CC: Indicates the S-NSSAI based congestion control.

 TransactionMetric:

 anyOf:

 - type: string

 enum:

 - PDU\_SES\_EST

 - PDU\_SES\_AUTH

 - PDU\_SES\_MODIF

 - PDU\_SES\_REL

 - type: string

 description: >

 This string Indicates Session Management Transaction metrics.

 description: >

 Possible values are

 - PDU\_SES\_EST: PDU Session Establishment

 - PDU\_SES\_AUTH: PDU Session Authentication

 - PDU\_SES\_MODIF: PDU Session Modification

 - PDU\_SES\_REL: PDU Session Release

 PduSessionStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVATED

 - DEACTIVATED

 - type: string

 description: >

 This string Indicates the status of the PDU Session.

 description: >

 Possible values are

 - ACTIVATED: PDU Session status is activated.

 - DEACTIVATED: PDU Session status is deactivated.

\*\*\* End of Changes \*\*\*